From 93032782a4803072d7ab1e22da029325f8f3cf44 Mon Sep 17 00:00:00 2001
From: Steve Sakoman <steve@sakoman.com>
Date: Thu, 17 Dec 2009 15:05:30 -0800
Subject: [PATCH 22/28] OMAP: DSS2: Add support for LG Philips LB035Q02 panel

---
 drivers/video/omap2/displays/Kconfig               |   12 +
 drivers/video/omap2/displays/Makefile              |    2 +
 .../omap2/displays/panel-lgphilips-lb035q02.c      |  244 ++++++++++++++++++++
 3 files changed, 258 insertions(+), 0 deletions(-)
 create mode 100644 drivers/video/omap2/displays/panel-lgphilips-lb035q02.c

diff --git a/drivers/video/omap2/displays/Kconfig b/drivers/video/omap2/displays/Kconfig
index 12327bb..48e872f 100644
--- a/drivers/video/omap2/displays/Kconfig
+++ b/drivers/video/omap2/displays/Kconfig
@@ -7,6 +7,18 @@ config PANEL_GENERIC
 	  Generic panel driver.
 	  Used for DVI output for Beagle and OMAP3 SDP.
 
+config PANEL_LGPHILIPS_LB035Q02
+	tristate "LG.Philips LB035Q02 LCD Panel"
+	depends on OMAP2_DSS
+	help
+	  LCD Panel used on Overo Palo35
+
+config PANEL_SAMSUNG_LTE430WQ_F0C
+        tristate "Samsung LTE430WQ-F0C LCD Panel"
+        depends on OMAP2_DSS
+        help
+          LCD Panel used on Overo Palo43
+
 config PANEL_SHARP_LS037V7DW01
         tristate "Sharp LS037V7DW01 LCD Panel"
         depends on OMAP2_DSS
diff --git a/drivers/video/omap2/displays/Makefile b/drivers/video/omap2/displays/Makefile
index aa38609..2fb1a57 100644
--- a/drivers/video/omap2/displays/Makefile
+++ b/drivers/video/omap2/displays/Makefile
@@ -1,4 +1,6 @@
 obj-$(CONFIG_PANEL_GENERIC) += panel-generic.o
+obj-$(CONFIG_PANEL_LGPHILIPS_LB035Q02) += panel-lgphilips-lb035q02.o
+obj-$(CONFIG_PANEL_SAMSUNG_LTE430WQ_F0C) += panel-samsung-lte430wq-f0c.o
 obj-$(CONFIG_PANEL_SHARP_LS037V7DW01) += panel-sharp-ls037v7dw01.o
 obj-$(CONFIG_PANEL_SHARP_LQ043T1DG01) += panel-sharp-lq043t1dg01.o
 
diff --git a/drivers/video/omap2/displays/panel-lgphilips-lb035q02.c b/drivers/video/omap2/displays/panel-lgphilips-lb035q02.c
new file mode 100644
index 0000000..4ad709d
--- /dev/null
+++ b/drivers/video/omap2/displays/panel-lgphilips-lb035q02.c
@@ -0,0 +1,244 @@
+/*
+ * LCD panel driver for LG.Philips LB035Q02
+ *
+ * Author: Steve Sakoman <steve@sakoman.com>
+ *
+ * This program is free software; you can redistribute it and/or modify it
+ * under the terms of the GNU General Public License version 2 as published by
+ * the Free Software Foundation.
+ *
+ * This program is distributed in the hope that it will be useful, but WITHOUT
+ * ANY WARRANTY; without even the implied warranty of MERCHANTABILITY or
+ * FITNESS FOR A PARTICULAR PURPOSE.  See the GNU General Public License for
+ * more details.
+ *
+ * You should have received a copy of the GNU General Public License along with
+ * this program.  If not, see <http://www.gnu.org/licenses/>.
+ */
+
+#include <linux/module.h>
+#include <linux/delay.h>
+#include <linux/spi/spi.h>
+
+#include <plat/display.h>
+
+static struct spi_device	*spidev;
+
+static struct omap_video_timings lb035q02_timings = {
+	.x_res = 320,
+	.y_res = 240,
+
+	.pixel_clock	= 6500,
+
+	.hsw		= 2,
+	.hfp		= 20,
+	.hbp		= 68,
+
+	.vsw		= 2,
+	.vfp		= 4,
+	.vbp		= 18,
+};
+
+static int lb035q02_write_reg(u8 reg, u16 val)
+{
+	struct spi_message msg;
+	struct spi_transfer index_xfer = {
+		.len		= 3,
+		.cs_change	= 1,
+	};
+	struct spi_transfer value_xfer = {
+		.len		= 3,
+	};
+	u8	buffer[16];
+
+	spi_message_init(&msg);
+
+	/* register index */
+	buffer[0] = 0x70;
+	buffer[1] = 0x00;
+	buffer[2] = reg & 0x7f;
+	index_xfer.tx_buf = buffer;
+	spi_message_add_tail(&index_xfer, &msg);
+
+	/* register value */
+	buffer[4] = 0x72;
+	buffer[5] = val >> 8;
+	buffer[6] = val;
+	value_xfer.tx_buf = buffer + 4;
+	spi_message_add_tail(&value_xfer, &msg);
+
+	return spi_sync(spidev, &msg);
+}
+
+static int lb035q02_panel_power_on(struct omap_dss_device *dssdev)
+{
+	int r;
+
+	if (dssdev->state == OMAP_DSS_DISPLAY_ACTIVE)
+		return 0;
+
+	r = omapdss_dpi_display_enable(dssdev);
+	if (r)
+		goto err0;
+
+	if (dssdev->platform_enable) {
+		r = dssdev->platform_enable(dssdev);
+		if (r)
+			goto err1;
+	}
+
+	/* Panel init sequence from page 28 of the spec */
+	lb035q02_write_reg(0x01, 0x6300);
+	lb035q02_write_reg(0x02, 0x0200);
+	lb035q02_write_reg(0x03, 0x0177);
+	lb035q02_write_reg(0x04, 0x04c7);
+	lb035q02_write_reg(0x05, 0xffc0);
+	lb035q02_write_reg(0x06, 0xe806);
+	lb035q02_write_reg(0x0a, 0x4008);
+	lb035q02_write_reg(0x0b, 0x0000);
+	lb035q02_write_reg(0x0d, 0x0030);
+	lb035q02_write_reg(0x0e, 0x2800);
+	lb035q02_write_reg(0x0f, 0x0000);
+	lb035q02_write_reg(0x16, 0x9f80);
+	lb035q02_write_reg(0x17, 0x0a0f);
+	lb035q02_write_reg(0x1e, 0x00c1);
+	lb035q02_write_reg(0x30, 0x0300);
+	lb035q02_write_reg(0x31, 0x0007);
+	lb035q02_write_reg(0x32, 0x0000);
+	lb035q02_write_reg(0x33, 0x0000);
+	lb035q02_write_reg(0x34, 0x0707);
+	lb035q02_write_reg(0x35, 0x0004);
+	lb035q02_write_reg(0x36, 0x0302);
+	lb035q02_write_reg(0x37, 0x0202);
+	lb035q02_write_reg(0x3a, 0x0a0d);
+	lb035q02_write_reg(0x3b, 0x0806);
+
+	return 0;
+err1:
+	omapdss_dpi_display_disable(dssdev);
+err0:
+	return r;
+}
+
+static void lb035q02_panel_power_off(struct omap_dss_device *dssdev)
+{
+	if (dssdev->state != OMAP_DSS_DISPLAY_ACTIVE)
+		return;
+
+	if (dssdev->platform_disable)
+		dssdev->platform_disable(dssdev);
+
+	omapdss_dpi_display_disable(dssdev);
+}
+
+static int lb035q02_panel_probe(struct omap_dss_device *dssdev)
+{
+	dssdev->panel.config = OMAP_DSS_LCD_TFT | OMAP_DSS_LCD_IVS |
+		OMAP_DSS_LCD_IHS;
+	dssdev->panel.timings = lb035q02_timings;
+
+	return 0;
+}
+
+static void lb035q02_panel_remove(struct omap_dss_device *dssdev)
+{
+}
+
+static int lb035q02_panel_enable(struct omap_dss_device *dssdev)
+{
+	int r = 0;
+
+	r = lb035q02_panel_power_on(dssdev);
+	if (r)
+		return r;
+
+	dssdev->state = OMAP_DSS_DISPLAY_ACTIVE;
+
+	return 0;
+}
+
+static void lb035q02_panel_disable(struct omap_dss_device *dssdev)
+{
+	lb035q02_panel_power_off(dssdev);
+
+	dssdev->state = OMAP_DSS_DISPLAY_DISABLED;
+}
+
+static int lb035q02_panel_suspend(struct omap_dss_device *dssdev)
+{
+	lb035q02_panel_disable(dssdev);
+	dssdev->state = OMAP_DSS_DISPLAY_SUSPENDED;
+	return 0;
+}
+
+static int lb035q02_panel_resume(struct omap_dss_device *dssdev)
+{
+	int r;
+
+	r = lb035q02_panel_power_on(dssdev);
+	if (r)
+		return r;
+
+	dssdev->state = OMAP_DSS_DISPLAY_ACTIVE;
+
+	return 0;
+}
+
+static struct omap_dss_driver lb035q02_driver = {
+	.probe		= lb035q02_panel_probe,
+	.remove		= lb035q02_panel_remove,
+
+	.enable		= lb035q02_panel_enable,
+	.disable	= lb035q02_panel_disable,
+	.suspend	= lb035q02_panel_suspend,
+	.resume		= lb035q02_panel_resume,
+
+	.driver         = {
+		.name   = "lgphilips_lb035q02_panel",
+		.owner  = THIS_MODULE,
+	},
+};
+
+static int __devinit lb035q02_panel_spi_probe(struct spi_device *spi)
+{
+	spidev = spi;
+	return 0;
+}
+
+static int __devexit lb035q02_panel_spi_remove(struct spi_device *spi)
+{
+	return 0;
+}
+
+static struct spi_driver lb035q02_spi_driver = {
+	.driver		= {
+		.name	= "lgphilips_lb035q02_panel-spi",
+		.owner	= THIS_MODULE,
+	},
+	.probe		= lb035q02_panel_spi_probe,
+	.remove		= __devexit_p (lb035q02_panel_spi_remove),
+};
+
+static int __init lb035q02_panel_drv_init(void)
+{
+	int r;
+	r = spi_register_driver(&lb035q02_spi_driver);
+	if (r != 0)
+		pr_err("lgphilips_lb035q02: Unable to register SPI driver: %d\n", r);
+
+	r = omap_dss_register_driver(&lb035q02_driver);
+	if (r != 0)
+		pr_err("lgphilips_lb035q02: Unable to register panel driver: %d\n", r);
+
+	return r;
+}
+
+static void __exit lb035q02_panel_drv_exit(void)
+{
+	spi_unregister_driver(&lb035q02_spi_driver);
+	omap_dss_unregister_driver(&lb035q02_driver);
+}
+
+module_init(lb035q02_panel_drv_init);
+module_exit(lb035q02_panel_drv_exit);
+MODULE_LICENSE("GPL");
-- 
1.6.6.1

