From 9f9d70c4d1caf249ab36c656c5e89db91d7c981b Mon Sep 17 00:00:00 2001
From: Steve Sakoman <steve@sakoman.com>
Date: Mon, 23 May 2011 12:16:50 -0700
Subject: [PATCH 30/30] omap: Change omap_device activate latency messages from pr_warning to pr_debug

Messages can be safely ignored, so reduce console noise

Signed-off-by: Steve Sakoman <steve@sakoman.com>
---
 arch/arm/plat-omap/omap_device.c |    4 ++--
 1 files changed, 2 insertions(+), 2 deletions(-)

diff --git a/arch/arm/plat-omap/omap_device.c b/arch/arm/plat-omap/omap_device.c
index 9bbda9a..ca8a479 100644
--- a/arch/arm/plat-omap/omap_device.c
+++ b/arch/arm/plat-omap/omap_device.c
@@ -145,12 +145,12 @@ static int _omap_device_activate(struct omap_device *od, u8 ignore_lat)
 			odpl->activate_lat_worst = act_lat;
 			if (odpl->flags & OMAP_DEVICE_LATENCY_AUTO_ADJUST) {
 				odpl->activate_lat = act_lat;
-				pr_warning("omap_device: %s.%d: new worst case "
+				pr_debug("omap_device: %s.%d: new worst case "
 					   "activate latency %d: %llu\n",
 					   od->pdev.name, od->pdev.id,
 					   od->pm_lat_level, act_lat);
 			} else
-				pr_warning("omap_device: %s.%d: activate "
+				pr_debug("omap_device: %s.%d: activate "
 					   "latency %d higher than exptected. "
 					   "(%llu > %d)\n",
 					   od->pdev.name, od->pdev.id,
-- 
1.6.6.1

