From aa44b466398b8b104c07ff1b7209509300fc4f47 Mon Sep 17 00:00:00 2001
From: Nishanth Menon <nm@ti.com>
Date: Mon, 14 Feb 2011 21:14:17 +0530
Subject: [PATCH 11/12] OMAP3+: SR: enable/disable SR only on need

Since we already know the state of the autocomp enablement, we can
see if the requested state is different from the current state and
enable/disable SR only on the need basis.

Signed-off-by: Nishanth Menon <nm@ti.com>
Signed-off-by: Kevin Hilman <khilman@ti.com>
Signed-off-by: Koen Kooi <koen@dominion.thruhere.net>
---
 arch/arm/mach-omap2/smartreflex.c |   11 +++++++----
 1 files changed, 7 insertions(+), 4 deletions(-)

diff --git a/arch/arm/mach-omap2/smartreflex.c b/arch/arm/mach-omap2/smartreflex.c
index 616ef62..3bd9fac 100644
--- a/arch/arm/mach-omap2/smartreflex.c
+++ b/arch/arm/mach-omap2/smartreflex.c
@@ -807,10 +807,13 @@ static int omap_sr_autocomp_store(void *data, u64 val)
 		return -EINVAL;
 	}
 
-	if (!val)
-		sr_stop_vddautocomp(sr_info);
-	else
-		sr_start_vddautocomp(sr_info);
+	/* control enable/disable only if there is a delta in value */
+	if (sr_info->autocomp_active != val) {
+		if (!val)
+			sr_stop_vddautocomp(sr_info);
+		else
+			sr_start_vddautocomp(sr_info);
+	}
 
 	return 0;
 }
-- 
1.6.6.1

