From bb40914cf9e313d70385e647f956a55df15e717f Mon Sep 17 00:00:00 2001
From: Sergio Aguirre <saaguirre@ti.com>
Date: Fri, 11 Jun 2010 16:17:56 -0500
Subject: [PATCH 03/75] mt9t111: Pass v4l2_int_device data

Signed-off-by: Sergio Aguirre <saaguirre@ti.com>
---
 drivers/media/video/mt9t111.c |    2 +-
 include/media/mt9t111.h       |    2 +-
 2 files changed, 2 insertions(+), 2 deletions(-)

diff --git a/drivers/media/video/mt9t111.c b/drivers/media/video/mt9t111.c
index 95e1508..6a7b2c0 100644
--- a/drivers/media/video/mt9t111.c
+++ b/drivers/media/video/mt9t111.c
@@ -371,7 +371,7 @@ static int ioctl_s_power(struct v4l2_int_device *s, enum v4l2_power on)
 	else
 		debug_dummy("debug_dummy -- enable clock\n");;
 
-	rval = sensor->pdata->power_set(on);
+	rval = sensor->pdata->power_set(s, on);
 	if (rval < 0) {
 		dev_err(&c->dev, "Unable to set the power state: " "mt9t111"
 								" sensor\n");
diff --git a/include/media/mt9t111.h b/include/media/mt9t111.h
index 0a5161a..aae3f99 100644
--- a/include/media/mt9t111.h
+++ b/include/media/mt9t111.h
@@ -56,7 +56,7 @@
 
 struct mt9t111_platform_data {
 	char *master;
-	int (*power_set) (enum v4l2_power on);
+	int (*power_set) (struct v4l2_int_device *s, enum v4l2_power on);
 	int (*ifparm) (struct v4l2_ifparm *p);
 	int (*priv_data_set) (void *);
 	/* Interface control params */
-- 
1.6.6.1

