From a04a493ead5afb10aafe2c0cf57bf9e3bf7aa844 Mon Sep 17 00:00:00 2001
From: Koen Kooi <koen@openembedded.org>
Date: Thu, 12 Mar 2009 14:15:42 -0300
Subject: [PATCH] dm355-leopard: add board file based on board-dm355-evm.c

---
 arch/arm/mach-davinci/Kconfig               |    8 +
 arch/arm/mach-davinci/Makefile              |    2 +
 arch/arm/mach-davinci/board-dm355-leopard.c |  295 +++++++++++++++++++++++++++
 3 files changed, 305 insertions(+), 0 deletions(-)
 create mode 100644 arch/arm/mach-davinci/board-dm355-leopard.c

diff --git a/arch/arm/mach-davinci/Kconfig b/arch/arm/mach-davinci/Kconfig
index 0010f2d..85424b8 100644
--- a/arch/arm/mach-davinci/Kconfig
+++ b/arch/arm/mach-davinci/Kconfig
@@ -50,6 +50,14 @@ config MACH_SFFSDR
 	  Say Y here to select the Lyrtech Small Form Factor
 	  Software Defined Radio (SFFSDR) board.
 
+config MACH_DM355_LEOPARD
+	bool "TI DM355 Leopard board"
+	default n
+	depends on ARCH_DAVINCI_DM355
+	help
+	  Configure this option to specify the whether the board used
+	  for development is a DM355 Leopard board.
+
 config DAVINCI_MUX
 	bool "DAVINCI multiplexing support"
 	depends on ARCH_DAVINCI
diff --git a/arch/arm/mach-davinci/Makefile b/arch/arm/mach-davinci/Makefile
index 6783681..96ef484 100644
--- a/arch/arm/mach-davinci/Makefile
+++ b/arch/arm/mach-davinci/Makefile
@@ -19,3 +19,5 @@ obj-$(CONFIG_MACH_DAVINCI_EVM)  	+= board-dm644x-evm.o
 obj-$(CONFIG_MACH_DAVINCI_DM646X_EVM)	+= board-dm646x-evm.o
 obj-$(CONFIG_MACH_DAVINCI_DM355_EVM)	+= board-dm355-evm.o
 obj-$(CONFIG_MACH_SFFSDR)		+= board-sffsdr.o
+obj-$(CONFIG_MACH_DM355_LEOPARD)	+= board-dm355-leopard.o
+
diff --git a/arch/arm/mach-davinci/board-dm355-leopard.c b/arch/arm/mach-davinci/board-dm355-leopard.c
new file mode 100644
index 0000000..a1e97e8
--- /dev/null
+++ b/arch/arm/mach-davinci/board-dm355-leopard.c
@@ -0,0 +1,295 @@
+/*
+ * TI DM355 leopard board support
+ *
+ * Based on board-dm355-evm.c
+ *
+ * This file is licensed under the terms of the GNU General Public 
+ * License version 2. This program is licensed "as is" without any
+ * warranty of any kind, whether express or implied.
+ */
+#include <linux/kernel.h>
+#include <linux/module.h>
+#include <linux/init.h>
+#include <linux/dma-mapping.h>
+#include <linux/platform_device.h>
+#include <linux/mtd/mtd.h>
+#include <linux/mtd/partitions.h>
+#include <linux/mtd/nand.h>
+#include <linux/i2c.h>
+#include <linux/io.h>
+#include <linux/gpio.h>
+#include <linux/clk.h>
+#include <linux/spi/spi.h>
+#include <linux/spi/eeprom.h>
+
+#include <asm/setup.h>
+#include <asm/mach-types.h>
+#include <asm/mach/arch.h>
+#include <asm/mach/map.h>
+#include <asm/mach/flash.h>
+
+#include <mach/hardware.h>
+#include <mach/dm355.h>
+#include <mach/psc.h>
+#include <mach/common.h>
+#include <mach/emac.h>
+#include <mach/i2c.h>
+#include <mach/serial.h>
+#include <mach/nand.h>
+#include <mach/mmc.h>
+
+#define DAVINCI_ASYNC_EMIF_CONTROL_BASE		0x01e10000
+#define DAVINCI_ASYNC_EMIF_DATA_CE0_BASE	0x02000000
+
+/* NOTE:  this is geared for the standard config, with a socketed
+ * 2 GByte Micron NAND (MT29F16G08FAA) using 128KB sectors.  If you
+ * swap chips, maybe with a different block size, partitioning may
+ * need to be changed.
+ */
+#define NAND_BLOCK_SIZE		SZ_128K
+
+static struct mtd_partition davinci_nand_partitions[] = {
+	{
+		/* UBL (a few copies) plus U-Boot */
+		.name		= "bootloader",
+		.offset		= 0,
+		.size		= 15 * NAND_BLOCK_SIZE,
+		.mask_flags	= MTD_WRITEABLE, /* force read-only */
+	}, {
+		/* U-Boot environment */
+		.name		= "params",
+		.offset		= MTDPART_OFS_APPEND,
+		.size		= 1 * NAND_BLOCK_SIZE,
+		.mask_flags	= 0,
+	}, {
+		.name		= "kernel",
+		.offset		= MTDPART_OFS_APPEND,
+		.size		= SZ_4M,
+		.mask_flags	= 0,
+	}, {
+		.name		= "filesystem1",
+		.offset		= MTDPART_OFS_APPEND,
+		.size		= SZ_512M,
+		.mask_flags	= 0,
+	}, {
+		.name		= "filesystem2",
+		.offset		= MTDPART_OFS_APPEND,
+		.size		= MTDPART_SIZ_FULL,
+		.mask_flags	= 0,
+	}
+	/* two blocks with bad block table (and mirror) at the end */
+};
+
+static struct davinci_nand_pdata davinci_nand_data = {
+	.mask_chipsel		= BIT(14),
+	.parts			= davinci_nand_partitions,
+	.nr_parts		= ARRAY_SIZE(davinci_nand_partitions),
+	.ecc_mode		= NAND_ECC_HW_SYNDROME,
+	.options		= NAND_USE_FLASH_BBT,
+};
+
+static struct resource davinci_nand_resources[] = {
+	{
+		.start		= DAVINCI_ASYNC_EMIF_DATA_CE0_BASE,
+		.end		= DAVINCI_ASYNC_EMIF_DATA_CE0_BASE + SZ_32M - 1,
+		.flags		= IORESOURCE_MEM,
+	}, {
+		.start		= DAVINCI_ASYNC_EMIF_CONTROL_BASE,
+		.end		= DAVINCI_ASYNC_EMIF_CONTROL_BASE + SZ_4K - 1,
+		.flags		= IORESOURCE_MEM,
+	},
+};
+
+static struct platform_device davinci_nand_device = {
+	.name			= "davinci_nand",
+	.id			= 0,
+
+	.num_resources		= ARRAY_SIZE(davinci_nand_resources),
+	.resource		= davinci_nand_resources,
+
+	.dev			= {
+		.platform_data	= &davinci_nand_data,
+	},
+};
+
+static struct davinci_i2c_platform_data i2c_pdata = {
+	.bus_freq	= 400	/* kHz */,
+	.bus_delay	= 0	/* usec */,
+};
+
+static int dm355leopard_mmc_gpios = -EINVAL;
+
+static void dm355leopard_mmcsd_gpios(unsigned gpio)
+{
+	gpio_request(gpio + 0, "mmc0_ro");
+	gpio_request(gpio + 1, "mmc0_cd");
+	gpio_request(gpio + 2, "mmc1_ro");
+	gpio_request(gpio + 3, "mmc1_cd");
+
+	/* we "know" these are input-only so we don't
+	 * need to call gpio_direction_input()
+	 */
+
+	dm355leopard_mmc_gpios = gpio;
+}
+
+static struct i2c_board_info dm355leopard_i2c_info[] = {
+	{ I2C_BOARD_INFO("dm355leopard_msp", 0x25),
+		.platform_data = dm355leopard_mmcsd_gpios,
+		/* plus irq */ },
+	/* { I2C_BOARD_INFO("tlv320aic3x", 0x1b), }, */
+	/* { I2C_BOARD_INFO("tvp5146", 0x5d), }, */
+};
+
+static void __init leopard_init_i2c(void)
+{
+	davinci_init_i2c(&i2c_pdata);
+
+	gpio_request(5, "dm355leopard_msp");
+	gpio_direction_input(5);
+	dm355leopard_i2c_info[0].irq = gpio_to_irq(5);
+
+	i2c_register_board_info(1, dm355leopard_i2c_info,
+			ARRAY_SIZE(dm355leopard_i2c_info));
+}
+
+static struct resource dm355leopard_dm9000_rsrc[] = {
+	{
+		/* addr */
+		.start	= 0x04000000,
+		.end	= 0x04000001,
+		.flags	= IORESOURCE_MEM,
+	}, {
+		/* data */
+		.start	= 0x04000016,
+		.end	= 0x04000017,
+		.flags	= IORESOURCE_MEM,
+	}, {
+		.flags	= IORESOURCE_IRQ
+			| IORESOURCE_IRQ_HIGHEDGE /* rising (active high) */,
+	},
+};
+
+static struct platform_device dm355leopard_dm9000 = {
+	.name		= "dm9000",
+	.id		= -1,
+	.resource	= dm355leopard_dm9000_rsrc,
+	.num_resources	= ARRAY_SIZE(dm355leopard_dm9000_rsrc),
+};
+
+static struct platform_device *davinci_leopard_devices[] __initdata = {
+	&dm355leopard_dm9000,
+	&davinci_nand_device,
+};
+
+static struct davinci_uart_config uart_config __initdata = {
+	.enabled_uarts = (1 << 0),
+};
+
+static void __init dm355_leopard_map_io(void)
+{
+	davinci_map_common_io();
+	dm355_init();
+}
+
+static int dm355leopard_mmc_get_cd(int module)
+{
+	if (!gpio_is_valid(dm355leopard_mmc_gpios))
+		return -ENXIO;
+	/* low == card present */
+	return !gpio_get_value_cansleep(dm355leopard_mmc_gpios + 2 * module + 1);
+}
+
+static int dm355leopard_mmc_get_ro(int module)
+{
+	if (!gpio_is_valid(dm355leopard_mmc_gpios))
+		return -ENXIO;
+	/* high == card's write protect switch active */
+	return gpio_get_value_cansleep(dm355leopard_mmc_gpios + 2 * module + 0);
+}
+
+static struct davinci_mmc_config dm355leopard_mmc_config = {
+	.get_cd		= dm355leopard_mmc_get_cd,
+	.get_ro		= dm355leopard_mmc_get_ro,
+	.wires		= 4,
+	.max_freq       = 50000000,
+	.caps           = MMC_CAP_MMC_HIGHSPEED | MMC_CAP_SD_HIGHSPEED,
+};
+
+/* Don't connect anything to J10 unless you're only using USB host
+ * mode *and* have to do so with some kind of gender-bender.  If
+ * you have proper Mini-B or Mini-A cables (or Mini-A adapters)
+ * the ID pin won't need any help.
+ */
+#ifdef CONFIG_USB_MUSB_PERIPHERAL
+#define USB_ID_VALUE	0	/* ID pulled high; *should* float */
+#else
+#define USB_ID_VALUE	1	/* ID pulled low */
+#endif
+
+static struct spi_eeprom at25640a = {
+	.byte_len	= SZ_64K / 8,
+	.name		= "at25640a",
+	.page_size	= 32,
+	.flags		= EE_ADDR2,
+};
+
+static struct spi_board_info dm355_leopard_spi_info[] __initconst = {
+	{
+		.modalias	= "at25",
+		.platform_data	= &at25640a,
+		.max_speed_hz	= 10 * 1000 * 1000,	/* at 3v3 */
+		.bus_num	= 0,
+		.chip_select	= 0,
+		.mode		= SPI_MODE_0,
+	},
+};
+
+static __init void dm355_leopard_init(void)
+{
+	struct clk *aemif;
+
+	gpio_request(9, "dm9000");
+	gpio_direction_input(9);
+	dm355leopard_dm9000_rsrc[2].start = gpio_to_irq(9);
+
+	aemif = clk_get(&dm355leopard_dm9000.dev, "aemif");
+	clk_enable(aemif);
+	clk_put(aemif);
+
+	platform_add_devices(davinci_leopard_devices,
+			     ARRAY_SIZE(davinci_leopard_devices));
+	leopard_init_i2c();
+	davinci_serial_init(&uart_config);
+
+	/* NOTE:  NAND flash timings set by the UBL are slower than
+	 * needed by MT29F16G08FAA chips ... EMIF.A1CR is 0x40400204
+	 * but could be 0x0400008c for about 25% faster page reads.
+	 */
+
+	gpio_request(2, "usb_id_toggle");
+	gpio_direction_output(2, USB_ID_VALUE);
+	/* irlml6401 switches over 1A in under 8 msec */
+	setup_usb(500, 8);
+
+	davinci_setup_mmc(0, &dm355leopard_mmc_config);
+	davinci_setup_mmc(1, &dm355leopard_mmc_config);
+
+	dm355_init_spi0(BIT(0), dm355_leopard_spi_info,
+			ARRAY_SIZE(dm355_leopard_spi_info));
+}
+
+static __init void dm355_leopard_irq_init(void)
+{
+	davinci_irq_init();
+}
+
+MACHINE_START(DM355_LEOPARD, "DaVinci DM355 leopard")
+	.phys_io      = IO_PHYS,
+	.io_pg_offst  = (__IO_ADDRESS(IO_PHYS) >> 18) & 0xfffc,
+	.boot_params  = (0x80000100),
+	.map_io	      = dm355_leopard_map_io,
+	.init_irq     = dm355_leopard_irq_init,
+	.timer	      = &davinci_timer,
+	.init_machine = dm355_leopard_init,
+MACHINE_END
-- 
1.6.1.2

