From 362f211f85aa5e0f7519fca599428e03b05cb05f Mon Sep 17 00:00:00 2001
From: Sergio Aguirre <saaguirre@ti.com>
Date: Sun, 18 Jul 2010 01:47:41 -0500
Subject: [PATCH 68/75] mt9t112: Make context B stream unlimited frames

Context A does this by default, so, only context B needs
to be configured like this.

Signed-off-by: Sergio Aguirre <saaguirre@ti.com>
---
 drivers/media/video/mt9t112.c |    3 +++
 1 files changed, 3 insertions(+), 0 deletions(-)

diff --git a/drivers/media/video/mt9t112.c b/drivers/media/video/mt9t112.c
index 18d7ce5..3c516b4 100644
--- a/drivers/media/video/mt9t112.c
+++ b/drivers/media/video/mt9t112.c
@@ -771,6 +771,9 @@ static int mt9t112_goto_capture(const struct i2c_client *client)
 	if (ret == 0x7)
 		return 0;
 
+	/* Num Frames Run (B) */
+	mt9t112_mcu_write(ret, client, VAR(27, 5), 0);
+
 	/* Go to capture mode */
 	mt9t112_mcu_write(ret, client, VAR8(1, 0), 2);
 	do {
-- 
1.6.6.1

