From f6b0d03d59c13ea30c17aa68d07c06a5229aee1f Mon Sep 17 00:00:00 2001
From: Koen Kooi <koen@dominion.thruhere.net>
Date: Thu, 20 Oct 2011 11:14:08 +0200
Subject: [PATCH 06/10] ARM: OMAP2+: beagleboard: make wilink init look more like pandaboard

Signed-off-by: Koen Kooi <koen@dominion.thruhere.net>
---
 arch/arm/mach-omap2/board-omap3beagle.c |    8 +-------
 1 files changed, 1 insertions(+), 7 deletions(-)

diff --git a/arch/arm/mach-omap2/board-omap3beagle.c b/arch/arm/mach-omap2/board-omap3beagle.c
index 5e1d9f9..13fffb0 100644
--- a/arch/arm/mach-omap2/board-omap3beagle.c
+++ b/arch/arm/mach-omap2/board-omap3beagle.c
@@ -203,13 +203,7 @@ static struct regulator_consumer_supply beagle_vmmc2_supply =
 
 static struct regulator_init_data beagle_vmmc2 = {
 	.constraints = {
-		.min_uV			= 1850000,
-		.max_uV			= 1850000,
-		.apply_uV		= true,
-		.valid_modes_mask	= REGULATOR_MODE_NORMAL
-					| REGULATOR_MODE_STANDBY,
-		.valid_ops_mask		= REGULATOR_CHANGE_MODE
-					| REGULATOR_CHANGE_STATUS,
+		.valid_ops_mask = REGULATOR_CHANGE_STATUS,
 	},
 	.num_consumer_supplies = 1,
 	.consumer_supplies = &beagle_vmmc2_supply,
-- 
1.6.6.1

