From 91da655eb768b52d085fac42648e6bcf342a1f7f Mon Sep 17 00:00:00 2001
From: Koen Kooi <koen@dominion.thruhere.net>
Date: Fri, 17 Jun 2011 09:33:03 +0200
Subject: [PATCH 13/30] beagleboard: load kernel from MMC ext, not FAT

Signed-off-by: Koen Kooi <koen@dominion.thruhere.net>
---
 include/configs/omap3_beagle.h |    3 ++-
 1 files changed, 2 insertions(+), 1 deletions(-)

diff --git a/include/configs/omap3_beagle.h b/include/configs/omap3_beagle.h
index 9a161cf..dbb77fb 100644
--- a/include/configs/omap3_beagle.h
+++ b/include/configs/omap3_beagle.h
@@ -246,7 +246,8 @@
 		"root=${ramroot} " \
 		"rootfstype=${ramrootfstype}\0" \
 	"loadramdisk=fatload mmc ${mmcdev} ${rdaddr} ramdisk.gz\0" \
-	"loaduimage=fatload mmc ${mmcdev} ${loadaddr} uImage\0" \
+	"loaduimagefat=fatload mmc ${mmcdev} ${loadaddr} uImage\0" \
+	"loaduimage=ext2load mmc ${mmcdev}:2 ${loadaddr} /boot/uImage\0" \
 	"mmcboot=echo Booting from mmc ...; " \
 		"run mmcargs; " \
 		"bootm ${loadaddr}\0" \
-- 
1.6.6.1

