From 335b633ec57a8ae7e4439f8dfe6a4a4333399ba4 Mon Sep 17 00:00:00 2001
From: Kevin Hilman <khilman@ti.com>
Date: Tue, 5 Apr 2011 16:27:21 -0700
Subject: [PATCH 140/149] OMAP3+: voltage: rename scale and reset functions using voltdm_ prefix

Rename voltage scaling related functions to use voltdm_ prefix intead
of omap_voltage_, and cleanup kerneldoc comments in the process.

s/omap_voltage_scale_vdd/voltdm_scale/
s/omap_voltage_reset/voltdm_reset/

Also, in voltdm_reset() s/target_uvdc/target_volt/ to be consistent with
naming throughout the file.

No functional changes.

Signed-off-by: Kevin Hilman <khilman@ti.com>
---
 arch/arm/mach-omap2/pm.c                 |    2 +-
 arch/arm/mach-omap2/smartreflex-class3.c |    2 +-
 arch/arm/mach-omap2/voltage.c            |   29 ++++++++++++++---------------
 arch/arm/mach-omap2/voltage.h            |    5 ++---
 4 files changed, 18 insertions(+), 20 deletions(-)

diff --git a/arch/arm/mach-omap2/pm.c b/arch/arm/mach-omap2/pm.c
index f81340e..659e400 100644
--- a/arch/arm/mach-omap2/pm.c
+++ b/arch/arm/mach-omap2/pm.c
@@ -214,7 +214,7 @@ static int __init omap2_set_init_voltage(char *vdd_name, char *clk_name,
 		goto exit;
 	}
 
-	omap_voltage_scale_vdd(voltdm, bootup_volt);
+	voltdm_scale(voltdm, bootup_volt);
 	return 0;
 
 exit:
diff --git a/arch/arm/mach-omap2/smartreflex-class3.c b/arch/arm/mach-omap2/smartreflex-class3.c
index f438cf4..4eac1bc 100644
--- a/arch/arm/mach-omap2/smartreflex-class3.c
+++ b/arch/arm/mach-omap2/smartreflex-class3.c
@@ -32,7 +32,7 @@ static int sr_class3_disable(struct voltagedomain *voltdm, int is_volt_reset)
 	omap_vp_disable(voltdm);
 	sr_disable(voltdm);
 	if (is_volt_reset)
-		omap_voltage_reset(voltdm);
+		voltdm_reset(voltdm);
 
 	return 0;
 }
diff --git a/arch/arm/mach-omap2/voltage.c b/arch/arm/mach-omap2/voltage.c
index 32f0873..7588480 100644
--- a/arch/arm/mach-omap2/voltage.c
+++ b/arch/arm/mach-omap2/voltage.c
@@ -94,16 +94,15 @@ unsigned long omap_voltage_get_nom_volt(struct voltagedomain *voltdm)
 }
 
 /**
- * omap_voltage_scale_vdd() - API to scale voltage of a particular
- *				voltage domain.
- * @voltdm:	pointer to the VDD which is to be scaled.
- * @target_volt:	The target voltage of the voltage domain
+ * voltdm_scale() - API to scale voltage of a particular voltage domain.
+ * @voltdm: pointer to the voltage domain which is to be scaled.
+ * @target_volt: The target voltage of the voltage domain
  *
  * This API should be called by the kernel to do the voltage scaling
- * for a particular voltage domain during dvfs or any other situation.
+ * for a particular voltage domain during DVFS.
  */
-int omap_voltage_scale_vdd(struct voltagedomain *voltdm,
-		unsigned long target_volt)
+int voltdm_scale(struct voltagedomain *voltdm,
+		 unsigned long target_volt)
 {
 	if (!voltdm || IS_ERR(voltdm)) {
 		pr_warning("%s: VDD specified does not exist!\n", __func__);
@@ -120,31 +119,31 @@ int omap_voltage_scale_vdd(struct voltagedomain *voltdm,
 }
 
 /**
- * omap_voltage_reset() - Resets the voltage of a particular voltage domain
- *			to that of the current OPP.
- * @voltdm:	pointer to the VDD whose voltage is to be reset.
+ * voltdm_reset() - Resets the voltage of a particular voltage domain
+ * 	            to that of the current OPP.
+ * @voltdm: pointer to the voltage domain whose voltage is to be reset.
  *
  * This API finds out the correct voltage the voltage domain is supposed
  * to be at and resets the voltage to that level. Should be used especially
  * while disabling any voltage compensation modules.
  */
-void omap_voltage_reset(struct voltagedomain *voltdm)
+void voltdm_reset(struct voltagedomain *voltdm)
 {
-	unsigned long target_uvdc;
+	unsigned long target_volt;
 
 	if (!voltdm || IS_ERR(voltdm)) {
 		pr_warning("%s: VDD specified does not exist!\n", __func__);
 		return;
 	}
 
-	target_uvdc = omap_voltage_get_nom_volt(voltdm);
-	if (!target_uvdc) {
+	target_volt = omap_voltage_get_nom_volt(voltdm);
+	if (!target_volt) {
 		pr_err("%s: unable to find current voltage for vdd_%s\n",
 			__func__, voltdm->name);
 		return;
 	}
 
-	omap_voltage_scale_vdd(voltdm, target_uvdc);
+	voltdm_scale(voltdm, target_volt);
 }
 
 /**
diff --git a/arch/arm/mach-omap2/voltage.h b/arch/arm/mach-omap2/voltage.h
index d2a0c24..e3efbf9 100644
--- a/arch/arm/mach-omap2/voltage.h
+++ b/arch/arm/mach-omap2/voltage.h
@@ -151,9 +151,6 @@ struct omap_vdd_info {
 	u32 curr_volt;
 };
 
-int omap_voltage_scale_vdd(struct voltagedomain *voltdm,
-		unsigned long target_volt);
-void omap_voltage_reset(struct voltagedomain *voltdm);
 void omap_voltage_get_volttable(struct voltagedomain *voltdm,
 		struct omap_volt_data **volt_data);
 struct omap_volt_data *omap_voltage_get_voltdata(struct voltagedomain *voltdm,
@@ -191,4 +188,6 @@ int voltdm_for_each(int (*fn)(struct voltagedomain *voltdm, void *user),
 int voltdm_for_each_pwrdm(struct voltagedomain *voltdm,
 			  int (*fn)(struct voltagedomain *voltdm,
 				    struct powerdomain *pwrdm));
+int voltdm_scale(struct voltagedomain *voltdm, unsigned long target_volt);
+void voltdm_reset(struct voltagedomain *voltdm);
 #endif
-- 
1.6.6.1

