From 5bf0bd6457468d636582fb238bb9d20e45f8bd92 Mon Sep 17 00:00:00 2001
From: Steve Sakoman <steve@sakoman.com>
Date: Fri, 1 Jul 2011 10:00:03 -0700
Subject: [PATCH 04/14] mtd: nand: Eliminate noisey "uncorrectable error" messages

Other layers of the stack give more informative messages when __nand_correct_data() fails

Signed-off-by: Steve Sakoman <steve@sakoman.com>
---
 drivers/mtd/nand/nand_ecc.c |    2 +-
 1 files changed, 1 insertions(+), 1 deletions(-)

diff --git a/drivers/mtd/nand/nand_ecc.c b/drivers/mtd/nand/nand_ecc.c
index 271b8e7..ad55e55 100644
--- a/drivers/mtd/nand/nand_ecc.c
+++ b/drivers/mtd/nand/nand_ecc.c
@@ -507,7 +507,7 @@ int __nand_correct_data(unsigned char *buf,
 	if ((bitsperbyte[b0] + bitsperbyte[b1] + bitsperbyte[b2]) == 1)
 		return 1;	/* error in ecc data; no action needed */
 
-	printk(KERN_ERR "uncorrectable error : ");
+	// printk(KERN_ERR "uncorrectable error : ");
 	return -1;
 }
 EXPORT_SYMBOL(__nand_correct_data);
-- 
1.6.6.1

