From 64bc651bb56435e4cd86d2ebfa4f301abdbac6e5 Mon Sep 17 00:00:00 2001
From: Keshava Munegowda <Keshava_mgowda@ti.com>
Date: Wed, 1 Jun 2011 11:02:58 -0700
Subject: [PATCH 06/13] arm: omap: usb: device name change for the clk names of usbhs

device name usbhs clocks are changed from
usbhs-omap.0 to usbhs_omap; this is because
in the hwmod registration the device name is set
as usbhs_omap

Signed-off-by: Keshava Munegowda <keshava_mgowda@ti.com>
---
 arch/arm/mach-omap2/clock3xxx_data.c |   28 ++++++++++++++--------------
 arch/arm/mach-omap2/clock44xx_data.c |   10 +++++-----
 drivers/mfd/omap-usb-host.c          |    2 +-
 3 files changed, 20 insertions(+), 20 deletions(-)

diff --git a/arch/arm/mach-omap2/clock3xxx_data.c b/arch/arm/mach-omap2/clock3xxx_data.c
index 75b119b..fabe482 100644
--- a/arch/arm/mach-omap2/clock3xxx_data.c
+++ b/arch/arm/mach-omap2/clock3xxx_data.c
@@ -3285,7 +3285,7 @@ static struct omap_clk omap3xxx_clks[] = {
 	CLK(NULL,	"cpefuse_fck",	&cpefuse_fck,	CK_3430ES2PLUS | CK_AM35XX | CK_36XX),
 	CLK(NULL,	"ts_fck",	&ts_fck,	CK_3430ES2PLUS | CK_AM35XX | CK_36XX),
 	CLK(NULL,	"usbtll_fck",	&usbtll_fck,	CK_3430ES2PLUS | CK_AM35XX | CK_36XX),
-	CLK("usbhs-omap.0",	"usbtll_fck",	&usbtll_fck,	CK_3430ES2PLUS | CK_AM35XX | CK_36XX),
+	CLK("usbhs_omap",	"usbtll_fck",	&usbtll_fck,	CK_3430ES2PLUS | CK_AM35XX | CK_36XX),
 	CLK("omap-mcbsp.1",	"prcm_fck",	&core_96m_fck,	CK_3XXX),
 	CLK("omap-mcbsp.5",	"prcm_fck",	&core_96m_fck,	CK_3XXX),
 	CLK(NULL,	"core_96m_fck",	&core_96m_fck,	CK_3XXX),
@@ -3321,7 +3321,7 @@ static struct omap_clk omap3xxx_clks[] = {
 	CLK(NULL,	"pka_ick",	&pka_ick,	CK_34XX | CK_36XX),
 	CLK(NULL,	"core_l4_ick",	&core_l4_ick,	CK_3XXX),
 	CLK(NULL,	"usbtll_ick",	&usbtll_ick,	CK_3430ES2PLUS | CK_AM35XX | CK_36XX),
-	CLK("usbhs-omap.0",	"usbtll_ick",	&usbtll_ick,	CK_3430ES2PLUS | CK_AM35XX | CK_36XX),
+	CLK("usbhs_omap",	"usbtll_ick",	&usbtll_ick,	CK_3430ES2PLUS | CK_AM35XX | CK_36XX),
 	CLK("omap_hsmmc.2",	"ick",	&mmchs3_ick,	CK_3430ES2PLUS | CK_AM35XX | CK_36XX),
 	CLK(NULL,	"icr_ick",	&icr_ick,	CK_34XX | CK_36XX),
 	CLK("omap-aes",	"ick",	&aes2_ick,	CK_34XX | CK_36XX),
@@ -3367,20 +3367,20 @@ static struct omap_clk omap3xxx_clks[] = {
 	CLK(NULL,	"cam_ick",	&cam_ick,	CK_34XX | CK_36XX),
 	CLK(NULL,	"csi2_96m_fck",	&csi2_96m_fck,	CK_34XX | CK_36XX),
 	CLK(NULL,	"usbhost_120m_fck", &usbhost_120m_fck, CK_3430ES2PLUS | CK_AM35XX | CK_36XX),
-	CLK("usbhs-omap.0",	"hs_fck", &usbhost_120m_fck, CK_3430ES2PLUS | CK_AM35XX | CK_36XX),
+	CLK("usbhs_omap",	"hs_fck", &usbhost_120m_fck, CK_3430ES2PLUS | CK_AM35XX | CK_36XX),
 	CLK(NULL,	"usbhost_48m_fck", &usbhost_48m_fck, CK_3430ES2PLUS | CK_AM35XX | CK_36XX),
-	CLK("usbhs-omap.0",	"fs_fck", &usbhost_48m_fck, CK_3430ES2PLUS | CK_AM35XX | CK_36XX),
+	CLK("usbhs_omap",	"fs_fck", &usbhost_48m_fck, CK_3430ES2PLUS | CK_AM35XX | CK_36XX),
 	CLK(NULL,	"usbhost_ick",	&usbhost_ick,	CK_3430ES2PLUS | CK_AM35XX | CK_36XX),
-	CLK("usbhs-omap.0",	"usbhost_ick",	&usbhost_ick,	CK_3430ES2PLUS | CK_AM35XX | CK_36XX),
-	CLK("usbhs-omap.0",	"utmi_p1_gfclk",	&dummy_ck,	CK_3XXX),
-	CLK("usbhs-omap.0",	"utmi_p2_gfclk",	&dummy_ck,	CK_3XXX),
-	CLK("usbhs-omap.0",	"xclk60mhsp1_ck",	&dummy_ck,	CK_3XXX),
-	CLK("usbhs-omap.0",	"xclk60mhsp2_ck",	&dummy_ck,	CK_3XXX),
-	CLK("usbhs-omap.0",	"usb_host_hs_utmi_p1_clk",	&dummy_ck,	CK_3XXX),
-	CLK("usbhs-omap.0",	"usb_host_hs_utmi_p2_clk",	&dummy_ck,	CK_3XXX),
-	CLK("usbhs-omap.0",	"usb_tll_hs_usb_ch0_clk",	&dummy_ck,	CK_3XXX),
-	CLK("usbhs-omap.0",	"usb_tll_hs_usb_ch1_clk",	&dummy_ck,	CK_3XXX),
-	CLK("usbhs-omap.0",	"init_60m_fclk",	&dummy_ck,	CK_3XXX),
+	CLK("usbhs_omap",	"usbhost_ick",	&usbhost_ick,	CK_3430ES2PLUS | CK_AM35XX | CK_36XX),
+	CLK("usbhs_omap",	"utmi_p1_gfclk",	&dummy_ck,	CK_3XXX),
+	CLK("usbhs_omap",	"utmi_p2_gfclk",	&dummy_ck,	CK_3XXX),
+	CLK("usbhs_omap",	"xclk60mhsp1_ck",	&dummy_ck,	CK_3XXX),
+	CLK("usbhs_omap",	"xclk60mhsp2_ck",	&dummy_ck,	CK_3XXX),
+	CLK("usbhs_omap",	"usb_host_hs_utmi_p1_clk",	&dummy_ck,	CK_3XXX),
+	CLK("usbhs_omap",	"usb_host_hs_utmi_p2_clk",	&dummy_ck,	CK_3XXX),
+	CLK("usbhs_omap",	"usb_tll_hs_usb_ch0_clk",	&dummy_ck,	CK_3XXX),
+	CLK("usbhs_omap",	"usb_tll_hs_usb_ch1_clk",	&dummy_ck,	CK_3XXX),
+	CLK("usbhs_omap",	"init_60m_fclk",	&dummy_ck,	CK_3XXX),
 	CLK(NULL,	"usim_fck",	&usim_fck,	CK_3430ES2PLUS | CK_36XX),
 	CLK(NULL,	"gpt1_fck",	&gpt1_fck,	CK_3XXX),
 	CLK(NULL,	"wkup_32k_fck",	&wkup_32k_fck,	CK_3XXX),
diff --git a/arch/arm/mach-omap2/clock44xx_data.c b/arch/arm/mach-omap2/clock44xx_data.c
index 8c96567..34e91eb 100644
--- a/arch/arm/mach-omap2/clock44xx_data.c
+++ b/arch/arm/mach-omap2/clock44xx_data.c
@@ -3205,7 +3205,7 @@ static struct omap_clk omap44xx_clks[] = {
 	CLK(NULL,	"uart3_fck",			&uart3_fck,	CK_443X),
 	CLK(NULL,	"uart4_fck",			&uart4_fck,	CK_443X),
 	CLK(NULL,	"usb_host_fs_fck",		&usb_host_fs_fck,	CK_443X),
-	CLK("usbhs-omap.0",	"fs_fck",		&usb_host_fs_fck,	CK_443X),
+	CLK("usbhs_omap",	"fs_fck",		&usb_host_fs_fck,	CK_443X),
 	CLK(NULL,	"utmi_p1_gfclk",		&utmi_p1_gfclk,	CK_443X),
 	CLK(NULL,	"usb_host_hs_utmi_p1_clk",	&usb_host_hs_utmi_p1_clk,	CK_443X),
 	CLK(NULL,	"utmi_p2_gfclk",		&utmi_p2_gfclk,	CK_443X),
@@ -3217,8 +3217,8 @@ static struct omap_clk omap44xx_clks[] = {
 	CLK(NULL,	"usb_host_hs_hsic480m_p2_clk",	&usb_host_hs_hsic480m_p2_clk,	CK_443X),
 	CLK(NULL,	"usb_host_hs_func48mclk",	&usb_host_hs_func48mclk,	CK_443X),
 	CLK(NULL,	"usb_host_hs_fck",		&usb_host_hs_fck,	CK_443X),
-	CLK("usbhs-omap.0",	"hs_fck",		&usb_host_hs_fck,	CK_443X),
-	CLK("usbhs-omap.0",	"usbhost_ick",		&dummy_ck,		CK_443X),
+	CLK("usbhs_omap",	"hs_fck",		&usb_host_hs_fck,	CK_443X),
+	CLK("usbhs_omap",	"usbhost_ick",		&dummy_ck,		CK_443X),
 	CLK(NULL,	"otg_60m_gfclk",		&otg_60m_gfclk,	CK_443X),
 	CLK(NULL,	"usb_otg_hs_xclk",		&usb_otg_hs_xclk,	CK_443X),
 	CLK("musb-omap2430",	"ick",				&usb_otg_hs_ick,	CK_443X),
@@ -3227,8 +3227,8 @@ static struct omap_clk omap44xx_clks[] = {
 	CLK(NULL,	"usb_tll_hs_usb_ch0_clk",	&usb_tll_hs_usb_ch0_clk,	CK_443X),
 	CLK(NULL,	"usb_tll_hs_usb_ch1_clk",	&usb_tll_hs_usb_ch1_clk,	CK_443X),
 	CLK(NULL,	"usb_tll_hs_ick",		&usb_tll_hs_ick,	CK_443X),
-	CLK("usbhs-omap.0",	"usbtll_ick",		&usb_tll_hs_ick,	CK_443X),
-	CLK("usbhs-omap.0",	"usbtll_fck",		&dummy_ck,	CK_443X),
+	CLK("usbhs_omap",	"usbtll_ick",		&usb_tll_hs_ick,	CK_443X),
+	CLK("usbhs_omap",	"usbtll_fck",		&dummy_ck,	CK_443X),
 	CLK(NULL,	"usim_ck",			&usim_ck,	CK_443X),
 	CLK(NULL,	"usim_fclk",			&usim_fclk,	CK_443X),
 	CLK(NULL,	"usim_fck",			&usim_fck,	CK_443X),
diff --git a/drivers/mfd/omap-usb-host.c b/drivers/mfd/omap-usb-host.c
index 8552195..43de12a 100644
--- a/drivers/mfd/omap-usb-host.c
+++ b/drivers/mfd/omap-usb-host.c
@@ -28,7 +28,7 @@
 #include <plat/usb.h>
 #include <linux/pm_runtime.h>
 
-#define USBHS_DRIVER_NAME	"usbhs-omap"
+#define USBHS_DRIVER_NAME	"usbhs_omap"
 #define OMAP_EHCI_DEVICE	"ehci-omap"
 #define OMAP_OHCI_DEVICE	"ohci-omap3"
 
-- 
1.6.6.1

