From 4c3ef06a333cf1f873a9a8de05af90959a5d1e68 Mon Sep 17 00:00:00 2001
From: Gregoire Gentil <gregoire@gentil.com>
Date: Fri, 12 Mar 2010 15:04:58 +0100
Subject: [PATCH 12/17] ads7846: don't error out when there's no pendown gpio

---
 drivers/input/touchscreen/ads7846.c |    7 -------
 1 files changed, 0 insertions(+), 7 deletions(-)

diff --git a/drivers/input/touchscreen/ads7846.c b/drivers/input/touchscreen/ads7846.c
index 1d9f97c..c72c3ae 100644
--- a/drivers/input/touchscreen/ads7846.c
+++ b/drivers/input/touchscreen/ads7846.c
@@ -952,13 +952,6 @@ static int __devinit setup_pendown(struct spi_device *spi, struct ads7846 *ts)
 		return 0;
 	}
 
-	err = gpio_request(pdata->gpio_pendown, "ads7846_pendown");
-	if (err) {
-		dev_err(&spi->dev, "failed to request pendown GPIO%d\n",
-				pdata->gpio_pendown);
-		return err;
-	}
-
 	ts->gpio_pendown = pdata->gpio_pendown;
 	return 0;
 }
-- 
1.6.6.1

