From 5b299acba0f1a1ed0003dcea0ae2c8e31b6ee4c7 Mon Sep 17 00:00:00 2001
From: Benoit Cousson <b-cousson@ti.com>
Date: Sun, 10 Jul 2011 05:56:31 -0600
Subject: [PATCH 083/149] OMAP4: prm: Remove deprecated functions

The new prminst_xxx accessors based on partition and offset
is now used, so removed all the previous prcm_xxx accessors.

Signed-off-by: Benoit Cousson <b-cousson@ti.com>
Cc: Paul Walmsley <paul@pwsan.com>
Cc: Rajendra Nayak <rnayak@ti.com>
[paul@pwsan.com: remove fn prototypes also]
Signed-off-by: Paul Walmsley <paul@pwsan.com>
---
 arch/arm/mach-omap2/prm44xx.c |   37 -------------------------------------
 arch/arm/mach-omap2/prm44xx.h |    4 ----
 2 files changed, 0 insertions(+), 41 deletions(-)

diff --git a/arch/arm/mach-omap2/prm44xx.c b/arch/arm/mach-omap2/prm44xx.c
index f815329..0016555 100644
--- a/arch/arm/mach-omap2/prm44xx.c
+++ b/arch/arm/mach-omap2/prm44xx.c
@@ -50,40 +50,3 @@ u32 omap4_prm_rmw_inst_reg_bits(u32 mask, u32 bits, s16 inst, s16 reg)
 
 	return v;
 }
-
-/* Read a PRM register, AND it, and shift the result down to bit 0 */
-/* XXX deprecated */
-u32 omap4_prm_read_bits_shift(void __iomem *reg, u32 mask)
-{
-	u32 v;
-
-	v = __raw_readl(reg);
-	v &= mask;
-	v >>= __ffs(mask);
-
-	return v;
-}
-
-/* Read-modify-write a register in a PRM module. Caller must lock */
-/* XXX deprecated */
-u32 omap4_prm_rmw_reg_bits(u32 mask, u32 bits, void __iomem *reg)
-{
-	u32 v;
-
-	v = __raw_readl(reg);
-	v &= ~mask;
-	v |= bits;
-	__raw_writel(v, reg);
-
-	return v;
-}
-
-u32 omap4_prm_set_inst_reg_bits(u32 bits, s16 inst, s16 reg)
-{
-	return omap4_prm_rmw_inst_reg_bits(bits, bits, inst, reg);
-}
-
-u32 omap4_prm_clear_inst_reg_bits(u32 bits, s16 inst, s16 reg)
-{
-	return omap4_prm_rmw_inst_reg_bits(bits, 0x0, inst, reg);
-}
diff --git a/arch/arm/mach-omap2/prm44xx.h b/arch/arm/mach-omap2/prm44xx.h
index 725a6a8..7dfa379 100644
--- a/arch/arm/mach-omap2/prm44xx.h
+++ b/arch/arm/mach-omap2/prm44xx.h
@@ -750,10 +750,6 @@
 extern u32 omap4_prm_read_inst_reg(s16 inst, u16 idx);
 extern void omap4_prm_write_inst_reg(u32 val, s16 inst, u16 idx);
 extern u32 omap4_prm_rmw_inst_reg_bits(u32 mask, u32 bits, s16 inst, s16 idx);
-extern u32 omap4_prm_rmw_reg_bits(u32 mask, u32 bits, void __iomem *reg);
-extern u32 omap4_prm_set_inst_reg_bits(u32 bits, s16 inst, s16 idx);
-extern u32 omap4_prm_clear_inst_reg_bits(u32 bits, s16 inst, s16 idx);
-extern u32 omap4_prm_read_bits_shift(void __iomem *reg, u32 mask);
 
 # endif
 
-- 
1.6.6.1

