From e07d57760fa95b7500bec64ef5d841d3f8c33450 Mon Sep 17 00:00:00 2001
From: Rajendra Nayak <rnayak@ti.com>
Date: Sun, 10 Jul 2011 05:56:54 -0600
Subject: [PATCH 091/149] OMAP2+: PM: idle clkdms only if already in idle

The omap_set_pwrdm_state function forces clockdomains
to idle, without checking the existing idle state
programmed, instead based solely on the HW capability
of the clockdomain to support idle.
This is wrong and the clockdomains should be idled
post a state_switch *only* if idle transitions on the
clockdomain were already enabled.

Signed-off-by: Rajendra Nayak <rnayak@ti.com>
Cc: Paul Walmsley <paul@pwsan.com>
Acked-by: Kevin Hilman <khilman@ti.com>
Signed-off-by: Paul Walmsley <paul@pwsan.com>
---
 arch/arm/mach-omap2/pm.c |    4 +++-
 1 files changed, 3 insertions(+), 1 deletions(-)

diff --git a/arch/arm/mach-omap2/pm.c b/arch/arm/mach-omap2/pm.c
index d48813f..3feb359 100644
--- a/arch/arm/mach-omap2/pm.c
+++ b/arch/arm/mach-omap2/pm.c
@@ -108,6 +108,7 @@ int omap_set_pwrdm_state(struct powerdomain *pwrdm, u32 state)
 	u32 cur_state;
 	int sleep_switch = -1;
 	int ret = 0;
+	int hwsup = 0;
 
 	if (pwrdm == NULL || IS_ERR(pwrdm))
 		return -EINVAL;
@@ -127,6 +128,7 @@ int omap_set_pwrdm_state(struct powerdomain *pwrdm, u32 state)
 			(pwrdm->flags & PWRDM_HAS_LOWPOWERSTATECHANGE)) {
 			sleep_switch = LOWPOWERSTATE_SWITCH;
 		} else {
+			hwsup = clkdm_in_hwsup(pwrdm->pwrdm_clkdms[0]);
 			clkdm_wakeup(pwrdm->pwrdm_clkdms[0]);
 			pwrdm_wait_transition(pwrdm);
 			sleep_switch = FORCEWAKEUP_SWITCH;
@@ -142,7 +144,7 @@ int omap_set_pwrdm_state(struct powerdomain *pwrdm, u32 state)
 
 	switch (sleep_switch) {
 	case FORCEWAKEUP_SWITCH:
-		if (pwrdm->pwrdm_clkdms[0]->flags & CLKDM_CAN_ENABLE_AUTO)
+		if (hwsup)
 			clkdm_allow_idle(pwrdm->pwrdm_clkdms[0]);
 		else
 			clkdm_sleep(pwrdm->pwrdm_clkdms[0]);
-- 
1.6.6.1

