From b18bc7b18ebb99e06ae5052eccf722a2dad4aaec Mon Sep 17 00:00:00 2001
From: Tony Lindgren <tony@atomide.com>
Date: Tue, 29 Mar 2011 15:54:48 -0700
Subject: [PATCH 006/149] omap: Make a subset of dmtimer functions into inline functions

This will allow us to share the code between system timer and
dmtimer device driver code without having to initialize all the
dmtimers early. This change will also make the timer_set_next_event
more efficient as the inline functions will optimize the code
better for the timer reprogramming.

Signed-off-by: Tony Lindgren <tony@atomide.com>
Reviewed-by: Kevin Hilman <khilman@ti.com>
---
 arch/arm/plat-omap/dmtimer.c              |   78 ++++---------------
 arch/arm/plat-omap/include/plat/dmtimer.h |  119 +++++++++++++++++++++++++++++
 2 files changed, 136 insertions(+), 61 deletions(-)

diff --git a/arch/arm/plat-omap/dmtimer.c b/arch/arm/plat-omap/dmtimer.c
index dfdc3b2..7c5cb4e 100644
--- a/arch/arm/plat-omap/dmtimer.c
+++ b/arch/arm/plat-omap/dmtimer.c
@@ -170,11 +170,7 @@ static spinlock_t dm_timer_lock;
  */
 static inline u32 omap_dm_timer_read_reg(struct omap_dm_timer *timer, u32 reg)
 {
-	if (timer->posted)
-		while (readl(timer->io_base + (OMAP_TIMER_WRITE_PEND_REG & 0xff))
-				& (reg >> WPSHIFT))
-			cpu_relax();
-	return readl(timer->io_base + (reg & 0xff));
+	return __omap_dm_timer_read(timer->io_base, reg, timer->posted);
 }
 
 /*
@@ -186,11 +182,7 @@ static inline u32 omap_dm_timer_read_reg(struct omap_dm_timer *timer, u32 reg)
 static void omap_dm_timer_write_reg(struct omap_dm_timer *timer, u32 reg,
 						u32 value)
 {
-	if (timer->posted)
-		while (readl(timer->io_base + (OMAP_TIMER_WRITE_PEND_REG & 0xff))
-				& (reg >> WPSHIFT))
-			cpu_relax();
-	writel(value, timer->io_base + (reg & 0xff));
+	__omap_dm_timer_write(timer->io_base, reg, value, timer->posted);
 }
 
 static void omap_dm_timer_wait_for_reset(struct omap_dm_timer *timer)
@@ -209,7 +201,7 @@ static void omap_dm_timer_wait_for_reset(struct omap_dm_timer *timer)
 
 static void omap_dm_timer_reset(struct omap_dm_timer *timer)
 {
-	u32 l;
+	int autoidle = 0, wakeup = 0;
 
 	if (!cpu_class_is_omap2() || timer != &dm_timers[0]) {
 		omap_dm_timer_write_reg(timer, OMAP_TIMER_IF_CTRL_REG, 0x06);
@@ -217,28 +209,21 @@ static void omap_dm_timer_reset(struct omap_dm_timer *timer)
 	}
 	omap_dm_timer_set_source(timer, OMAP_TIMER_SRC_32_KHZ);
 
-	l = omap_dm_timer_read_reg(timer, OMAP_TIMER_OCP_CFG_REG);
-	l |= 0x02 << 3;  /* Set to smart-idle mode */
-	l |= 0x2 << 8;   /* Set clock activity to perserve f-clock on idle */
-
 	/* Enable autoidle on OMAP2 / OMAP3 */
 	if (cpu_is_omap24xx() || cpu_is_omap34xx())
-		l |= 0x1 << 0;
+		autoidle = 1;
 
 	/*
 	 * Enable wake-up on OMAP2 CPUs.
 	 */
 	if (cpu_class_is_omap2())
-		l |= 1 << 2;
-	omap_dm_timer_write_reg(timer, OMAP_TIMER_OCP_CFG_REG, l);
+		wakeup = 1;
 
-	/* Match hardware reset default of posted mode */
-	omap_dm_timer_write_reg(timer, OMAP_TIMER_IF_CTRL_REG,
-			OMAP_TIMER_CTRL_POSTED);
+	__omap_dm_timer_reset(timer->io_base, autoidle, wakeup);
 	timer->posted = 1;
 }
 
-static void omap_dm_timer_prepare(struct omap_dm_timer *timer)
+void omap_dm_timer_prepare(struct omap_dm_timer *timer)
 {
 	omap_dm_timer_enable(timer);
 	omap_dm_timer_reset(timer);
@@ -410,25 +395,13 @@ EXPORT_SYMBOL_GPL(omap_dm_timer_start);
 
 void omap_dm_timer_stop(struct omap_dm_timer *timer)
 {
-	u32 l;
+	unsigned long rate = 0;
 
-	l = omap_dm_timer_read_reg(timer, OMAP_TIMER_CTRL_REG);
-	if (l & OMAP_TIMER_CTRL_ST) {
-		l &= ~0x1;
-		omap_dm_timer_write_reg(timer, OMAP_TIMER_CTRL_REG, l);
 #ifdef CONFIG_ARCH_OMAP2PLUS
-		/* Readback to make sure write has completed */
-		omap_dm_timer_read_reg(timer, OMAP_TIMER_CTRL_REG);
-		 /*
-		  * Wait for functional clock period x 3.5 to make sure that
-		  * timer is stopped
-		  */
-		udelay(3500000 / clk_get_rate(timer->fclk) + 1);
+	rate = clk_get_rate(timer->fclk);
 #endif
-	}
-	/* Ack possibly pending interrupt */
-	omap_dm_timer_write_reg(timer, OMAP_TIMER_STAT_REG,
-			OMAP_TIMER_INT_OVERFLOW);
+
+	__omap_dm_timer_stop(timer->io_base, timer->posted, rate);
 }
 EXPORT_SYMBOL_GPL(omap_dm_timer_stop);
 
@@ -451,22 +424,11 @@ EXPORT_SYMBOL_GPL(omap_dm_timer_set_source);
 
 int omap_dm_timer_set_source(struct omap_dm_timer *timer, int source)
 {
-	int ret = -EINVAL;
-
 	if (source < 0 || source >= 3)
 		return -EINVAL;
 
-	clk_disable(timer->fclk);
-	ret = clk_set_parent(timer->fclk, dm_source_clocks[source]);
-	clk_enable(timer->fclk);
-
-	/*
-	 * When the functional clock disappears, too quick writes seem
-	 * to cause an abort. XXX Is this still necessary?
-	 */
-	__delay(300000);
-
-	return ret;
+	return __omap_dm_timer_set_source(timer->fclk,
+						dm_source_clocks[source]);
 }
 EXPORT_SYMBOL_GPL(omap_dm_timer_set_source);
 
@@ -504,8 +466,7 @@ void omap_dm_timer_set_load_start(struct omap_dm_timer *timer, int autoreload,
 	}
 	l |= OMAP_TIMER_CTRL_ST;
 
-	omap_dm_timer_write_reg(timer, OMAP_TIMER_COUNTER_REG, load);
-	omap_dm_timer_write_reg(timer, OMAP_TIMER_CTRL_REG, l);
+	__omap_dm_timer_load_start(timer->io_base, l, load, timer->posted);
 }
 EXPORT_SYMBOL_GPL(omap_dm_timer_set_load_start);
 
@@ -558,8 +519,7 @@ EXPORT_SYMBOL_GPL(omap_dm_timer_set_prescaler);
 void omap_dm_timer_set_int_enable(struct omap_dm_timer *timer,
 				  unsigned int value)
 {
-	omap_dm_timer_write_reg(timer, OMAP_TIMER_INT_EN_REG, value);
-	omap_dm_timer_write_reg(timer, OMAP_TIMER_WAKEUP_EN_REG, value);
+	__omap_dm_timer_int_enable(timer->io_base, value);
 }
 EXPORT_SYMBOL_GPL(omap_dm_timer_set_int_enable);
 
@@ -575,17 +535,13 @@ EXPORT_SYMBOL_GPL(omap_dm_timer_read_status);
 
 void omap_dm_timer_write_status(struct omap_dm_timer *timer, unsigned int value)
 {
-	omap_dm_timer_write_reg(timer, OMAP_TIMER_STAT_REG, value);
+	__omap_dm_timer_write_status(timer->io_base, value);
 }
 EXPORT_SYMBOL_GPL(omap_dm_timer_write_status);
 
 unsigned int omap_dm_timer_read_counter(struct omap_dm_timer *timer)
 {
-	unsigned int l;
-
-	l = omap_dm_timer_read_reg(timer, OMAP_TIMER_COUNTER_REG);
-
-	return l;
+	return __omap_dm_timer_read_counter(timer->io_base, timer->posted);
 }
 EXPORT_SYMBOL_GPL(omap_dm_timer_read_counter);
 
diff --git a/arch/arm/plat-omap/include/plat/dmtimer.h b/arch/arm/plat-omap/include/plat/dmtimer.h
index 3203105..54664a7 100644
--- a/arch/arm/plat-omap/include/plat/dmtimer.h
+++ b/arch/arm/plat-omap/include/plat/dmtimer.h
@@ -32,6 +32,9 @@
  * 675 Mass Ave, Cambridge, MA 02139, USA.
  */
 
+#include <linux/clk.h>
+#include <linux/delay.h>
+
 #ifndef __ASM_ARCH_DMTIMER_H
 #define __ASM_ARCH_DMTIMER_H
 
@@ -218,4 +221,120 @@ struct omap_dm_timer {
 	unsigned posted:1;
 };
 
+void omap_dm_timer_prepare(struct omap_dm_timer *timer);
+
+static inline u32 __omap_dm_timer_read(void __iomem *base, u32 reg,
+						int posted)
+{
+	if (posted)
+		while (__raw_readl(base + (OMAP_TIMER_WRITE_PEND_REG & 0xff))
+				& (reg >> WPSHIFT))
+			cpu_relax();
+
+	return __raw_readl(base + (reg & 0xff));
+}
+
+static inline void __omap_dm_timer_write(void __iomem *base, u32 reg, u32 val,
+						int posted)
+{
+	if (posted)
+		while (__raw_readl(base + (OMAP_TIMER_WRITE_PEND_REG & 0xff))
+				& (reg >> WPSHIFT))
+			cpu_relax();
+
+	__raw_writel(val, base + (reg & 0xff));
+}
+
+/* Assumes the source clock has been set by caller */
+static inline void __omap_dm_timer_reset(void __iomem *base, int autoidle,
+						int wakeup)
+{
+	u32 l;
+
+	l = __omap_dm_timer_read(base, OMAP_TIMER_OCP_CFG_REG, 0);
+	l |= 0x02 << 3;  /* Set to smart-idle mode */
+	l |= 0x2 << 8;   /* Set clock activity to perserve f-clock on idle */
+
+	if (autoidle)
+		l |= 0x1 << 0;
+
+	if (wakeup)
+		l |= 1 << 2;
+
+	__omap_dm_timer_write(base, OMAP_TIMER_OCP_CFG_REG, l, 0);
+
+	/* Match hardware reset default of posted mode */
+	__omap_dm_timer_write(base, OMAP_TIMER_IF_CTRL_REG,
+					OMAP_TIMER_CTRL_POSTED, 0);
+}
+
+static inline int __omap_dm_timer_set_source(struct clk *timer_fck,
+						struct clk *parent)
+{
+	int ret;
+
+	clk_disable(timer_fck);
+	ret = clk_set_parent(timer_fck, parent);
+	clk_enable(timer_fck);
+
+	/*
+	 * When the functional clock disappears, too quick writes seem
+	 * to cause an abort. XXX Is this still necessary?
+	 */
+	__delay(300000);
+
+	return ret;
+}
+
+static inline void __omap_dm_timer_stop(void __iomem *base, int posted,
+						unsigned long rate)
+{
+	u32 l;
+
+	l = __omap_dm_timer_read(base, OMAP_TIMER_CTRL_REG, posted);
+	if (l & OMAP_TIMER_CTRL_ST) {
+		l &= ~0x1;
+		__omap_dm_timer_write(base, OMAP_TIMER_CTRL_REG, l, posted);
+#ifdef CONFIG_ARCH_OMAP2PLUS
+		/* Readback to make sure write has completed */
+		__omap_dm_timer_read(base, OMAP_TIMER_CTRL_REG, posted);
+		/*
+		 * Wait for functional clock period x 3.5 to make sure that
+		 * timer is stopped
+		 */
+		udelay(3500000 / rate + 1);
+#endif
+	}
+
+	/* Ack possibly pending interrupt */
+	__omap_dm_timer_write(base, OMAP_TIMER_STAT_REG,
+					OMAP_TIMER_INT_OVERFLOW, 0);
+}
+
+static inline void __omap_dm_timer_load_start(void __iomem *base, u32 ctrl,
+						unsigned int load, int posted)
+{
+	__omap_dm_timer_write(base, OMAP_TIMER_COUNTER_REG, load, posted);
+	__omap_dm_timer_write(base, OMAP_TIMER_CTRL_REG, ctrl, posted);
+}
+
+static inline void __omap_dm_timer_int_enable(void __iomem *base,
+						unsigned int value)
+{
+	__omap_dm_timer_write(base, OMAP_TIMER_INT_EN_REG, value, 0);
+	__omap_dm_timer_write(base, OMAP_TIMER_WAKEUP_EN_REG, value, 0);
+}
+
+static inline unsigned int __omap_dm_timer_read_counter(void __iomem *base,
+							int posted)
+{
+	return __omap_dm_timer_read(base, OMAP_TIMER_COUNTER_REG, posted);
+}
+
+static inline void __omap_dm_timer_write_status(void __iomem *base,
+						unsigned int value)
+{
+	__omap_dm_timer_write(base, OMAP_TIMER_STAT_REG, value, 0);
+}
+
 #endif /* __ASM_ARCH_DMTIMER_H */
-- 
1.6.6.1

