From b10de9a3ea356e2e0994f9b248f140f3807a6cd4 Mon Sep 17 00:00:00 2001
From: Tony Lindgren <tony@atomide.com>
Date: Tue, 29 Mar 2011 15:54:48 -0700
Subject: [PATCH 004/149] omap: Set separate timer init functions to avoid cpu_is_omap tests

This is needed for the following patches so we can initialize the
rest of the hardware timers later on.

As with the init_irq calls, there's no need to do cpu_is_omap calls
during the timer init as we only care about the major omap generation.
This means that we can initialize the sys_timer with the .timer
entries alone.

Note that for now we just set stubs for the various sys_timer entries
that will get populated in a later patch. The following patches will
also remove the omap_dm_timer_init calls and change the init for the
rest of the hardware timers to happen with an arch_initcall.

Signed-off-by: Tony Lindgren <tony@atomide.com>
Reviewed-by: Kevin Hilman <khilman@ti.com>
---
 arch/arm/mach-omap1/board-ams-delta.c      |    2 +-
 arch/arm/mach-omap1/board-fsample.c        |    2 +-
 arch/arm/mach-omap1/board-generic.c        |    2 +-
 arch/arm/mach-omap1/board-h2.c             |    2 +-
 arch/arm/mach-omap1/board-h3.c             |    2 +-
 arch/arm/mach-omap1/board-htcherald.c      |    2 +-
 arch/arm/mach-omap1/board-innovator.c      |    2 +-
 arch/arm/mach-omap1/board-nokia770.c       |    2 +-
 arch/arm/mach-omap1/board-osk.c            |    2 +-
 arch/arm/mach-omap1/board-palmte.c         |    2 +-
 arch/arm/mach-omap1/board-palmtt.c         |    2 +-
 arch/arm/mach-omap1/board-palmz71.c        |    2 +-
 arch/arm/mach-omap1/board-perseus2.c       |    2 +-
 arch/arm/mach-omap1/board-sx1.c            |    2 +-
 arch/arm/mach-omap1/board-voiceblue.c      |    2 +-
 arch/arm/mach-omap1/time.c                 |    6 ++--
 arch/arm/mach-omap2/board-2430sdp.c        |    2 +-
 arch/arm/mach-omap2/board-3430sdp.c        |    2 +-
 arch/arm/mach-omap2/board-3630sdp.c        |    2 +-
 arch/arm/mach-omap2/board-4430sdp.c        |    2 +-
 arch/arm/mach-omap2/board-am3517crane.c    |    2 +-
 arch/arm/mach-omap2/board-am3517evm.c      |    2 +-
 arch/arm/mach-omap2/board-apollon.c        |    2 +-
 arch/arm/mach-omap2/board-cm-t35.c         |    2 +-
 arch/arm/mach-omap2/board-cm-t3517.c       |    2 +-
 arch/arm/mach-omap2/board-devkit8000.c     |    2 +-
 arch/arm/mach-omap2/board-generic.c        |    2 +-
 arch/arm/mach-omap2/board-h4.c             |    2 +-
 arch/arm/mach-omap2/board-igep0020.c       |    4 +-
 arch/arm/mach-omap2/board-ldp.c            |    2 +-
 arch/arm/mach-omap2/board-n8x0.c           |    6 ++--
 arch/arm/mach-omap2/board-omap3beagle.c    |    2 +-
 arch/arm/mach-omap2/board-omap3evm.c       |    2 +-
 arch/arm/mach-omap2/board-omap3logic.c     |    4 +-
 arch/arm/mach-omap2/board-omap3pandora.c   |    2 +-
 arch/arm/mach-omap2/board-omap3stalker.c   |    2 +-
 arch/arm/mach-omap2/board-omap3touchbook.c |    2 +-
 arch/arm/mach-omap2/board-omap4panda.c     |    2 +-
 arch/arm/mach-omap2/board-overo.c          |    2 +-
 arch/arm/mach-omap2/board-rm680.c          |    2 +-
 arch/arm/mach-omap2/board-rx51.c           |    2 +-
 arch/arm/mach-omap2/board-ti8168evm.c      |    2 +-
 arch/arm/mach-omap2/board-zoom.c           |    4 +-
 arch/arm/mach-omap2/timer-gp.c             |   41 +++++++++++++++++++++-------
 arch/arm/plat-omap/include/plat/common.h   |    6 +++-
 arch/arm/plat-omap/include/plat/dmtimer.h  |    1 -
 46 files changed, 86 insertions(+), 62 deletions(-)

diff --git a/arch/arm/mach-omap1/board-ams-delta.c b/arch/arm/mach-omap1/board-ams-delta.c
index e3caef8..312ea6b 100644
--- a/arch/arm/mach-omap1/board-ams-delta.c
+++ b/arch/arm/mach-omap1/board-ams-delta.c
@@ -391,7 +391,7 @@ MACHINE_START(AMS_DELTA, "Amstrad E3 (Delta)")
 	.reserve	= omap_reserve,
 	.init_irq	= ams_delta_init_irq,
 	.init_machine	= ams_delta_init,
-	.timer		= &omap_timer,
+	.timer		= &omap1_timer,
 MACHINE_END
 
 EXPORT_SYMBOL(ams_delta_latch1_write);
diff --git a/arch/arm/mach-omap1/board-fsample.c b/arch/arm/mach-omap1/board-fsample.c
index eaff305..a6b1bea 100644
--- a/arch/arm/mach-omap1/board-fsample.c
+++ b/arch/arm/mach-omap1/board-fsample.c
@@ -394,5 +394,5 @@ MACHINE_START(OMAP_FSAMPLE, "OMAP730 F-Sample")
 	.reserve	= omap_reserve,
 	.init_irq	= omap_fsample_init_irq,
 	.init_machine	= omap_fsample_init,
-	.timer		= &omap_timer,
+	.timer		= &omap1_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap1/board-generic.c b/arch/arm/mach-omap1/board-generic.c
index 3fd6b40..04fc356 100644
--- a/arch/arm/mach-omap1/board-generic.c
+++ b/arch/arm/mach-omap1/board-generic.c
@@ -99,5 +99,5 @@ MACHINE_START(OMAP_GENERIC, "Generic OMAP1510/1610/1710")
 	.reserve	= omap_reserve,
 	.init_irq	= omap_generic_init_irq,
 	.init_machine	= omap_generic_init,
-	.timer		= &omap_timer,
+	.timer		= &omap1_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap1/board-h2.c b/arch/arm/mach-omap1/board-h2.c
index 8147b04..cb7fb1a 100644
--- a/arch/arm/mach-omap1/board-h2.c
+++ b/arch/arm/mach-omap1/board-h2.c
@@ -466,5 +466,5 @@ MACHINE_START(OMAP_H2, "TI-H2")
 	.reserve	= omap_reserve,
 	.init_irq	= h2_init_irq,
 	.init_machine	= h2_init,
-	.timer		= &omap_timer,
+	.timer		= &omap1_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap1/board-h3.c b/arch/arm/mach-omap1/board-h3.c
index 1b448f6..31f3487 100644
--- a/arch/arm/mach-omap1/board-h3.c
+++ b/arch/arm/mach-omap1/board-h3.c
@@ -454,5 +454,5 @@ MACHINE_START(OMAP_H3, "TI OMAP1710 H3 board")
 	.reserve	= omap_reserve,
 	.init_irq	= h3_init_irq,
 	.init_machine	= h3_init,
-	.timer		= &omap_timer,
+	.timer		= &omap1_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap1/board-htcherald.c b/arch/arm/mach-omap1/board-htcherald.c
index 1bd4d8e..36e06ea 100644
--- a/arch/arm/mach-omap1/board-htcherald.c
+++ b/arch/arm/mach-omap1/board-htcherald.c
@@ -616,5 +616,5 @@ MACHINE_START(HERALD, "HTC Herald")
 	.reserve	= omap_reserve,
 	.init_irq       = htcherald_init_irq,
 	.init_machine   = htcherald_init,
-	.timer          = &omap_timer,
+	.timer          = &omap1_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap1/board-innovator.c b/arch/arm/mach-omap1/board-innovator.c
index 5926b0c..0b1ba46 100644
--- a/arch/arm/mach-omap1/board-innovator.c
+++ b/arch/arm/mach-omap1/board-innovator.c
@@ -464,5 +464,5 @@ MACHINE_START(OMAP_INNOVATOR, "TI-Innovator")
 	.reserve	= omap_reserve,
 	.init_irq	= innovator_init_irq,
 	.init_machine	= innovator_init,
-	.timer		= &omap_timer,
+	.timer		= &omap1_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap1/board-nokia770.c b/arch/arm/mach-omap1/board-nokia770.c
index e3cf21d..5469ce2 100644
--- a/arch/arm/mach-omap1/board-nokia770.c
+++ b/arch/arm/mach-omap1/board-nokia770.c
@@ -269,5 +269,5 @@ MACHINE_START(NOKIA770, "Nokia 770")
 	.reserve	= omap_reserve,
 	.init_irq	= omap_nokia770_init_irq,
 	.init_machine	= omap_nokia770_init,
-	.timer		= &omap_timer,
+	.timer		= &omap1_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap1/board-osk.c b/arch/arm/mach-omap1/board-osk.c
index 1e7823d..b08a213 100644
--- a/arch/arm/mach-omap1/board-osk.c
+++ b/arch/arm/mach-omap1/board-osk.c
@@ -588,5 +588,5 @@ MACHINE_START(OMAP_OSK, "TI-OSK")
 	.reserve	= omap_reserve,
 	.init_irq	= osk_init_irq,
 	.init_machine	= osk_init,
-	.timer		= &omap_timer,
+	.timer		= &omap1_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap1/board-palmte.c b/arch/arm/mach-omap1/board-palmte.c
index 8b6a881..459cb6b 100644
--- a/arch/arm/mach-omap1/board-palmte.c
+++ b/arch/arm/mach-omap1/board-palmte.c
@@ -280,5 +280,5 @@ MACHINE_START(OMAP_PALMTE, "OMAP310 based Palm Tungsten E")
 	.reserve	= omap_reserve,
 	.init_irq	= omap_palmte_init_irq,
 	.init_machine	= omap_palmte_init,
-	.timer		= &omap_timer,
+	.timer		= &omap1_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap1/board-palmtt.c b/arch/arm/mach-omap1/board-palmtt.c
index f2de43d..b214f45 100644
--- a/arch/arm/mach-omap1/board-palmtt.c
+++ b/arch/arm/mach-omap1/board-palmtt.c
@@ -326,5 +326,5 @@ MACHINE_START(OMAP_PALMTT, "OMAP1510 based Palm Tungsten|T")
 	.reserve	= omap_reserve,
 	.init_irq	= omap_palmtt_init_irq,
 	.init_machine	= omap_palmtt_init,
-	.timer		= &omap_timer,
+	.timer		= &omap1_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap1/board-palmz71.c b/arch/arm/mach-omap1/board-palmz71.c
index 6665d2d..9b0ea48 100644
--- a/arch/arm/mach-omap1/board-palmz71.c
+++ b/arch/arm/mach-omap1/board-palmz71.c
@@ -346,5 +346,5 @@ MACHINE_START(OMAP_PALMZ71, "OMAP310 based Palm Zire71")
 	.reserve	= omap_reserve,
 	.init_irq	= omap_palmz71_init_irq,
 	.init_machine	= omap_palmz71_init,
-	.timer		= &omap_timer,
+	.timer		= &omap1_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap1/board-perseus2.c b/arch/arm/mach-omap1/board-perseus2.c
index 7f019e5..67acd41 100644
--- a/arch/arm/mach-omap1/board-perseus2.c
+++ b/arch/arm/mach-omap1/board-perseus2.c
@@ -355,5 +355,5 @@ MACHINE_START(OMAP_PERSEUS2, "OMAP730 Perseus2")
 	.reserve	= omap_reserve,
 	.init_irq	= omap_perseus2_init_irq,
 	.init_machine	= omap_perseus2_init,
-	.timer		= &omap_timer,
+	.timer		= &omap1_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap1/board-sx1.c b/arch/arm/mach-omap1/board-sx1.c
index 24f0f7b..9c3b7c5 100644
--- a/arch/arm/mach-omap1/board-sx1.c
+++ b/arch/arm/mach-omap1/board-sx1.c
@@ -426,5 +426,5 @@ MACHINE_START(SX1, "OMAP310 based Siemens SX1")
 	.reserve	= omap_reserve,
 	.init_irq	= omap_sx1_init_irq,
 	.init_machine	= omap_sx1_init,
-	.timer		= &omap_timer,
+	.timer		= &omap1_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap1/board-voiceblue.c b/arch/arm/mach-omap1/board-voiceblue.c
index 98826e2..036edc0 100644
--- a/arch/arm/mach-omap1/board-voiceblue.c
+++ b/arch/arm/mach-omap1/board-voiceblue.c
@@ -306,5 +306,5 @@ MACHINE_START(VOICEBLUE, "VoiceBlue OMAP5910")
 	.reserve	= omap_reserve,
 	.init_irq	= voiceblue_init_irq,
 	.init_machine	= voiceblue_init,
-	.timer		= &omap_timer,
+	.timer		= &omap1_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap1/time.c b/arch/arm/mach-omap1/time.c
index 03e1e10..a183777 100644
--- a/arch/arm/mach-omap1/time.c
+++ b/arch/arm/mach-omap1/time.c
@@ -297,7 +297,7 @@ static inline int omap_32k_timer_usable(void)
  * Timer initialization
  * ---------------------------------------------------------------------------
  */
-static void __init omap_timer_init(void)
+static void __init omap1_timer_init(void)
 {
 	if (omap_32k_timer_usable()) {
 		preferred_sched_clock_init(1);
@@ -307,6 +307,6 @@ static void __init omap_timer_init(void)
 	}
 }
 
-struct sys_timer omap_timer = {
-	.init		= omap_timer_init,
+struct sys_timer omap1_timer = {
+	.init		= omap1_timer_init,
 };
diff --git a/arch/arm/mach-omap2/board-2430sdp.c b/arch/arm/mach-omap2/board-2430sdp.c
index 45cabc5..2028464 100644
--- a/arch/arm/mach-omap2/board-2430sdp.c
+++ b/arch/arm/mach-omap2/board-2430sdp.c
@@ -262,5 +262,5 @@ MACHINE_START(OMAP_2430SDP, "OMAP2430 sdp2430 board")
 	.init_early	= omap_2430sdp_init_early,
 	.init_irq	= omap2_init_irq,
 	.init_machine	= omap_2430sdp_init,
-	.timer		= &omap_timer,
+	.timer		= &omap2_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-3430sdp.c b/arch/arm/mach-omap2/board-3430sdp.c
index 85b207f..12fae21 100644
--- a/arch/arm/mach-omap2/board-3430sdp.c
+++ b/arch/arm/mach-omap2/board-3430sdp.c
@@ -806,5 +806,5 @@ MACHINE_START(OMAP_3430SDP, "OMAP3430 3430SDP board")
 	.init_early	= omap_3430sdp_init_early,
 	.init_irq	= omap3_init_irq,
 	.init_machine	= omap_3430sdp_init,
-	.timer		= &omap_timer,
+	.timer		= &omap3_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-3630sdp.c b/arch/arm/mach-omap2/board-3630sdp.c
index 2ec2d76..e4f37b5 100644
--- a/arch/arm/mach-omap2/board-3630sdp.c
+++ b/arch/arm/mach-omap2/board-3630sdp.c
@@ -221,5 +221,5 @@ MACHINE_START(OMAP_3630SDP, "OMAP 3630SDP board")
 	.init_early	= omap_sdp_init_early,
 	.init_irq	= omap3_init_irq,
 	.init_machine	= omap_sdp_init,
-	.timer		= &omap_timer,
+	.timer		= &omap3_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-4430sdp.c b/arch/arm/mach-omap2/board-4430sdp.c
index 39a8062..e8caced 100644
--- a/arch/arm/mach-omap2/board-4430sdp.c
+++ b/arch/arm/mach-omap2/board-4430sdp.c
@@ -768,5 +768,5 @@ MACHINE_START(OMAP_4430SDP, "OMAP4430 4430SDP board")
 	.init_early	= omap_4430sdp_init_early,
 	.init_irq	= gic_init_irq,
 	.init_machine	= omap_4430sdp_init,
-	.timer		= &omap_timer,
+	.timer		= &omap4_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-am3517crane.c b/arch/arm/mach-omap2/board-am3517crane.c
index 0bed0a4..5f2b55f 100644
--- a/arch/arm/mach-omap2/board-am3517crane.c
+++ b/arch/arm/mach-omap2/board-am3517crane.c
@@ -106,5 +106,5 @@ MACHINE_START(CRANEBOARD, "AM3517/05 CRANEBOARD")
 	.init_early	= am3517_crane_init_early,
 	.init_irq	= omap3_init_irq,
 	.init_machine	= am3517_crane_init,
-	.timer		= &omap_timer,
+	.timer		= &omap3_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-am3517evm.c b/arch/arm/mach-omap2/board-am3517evm.c
index 0db0fb8..f3006c3 100644
--- a/arch/arm/mach-omap2/board-am3517evm.c
+++ b/arch/arm/mach-omap2/board-am3517evm.c
@@ -496,5 +496,5 @@ MACHINE_START(OMAP3517EVM, "OMAP3517/AM3517 EVM")
 	.init_early	= am3517_evm_init_early,
 	.init_irq	= omap3_init_irq,
 	.init_machine	= am3517_evm_init,
-	.timer		= &omap_timer,
+	.timer		= &omap3_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-apollon.c b/arch/arm/mach-omap2/board-apollon.c
index 93576c8..7021170 100644
--- a/arch/arm/mach-omap2/board-apollon.c
+++ b/arch/arm/mach-omap2/board-apollon.c
@@ -356,5 +356,5 @@ MACHINE_START(OMAP_APOLLON, "OMAP24xx Apollon")
 	.init_early	= omap_apollon_init_early,
 	.init_irq	= omap2_init_irq,
 	.init_machine	= omap_apollon_init,
-	.timer		= &omap_timer,
+	.timer		= &omap2_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-cm-t35.c b/arch/arm/mach-omap2/board-cm-t35.c
index 43b1de5..1a18d3b 100644
--- a/arch/arm/mach-omap2/board-cm-t35.c
+++ b/arch/arm/mach-omap2/board-cm-t35.c
@@ -646,5 +646,5 @@ MACHINE_START(CM_T35, "Compulab CM-T35")
 	.init_early	= cm_t35_init_early,
 	.init_irq	= omap3_init_irq,
 	.init_machine	= cm_t35_init,
-	.timer		= &omap_timer,
+	.timer		= &omap3_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-cm-t3517.c b/arch/arm/mach-omap2/board-cm-t3517.c
index 8f15222..aa67240 100644
--- a/arch/arm/mach-omap2/board-cm-t3517.c
+++ b/arch/arm/mach-omap2/board-cm-t3517.c
@@ -306,5 +306,5 @@ MACHINE_START(CM_T3517, "Compulab CM-T3517")
 	.init_early	= cm_t3517_init_early,
 	.init_irq	= omap3_init_irq,
 	.init_machine	= cm_t3517_init,
-	.timer		= &omap_timer,
+	.timer		= &omap3_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-devkit8000.c b/arch/arm/mach-omap2/board-devkit8000.c
index 73f3a22..46d144d 100644
--- a/arch/arm/mach-omap2/board-devkit8000.c
+++ b/arch/arm/mach-omap2/board-devkit8000.c
@@ -709,5 +709,5 @@ MACHINE_START(DEVKIT8000, "OMAP3 Devkit8000")
 	.init_early	= devkit8000_init_early,
 	.init_irq	= devkit8000_init_irq,
 	.init_machine	= devkit8000_init,
-	.timer		= &omap_timer,
+	.timer		= &omap3_secure_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-generic.c b/arch/arm/mach-omap2/board-generic.c
index ccd503a..c6ecf60 100644
--- a/arch/arm/mach-omap2/board-generic.c
+++ b/arch/arm/mach-omap2/board-generic.c
@@ -72,5 +72,5 @@ MACHINE_START(OMAP_GENERIC, "Generic OMAP24xx")
 	.init_early	= omap_generic_init_early,
 	.init_irq	= omap2_init_irq,
 	.init_machine	= omap_generic_init,
-	.timer		= &omap_timer,
+	.timer		= &omap3_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-h4.c b/arch/arm/mach-omap2/board-h4.c
index 2e16d6c..45de2b3 100644
--- a/arch/arm/mach-omap2/board-h4.c
+++ b/arch/arm/mach-omap2/board-h4.c
@@ -388,5 +388,5 @@ MACHINE_START(OMAP_H4, "OMAP2420 H4 board")
 	.init_early	= omap_h4_init_early,
 	.init_irq	= omap_h4_init_irq,
 	.init_machine	= omap_h4_init,
-	.timer		= &omap_timer,
+	.timer		= &omap2_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-igep0020.c b/arch/arm/mach-omap2/board-igep0020.c
index f22a76a..f683835 100644
--- a/arch/arm/mach-omap2/board-igep0020.c
+++ b/arch/arm/mach-omap2/board-igep0020.c
@@ -708,7 +708,7 @@ MACHINE_START(IGEP0020, "IGEP v2 board")
 	.init_early	= igep_init_early,
 	.init_irq	= omap3_init_irq,
 	.init_machine	= igep_init,
-	.timer		= &omap_timer,
+	.timer		= &omap3_timer,
 MACHINE_END
 
 MACHINE_START(IGEP0030, "IGEP OMAP3 module")
@@ -718,5 +718,5 @@ MACHINE_START(IGEP0030, "IGEP OMAP3 module")
 	.init_early	= igep_init_early,
 	.init_irq	= omap3_init_irq,
 	.init_machine	= igep_init,
-	.timer		= &omap_timer,
+	.timer		= &omap3_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-ldp.c b/arch/arm/mach-omap2/board-ldp.c
index 9671843..5d4328f 100644
--- a/arch/arm/mach-omap2/board-ldp.c
+++ b/arch/arm/mach-omap2/board-ldp.c
@@ -350,5 +350,5 @@ MACHINE_START(OMAP_LDP, "OMAP LDP board")
 	.init_early	= omap_ldp_init_early,
 	.init_irq	= omap3_init_irq,
 	.init_machine	= omap_ldp_init,
-	.timer		= &omap_timer,
+	.timer		= &omap3_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-n8x0.c b/arch/arm/mach-omap2/board-n8x0.c
index 9c791a2..e11f0c5 100644
--- a/arch/arm/mach-omap2/board-n8x0.c
+++ b/arch/arm/mach-omap2/board-n8x0.c
@@ -701,7 +701,7 @@ MACHINE_START(NOKIA_N800, "Nokia N800")
 	.init_early	= n8x0_init_early,
 	.init_irq	= omap2_init_irq,
 	.init_machine	= n8x0_init_machine,
-	.timer		= &omap_timer,
+	.timer		= &omap2_timer,
 MACHINE_END
 
 MACHINE_START(NOKIA_N810, "Nokia N810")
@@ -711,7 +711,7 @@ MACHINE_START(NOKIA_N810, "Nokia N810")
 	.init_early	= n8x0_init_early,
 	.init_irq	= omap2_init_irq,
 	.init_machine	= n8x0_init_machine,
-	.timer		= &omap_timer,
+	.timer		= &omap2_timer,
 MACHINE_END
 
 MACHINE_START(NOKIA_N810_WIMAX, "Nokia N810 WiMAX")
@@ -721,5 +721,5 @@ MACHINE_START(NOKIA_N810_WIMAX, "Nokia N810 WiMAX")
 	.init_early	= n8x0_init_early,
 	.init_irq	= omap2_init_irq,
 	.init_machine	= n8x0_init_machine,
-	.timer		= &omap_timer,
+	.timer		= &omap2_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-omap3beagle.c b/arch/arm/mach-omap2/board-omap3beagle.c
index eaead5e..9ee16f6 100644
--- a/arch/arm/mach-omap2/board-omap3beagle.c
+++ b/arch/arm/mach-omap2/board-omap3beagle.c
@@ -596,5 +596,5 @@ MACHINE_START(OMAP3_BEAGLE, "OMAP3 Beagle Board")
 	.init_early	= omap3_beagle_init_early,
 	.init_irq	= omap3_beagle_init_irq,
 	.init_machine	= omap3_beagle_init,
-	.timer		= &omap_timer,
+	.timer		= &omap3_secure_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-omap3evm.c b/arch/arm/mach-omap2/board-omap3evm.c
index d39f53f..6f957ed 100644
--- a/arch/arm/mach-omap2/board-omap3evm.c
+++ b/arch/arm/mach-omap2/board-omap3evm.c
@@ -741,5 +741,5 @@ MACHINE_START(OMAP3EVM, "OMAP3 EVM")
 	.init_early	= omap3_evm_init_early,
 	.init_irq	= omap3_init_irq,
 	.init_machine	= omap3_evm_init,
-	.timer		= &omap_timer,
+	.timer		= &omap3_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-omap3logic.c b/arch/arm/mach-omap2/board-omap3logic.c
index b63f1c2..469259a 100644
--- a/arch/arm/mach-omap2/board-omap3logic.c
+++ b/arch/arm/mach-omap2/board-omap3logic.c
@@ -215,7 +215,7 @@ MACHINE_START(OMAP3_TORPEDO, "Logic OMAP3 Torpedo board")
 	.init_early	= omap3logic_init_early,
 	.init_irq	= omap3_init_irq,
 	.init_machine	= omap3logic_init,
-	.timer		= &omap_timer,
+	.timer		= &omap3_timer,
 MACHINE_END
 
 MACHINE_START(OMAP3530_LV_SOM, "OMAP Logic 3530 LV SOM board")
@@ -224,5 +224,5 @@ MACHINE_START(OMAP3530_LV_SOM, "OMAP Logic 3530 LV SOM board")
 	.init_early	= omap3logic_init_early,
 	.init_irq	= omap3_init_irq,
 	.init_machine	= omap3logic_init,
-	.timer		= &omap_timer,
+	.timer		= &omap3_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-omap3pandora.c b/arch/arm/mach-omap2/board-omap3pandora.c
index 1d90b90..d4ea940 100644
--- a/arch/arm/mach-omap2/board-omap3pandora.c
+++ b/arch/arm/mach-omap2/board-omap3pandora.c
@@ -652,5 +652,5 @@ MACHINE_START(OMAP3_PANDORA, "Pandora Handheld Console")
 	.init_early	= omap3pandora_init_early,
 	.init_irq	= omap3_init_irq,
 	.init_machine	= omap3pandora_init,
-	.timer		= &omap_timer,
+	.timer		= &omap3_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-omap3stalker.c b/arch/arm/mach-omap2/board-omap3stalker.c
index dfa1401..2fa8fae 100644
--- a/arch/arm/mach-omap2/board-omap3stalker.c
+++ b/arch/arm/mach-omap2/board-omap3stalker.c
@@ -557,5 +557,5 @@ MACHINE_START(SBC3530, "OMAP3 STALKER")
 	.init_early		= omap3_stalker_init_early,
 	.init_irq		= omap3_stalker_init_irq,
 	.init_machine		= omap3_stalker_init,
-	.timer			= &omap_timer,
+	.timer			= &omap3_secure_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-omap3touchbook.c b/arch/arm/mach-omap2/board-omap3touchbook.c
index ae97910..8c71fd2 100644
--- a/arch/arm/mach-omap2/board-omap3touchbook.c
+++ b/arch/arm/mach-omap2/board-omap3touchbook.c
@@ -449,5 +449,5 @@ MACHINE_START(TOUCHBOOK, "OMAP3 touchbook Board")
 	.init_early	= omap3_touchbook_init_early,
 	.init_irq	= omap3_touchbook_init_irq,
 	.init_machine	= omap3_touchbook_init,
-	.timer		= &omap_timer,
+	.timer		= &omap3_secure_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-omap4panda.c b/arch/arm/mach-omap2/board-omap4panda.c
index 6d2372b..dc1d6dc 100644
--- a/arch/arm/mach-omap2/board-omap4panda.c
+++ b/arch/arm/mach-omap2/board-omap4panda.c
@@ -712,5 +712,5 @@ MACHINE_START(OMAP4_PANDA, "OMAP4 Panda board")
 	.init_early	= omap4_panda_init_early,
 	.init_irq	= gic_init_irq,
 	.init_machine	= omap4_panda_init,
-	.timer		= &omap_timer,
+	.timer		= &omap4_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-overo.c b/arch/arm/mach-omap2/board-overo.c
index e3928f2..1bf2f39 100644
--- a/arch/arm/mach-omap2/board-overo.c
+++ b/arch/arm/mach-omap2/board-overo.c
@@ -617,5 +617,5 @@ MACHINE_START(OVERO, "Gumstix Overo")
 	.init_early	= overo_init_early,
 	.init_irq	= omap3_init_irq,
 	.init_machine	= overo_init,
-	.timer		= &omap_timer,
+	.timer		= &omap3_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-rm680.c b/arch/arm/mach-omap2/board-rm680.c
index 9c3d115..54dceb1 100644
--- a/arch/arm/mach-omap2/board-rm680.c
+++ b/arch/arm/mach-omap2/board-rm680.c
@@ -165,5 +165,5 @@ MACHINE_START(NOKIA_RM680, "Nokia RM-680 board")
 	.init_early	= rm680_init_early,
 	.init_irq	= omap3_init_irq,
 	.init_machine	= rm680_init,
-	.timer		= &omap_timer,
+	.timer		= &omap3_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-rx51.c b/arch/arm/mach-omap2/board-rx51.c
index ee35e4e..5ea142f 100644
--- a/arch/arm/mach-omap2/board-rx51.c
+++ b/arch/arm/mach-omap2/board-rx51.c
@@ -162,5 +162,5 @@ MACHINE_START(NOKIA_RX51, "Nokia RX-51 board")
 	.init_early	= rx51_init_early,
 	.init_irq	= omap3_init_irq,
 	.init_machine	= rx51_init,
-	.timer		= &omap_timer,
+	.timer		= &omap3_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-ti8168evm.c b/arch/arm/mach-omap2/board-ti8168evm.c
index 713c20f..a85d5b0 100644
--- a/arch/arm/mach-omap2/board-ti8168evm.c
+++ b/arch/arm/mach-omap2/board-ti8168evm.c
@@ -52,6 +52,6 @@ MACHINE_START(TI8168EVM, "ti8168evm")
 	.map_io		= ti8168_evm_map_io,
 	.init_early	= ti8168_init_early,
 	.init_irq	= ti816x_init_irq,
-	.timer		= &omap_timer,
+	.timer		= &omap3_timer,
 	.init_machine	= ti8168_evm_init,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/board-zoom.c b/arch/arm/mach-omap2/board-zoom.c
index 97a3f0b..8a98c3c 100644
--- a/arch/arm/mach-omap2/board-zoom.c
+++ b/arch/arm/mach-omap2/board-zoom.c
@@ -139,7 +139,7 @@ MACHINE_START(OMAP_ZOOM2, "OMAP Zoom2 board")
 	.init_early	= omap_zoom_init_early,
 	.init_irq	= omap3_init_irq,
 	.init_machine	= omap_zoom_init,
-	.timer		= &omap_timer,
+	.timer		= &omap3_timer,
 MACHINE_END
 
 MACHINE_START(OMAP_ZOOM3, "OMAP Zoom3 board")
@@ -149,5 +149,5 @@ MACHINE_START(OMAP_ZOOM3, "OMAP Zoom3 board")
 	.init_early	= omap_zoom_init_early,
 	.init_irq	= omap3_init_irq,
 	.init_machine	= omap_zoom_init,
-	.timer		= &omap_timer,
+	.timer		= &omap3_timer,
 MACHINE_END
diff --git a/arch/arm/mach-omap2/timer-gp.c b/arch/arm/mach-omap2/timer-gp.c
index 3b9cf85..a0d8e83 100644
--- a/arch/arm/mach-omap2/timer-gp.c
+++ b/arch/arm/mach-omap2/timer-gp.c
@@ -247,20 +247,41 @@ static void __init omap2_gp_clocksource_init(void)
 }
 #endif
 
-static void __init omap2_gp_timer_init(void)
+#define OMAP_SYS_TIMER_INIT(name)					\
+static void __init omap##name##_timer_init(void)			\
+{									\
+	omap_dm_timer_init();						\
+	omap2_gp_clockevent_init();					\
+	omap2_gp_clocksource_init();					\
+}
+
+#define OMAP_SYS_TIMER(name)						\
+struct sys_timer omap##name##_timer = {					\
+	.init	= omap##name##_timer_init,				\
+};
+
+#ifdef CONFIG_ARCH_OMAP2
+OMAP_SYS_TIMER_INIT(2)
+OMAP_SYS_TIMER(2)
+#endif
+
+#ifdef CONFIG_ARCH_OMAP3
+OMAP_SYS_TIMER_INIT(3)
+OMAP_SYS_TIMER(3)
+OMAP_SYS_TIMER_INIT(3_secure)
+OMAP_SYS_TIMER(3_secure)
+#endif
+
+#ifdef CONFIG_ARCH_OMAP4
+static void __init omap4_timer_init(void)
 {
 #ifdef CONFIG_LOCAL_TIMERS
-	if (cpu_is_omap44xx()) {
-		twd_base = ioremap(OMAP44XX_LOCAL_TWD_BASE, SZ_256);
-		BUG_ON(!twd_base);
-	}
+	twd_base = ioremap(OMAP44XX_LOCAL_TWD_BASE, SZ_256);
+	BUG_ON(!twd_base);
 #endif
 	omap_dm_timer_init();
-
 	omap2_gp_clockevent_init();
 	omap2_gp_clocksource_init();
 }
-
-struct sys_timer omap_timer = {
-	.init	= omap2_gp_timer_init,
-};
+OMAP_SYS_TIMER(4)
+#endif
diff --git a/arch/arm/plat-omap/include/plat/common.h b/arch/arm/plat-omap/include/plat/common.h
index 5288130..4564cc6 100644
--- a/arch/arm/plat-omap/include/plat/common.h
+++ b/arch/arm/plat-omap/include/plat/common.h
@@ -34,7 +34,11 @@
 struct sys_timer;
 
 extern void omap_map_common_io(void);
-extern struct sys_timer omap_timer;
+extern struct sys_timer omap1_timer;
+extern struct sys_timer omap2_timer;
+extern struct sys_timer omap3_timer;
+extern struct sys_timer omap3_secure_timer;
+extern struct sys_timer omap4_timer;
 extern bool omap_32k_timer_init(void);
 extern int __init omap_init_clocksource_32k(void);
 extern unsigned long long notrace omap_32k_sched_clock(void);
diff --git a/arch/arm/plat-omap/include/plat/dmtimer.h b/arch/arm/plat-omap/include/plat/dmtimer.h
index d6c70d2..330bd17 100644
--- a/arch/arm/plat-omap/include/plat/dmtimer.h
+++ b/arch/arm/plat-omap/include/plat/dmtimer.h
@@ -57,7 +57,6 @@
 #define OMAP_TIMER_IP_VERSION_1                        0x1
 struct omap_dm_timer;
 extern struct omap_dm_timer *gptimer_wakeup;
-extern struct sys_timer omap_timer;
 struct clk;
 
 int omap_dm_timer_init(void);
-- 
1.6.6.1

