From 12cd5e0b1bb1d3a77fcceef0570134495c959e33 Mon Sep 17 00:00:00 2001
From: Paul Walmsley <paul@pwsan.com>
Date: Sat, 9 Jul 2011 19:14:07 -0600
Subject: [PATCH 040/149] omap_hwmod: share identical omap_hwmod_mpu_irqs arrays

To reduce kernel source file data duplication, share struct
omap_hwmod_mpu_irqs arrays across OMAP2xxx and 3xxx hwmod data files.

Signed-off-by: Paul Walmsley <paul@pwsan.com>
---
 arch/arm/mach-omap2/Makefile                       |   11 +-
 arch/arm/mach-omap2/omap_hwmod_2420_data.c         |  167 +++-----------------
 arch/arm/mach-omap2/omap_hwmod_2430_data.c         |  166 +++-----------------
 .../mach-omap2/omap_hwmod_2xxx_3xxx_ipblock_data.c |  142 +++++++++++++++++
 arch/arm/mach-omap2/omap_hwmod_2xxx_ipblock_data.c |   21 +++
 arch/arm/mach-omap2/omap_hwmod_3xxx_data.c         |  162 +++----------------
 arch/arm/mach-omap2/omap_hwmod_common_data.h       |   29 ++++
 7 files changed, 275 insertions(+), 423 deletions(-)
 create mode 100644 arch/arm/mach-omap2/omap_hwmod_2xxx_3xxx_ipblock_data.c
 create mode 100644 arch/arm/mach-omap2/omap_hwmod_2xxx_ipblock_data.c

diff --git a/arch/arm/mach-omap2/Makefile b/arch/arm/mach-omap2/Makefile
index 8a75d17..f343365 100644
--- a/arch/arm/mach-omap2/Makefile
+++ b/arch/arm/mach-omap2/Makefile
@@ -145,13 +145,18 @@ obj-$(CONFIG_SOC_OMAP2420)		+= opp2420_data.o
 obj-$(CONFIG_SOC_OMAP2430)		+= opp2430_data.o
 
 # hwmod data
-obj-$(CONFIG_SOC_OMAP2420)		+= omap_hwmod_2xxx_interconnect_data.o \
+obj-$(CONFIG_SOC_OMAP2420)		+= omap_hwmod_2xxx_ipblock_data.o \
+					   omap_hwmod_2xxx_3xxx_ipblock_data.o \
+					   omap_hwmod_2xxx_interconnect_data.o \
 					   omap_hwmod_2xxx_3xxx_interconnect_data.o \
 					   omap_hwmod_2420_data.o
-obj-$(CONFIG_SOC_OMAP2430)		+= omap_hwmod_2xxx_interconnect_data.o \
+obj-$(CONFIG_SOC_OMAP2430)		+= omap_hwmod_2xxx_ipblock_data.o \
+					   omap_hwmod_2xxx_3xxx_ipblock_data.o \
+					   omap_hwmod_2xxx_interconnect_data.o \
 					   omap_hwmod_2xxx_3xxx_interconnect_data.o \
 					   omap_hwmod_2430_data.o
-obj-$(CONFIG_ARCH_OMAP3)		+= omap_hwmod_2xxx_3xxx_interconnect_data.o \
+obj-$(CONFIG_ARCH_OMAP3)		+= omap_hwmod_2xxx_3xxx_ipblock_data.o \
+					   omap_hwmod_2xxx_3xxx_interconnect_data.o \
 					   omap_hwmod_3xxx_data.o
 obj-$(CONFIG_ARCH_OMAP4)		+= omap_hwmod_44xx_data.o
 
diff --git a/arch/arm/mach-omap2/omap_hwmod_2420_data.c b/arch/arm/mach-omap2/omap_hwmod_2420_data.c
index 04730d3..73157ee 100644
--- a/arch/arm/mach-omap2/omap_hwmod_2420_data.c
+++ b/arch/arm/mach-omap2/omap_hwmod_2420_data.c
@@ -294,10 +294,6 @@ static struct omap_hwmod_class omap2420_timer_hwmod_class = {
 
 /* timer1 */
 static struct omap_hwmod omap2420_timer1_hwmod;
-static struct omap_hwmod_irq_info omap2420_timer1_mpu_irqs[] = {
-	{ .irq = 37, },
-	{ .irq = -1 }
-};
 
 static struct omap_hwmod_addr_space omap2420_timer1_addrs[] = {
 	{
@@ -325,7 +321,7 @@ static struct omap_hwmod_ocp_if *omap2420_timer1_slaves[] = {
 /* timer1 hwmod */
 static struct omap_hwmod omap2420_timer1_hwmod = {
 	.name		= "timer1",
-	.mpu_irqs	= omap2420_timer1_mpu_irqs,
+	.mpu_irqs	= omap2_timer1_mpu_irqs,
 	.main_clk	= "gpt1_fck",
 	.prcm		= {
 		.omap2 = {
@@ -344,11 +340,6 @@ static struct omap_hwmod omap2420_timer1_hwmod = {
 
 /* timer2 */
 static struct omap_hwmod omap2420_timer2_hwmod;
-static struct omap_hwmod_irq_info omap2420_timer2_mpu_irqs[] = {
-	{ .irq = 38, },
-	{ .irq = -1 }
-};
-
 
 /* l4_core -> timer2 */
 static struct omap_hwmod_ocp_if omap2420_l4_core__timer2 = {
@@ -367,7 +358,7 @@ static struct omap_hwmod_ocp_if *omap2420_timer2_slaves[] = {
 /* timer2 hwmod */
 static struct omap_hwmod omap2420_timer2_hwmod = {
 	.name		= "timer2",
-	.mpu_irqs	= omap2420_timer2_mpu_irqs,
+	.mpu_irqs	= omap2_timer2_mpu_irqs,
 	.main_clk	= "gpt2_fck",
 	.prcm		= {
 		.omap2 = {
@@ -386,10 +377,6 @@ static struct omap_hwmod omap2420_timer2_hwmod = {
 
 /* timer3 */
 static struct omap_hwmod omap2420_timer3_hwmod;
-static struct omap_hwmod_irq_info omap2420_timer3_mpu_irqs[] = {
-	{ .irq = 39, },
-	{ .irq = -1 }
-};
 
 /* l4_core -> timer3 */
 static struct omap_hwmod_ocp_if omap2420_l4_core__timer3 = {
@@ -408,7 +395,7 @@ static struct omap_hwmod_ocp_if *omap2420_timer3_slaves[] = {
 /* timer3 hwmod */
 static struct omap_hwmod omap2420_timer3_hwmod = {
 	.name		= "timer3",
-	.mpu_irqs	= omap2420_timer3_mpu_irqs,
+	.mpu_irqs	= omap2_timer3_mpu_irqs,
 	.main_clk	= "gpt3_fck",
 	.prcm		= {
 		.omap2 = {
@@ -427,10 +414,6 @@ static struct omap_hwmod omap2420_timer3_hwmod = {
 
 /* timer4 */
 static struct omap_hwmod omap2420_timer4_hwmod;
-static struct omap_hwmod_irq_info omap2420_timer4_mpu_irqs[] = {
-	{ .irq = 40, },
-	{ .irq = -1 }
-};
 
 /* l4_core -> timer4 */
 static struct omap_hwmod_ocp_if omap2420_l4_core__timer4 = {
@@ -449,7 +432,7 @@ static struct omap_hwmod_ocp_if *omap2420_timer4_slaves[] = {
 /* timer4 hwmod */
 static struct omap_hwmod omap2420_timer4_hwmod = {
 	.name		= "timer4",
-	.mpu_irqs	= omap2420_timer4_mpu_irqs,
+	.mpu_irqs	= omap2_timer4_mpu_irqs,
 	.main_clk	= "gpt4_fck",
 	.prcm		= {
 		.omap2 = {
@@ -468,10 +451,6 @@ static struct omap_hwmod omap2420_timer4_hwmod = {
 
 /* timer5 */
 static struct omap_hwmod omap2420_timer5_hwmod;
-static struct omap_hwmod_irq_info omap2420_timer5_mpu_irqs[] = {
-	{ .irq = 41, },
-	{ .irq = -1 }
-};
 
 /* l4_core -> timer5 */
 static struct omap_hwmod_ocp_if omap2420_l4_core__timer5 = {
@@ -490,7 +469,7 @@ static struct omap_hwmod_ocp_if *omap2420_timer5_slaves[] = {
 /* timer5 hwmod */
 static struct omap_hwmod omap2420_timer5_hwmod = {
 	.name		= "timer5",
-	.mpu_irqs	= omap2420_timer5_mpu_irqs,
+	.mpu_irqs	= omap2_timer5_mpu_irqs,
 	.main_clk	= "gpt5_fck",
 	.prcm		= {
 		.omap2 = {
@@ -510,10 +489,6 @@ static struct omap_hwmod omap2420_timer5_hwmod = {
 
 /* timer6 */
 static struct omap_hwmod omap2420_timer6_hwmod;
-static struct omap_hwmod_irq_info omap2420_timer6_mpu_irqs[] = {
-	{ .irq = 42, },
-	{ .irq = -1 }
-};
 
 /* l4_core -> timer6 */
 static struct omap_hwmod_ocp_if omap2420_l4_core__timer6 = {
@@ -532,7 +507,7 @@ static struct omap_hwmod_ocp_if *omap2420_timer6_slaves[] = {
 /* timer6 hwmod */
 static struct omap_hwmod omap2420_timer6_hwmod = {
 	.name		= "timer6",
-	.mpu_irqs	= omap2420_timer6_mpu_irqs,
+	.mpu_irqs	= omap2_timer6_mpu_irqs,
 	.main_clk	= "gpt6_fck",
 	.prcm		= {
 		.omap2 = {
@@ -551,10 +526,6 @@ static struct omap_hwmod omap2420_timer6_hwmod = {
 
 /* timer7 */
 static struct omap_hwmod omap2420_timer7_hwmod;
-static struct omap_hwmod_irq_info omap2420_timer7_mpu_irqs[] = {
-	{ .irq = 43, },
-	{ .irq = -1 }
-};
 
 /* l4_core -> timer7 */
 static struct omap_hwmod_ocp_if omap2420_l4_core__timer7 = {
@@ -573,7 +544,7 @@ static struct omap_hwmod_ocp_if *omap2420_timer7_slaves[] = {
 /* timer7 hwmod */
 static struct omap_hwmod omap2420_timer7_hwmod = {
 	.name		= "timer7",
-	.mpu_irqs	= omap2420_timer7_mpu_irqs,
+	.mpu_irqs	= omap2_timer7_mpu_irqs,
 	.main_clk	= "gpt7_fck",
 	.prcm		= {
 		.omap2 = {
@@ -592,10 +563,6 @@ static struct omap_hwmod omap2420_timer7_hwmod = {
 
 /* timer8 */
 static struct omap_hwmod omap2420_timer8_hwmod;
-static struct omap_hwmod_irq_info omap2420_timer8_mpu_irqs[] = {
-	{ .irq = 44, },
-	{ .irq = -1 }
-};
 
 /* l4_core -> timer8 */
 static struct omap_hwmod_ocp_if omap2420_l4_core__timer8 = {
@@ -614,7 +581,7 @@ static struct omap_hwmod_ocp_if *omap2420_timer8_slaves[] = {
 /* timer8 hwmod */
 static struct omap_hwmod omap2420_timer8_hwmod = {
 	.name		= "timer8",
-	.mpu_irqs	= omap2420_timer8_mpu_irqs,
+	.mpu_irqs	= omap2_timer8_mpu_irqs,
 	.main_clk	= "gpt8_fck",
 	.prcm		= {
 		.omap2 = {
@@ -633,10 +600,6 @@ static struct omap_hwmod omap2420_timer8_hwmod = {
 
 /* timer9 */
 static struct omap_hwmod omap2420_timer9_hwmod;
-static struct omap_hwmod_irq_info omap2420_timer9_mpu_irqs[] = {
-	{ .irq = 45, },
-	{ .irq = -1 }
-};
 
 /* l4_core -> timer9 */
 static struct omap_hwmod_ocp_if omap2420_l4_core__timer9 = {
@@ -655,7 +618,7 @@ static struct omap_hwmod_ocp_if *omap2420_timer9_slaves[] = {
 /* timer9 hwmod */
 static struct omap_hwmod omap2420_timer9_hwmod = {
 	.name		= "timer9",
-	.mpu_irqs	= omap2420_timer9_mpu_irqs,
+	.mpu_irqs	= omap2_timer9_mpu_irqs,
 	.main_clk	= "gpt9_fck",
 	.prcm		= {
 		.omap2 = {
@@ -674,10 +637,6 @@ static struct omap_hwmod omap2420_timer9_hwmod = {
 
 /* timer10 */
 static struct omap_hwmod omap2420_timer10_hwmod;
-static struct omap_hwmod_irq_info omap2420_timer10_mpu_irqs[] = {
-	{ .irq = 46, },
-	{ .irq = -1 }
-};
 
 /* l4_core -> timer10 */
 static struct omap_hwmod_ocp_if omap2420_l4_core__timer10 = {
@@ -696,7 +655,7 @@ static struct omap_hwmod_ocp_if *omap2420_timer10_slaves[] = {
 /* timer10 hwmod */
 static struct omap_hwmod omap2420_timer10_hwmod = {
 	.name		= "timer10",
-	.mpu_irqs	= omap2420_timer10_mpu_irqs,
+	.mpu_irqs	= omap2_timer10_mpu_irqs,
 	.main_clk	= "gpt10_fck",
 	.prcm		= {
 		.omap2 = {
@@ -715,10 +674,6 @@ static struct omap_hwmod omap2420_timer10_hwmod = {
 
 /* timer11 */
 static struct omap_hwmod omap2420_timer11_hwmod;
-static struct omap_hwmod_irq_info omap2420_timer11_mpu_irqs[] = {
-	{ .irq = 47, },
-	{ .irq = -1 }
-};
 
 /* l4_core -> timer11 */
 static struct omap_hwmod_ocp_if omap2420_l4_core__timer11 = {
@@ -737,7 +692,7 @@ static struct omap_hwmod_ocp_if *omap2420_timer11_slaves[] = {
 /* timer11 hwmod */
 static struct omap_hwmod omap2420_timer11_hwmod = {
 	.name		= "timer11",
-	.mpu_irqs	= omap2420_timer11_mpu_irqs,
+	.mpu_irqs	= omap2_timer11_mpu_irqs,
 	.main_clk	= "gpt11_fck",
 	.prcm		= {
 		.omap2 = {
@@ -756,10 +711,6 @@ static struct omap_hwmod omap2420_timer11_hwmod = {
 
 /* timer12 */
 static struct omap_hwmod omap2420_timer12_hwmod;
-static struct omap_hwmod_irq_info omap2420_timer12_mpu_irqs[] = {
-	{ .irq = 48, },
-	{ .irq = -1 }
-};
 
 /* l4_core -> timer12 */
 static struct omap_hwmod_ocp_if omap2420_l4_core__timer12 = {
@@ -778,7 +729,7 @@ static struct omap_hwmod_ocp_if *omap2420_timer12_slaves[] = {
 /* timer12 hwmod */
 static struct omap_hwmod omap2420_timer12_hwmod = {
 	.name		= "timer12",
-	.mpu_irqs	= omap2420_timer12_mpu_irqs,
+	.mpu_irqs	= omap2xxx_timer12_mpu_irqs,
 	.main_clk	= "gpt12_fck",
 	.prcm		= {
 		.omap2 = {
@@ -877,11 +828,6 @@ static struct omap_hwmod_class uart_class = {
 
 /* UART1 */
 
-static struct omap_hwmod_irq_info uart1_mpu_irqs[] = {
-	{ .irq = INT_24XX_UART1_IRQ, },
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_dma_info uart1_sdma_reqs[] = {
 	{ .name = "rx",	.dma_req = OMAP24XX_DMA_UART1_RX, },
 	{ .name = "tx",	.dma_req = OMAP24XX_DMA_UART1_TX, },
@@ -893,7 +839,7 @@ static struct omap_hwmod_ocp_if *omap2420_uart1_slaves[] = {
 
 static struct omap_hwmod omap2420_uart1_hwmod = {
 	.name		= "uart1",
-	.mpu_irqs	= uart1_mpu_irqs,
+	.mpu_irqs	= omap2_uart1_mpu_irqs,
 	.sdma_reqs	= uart1_sdma_reqs,
 	.sdma_reqs_cnt	= ARRAY_SIZE(uart1_sdma_reqs),
 	.main_clk	= "uart1_fck",
@@ -914,11 +860,6 @@ static struct omap_hwmod omap2420_uart1_hwmod = {
 
 /* UART2 */
 
-static struct omap_hwmod_irq_info uart2_mpu_irqs[] = {
-	{ .irq = INT_24XX_UART2_IRQ, },
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_dma_info uart2_sdma_reqs[] = {
 	{ .name = "rx",	.dma_req = OMAP24XX_DMA_UART2_RX, },
 	{ .name = "tx",	.dma_req = OMAP24XX_DMA_UART2_TX, },
@@ -930,7 +871,7 @@ static struct omap_hwmod_ocp_if *omap2420_uart2_slaves[] = {
 
 static struct omap_hwmod omap2420_uart2_hwmod = {
 	.name		= "uart2",
-	.mpu_irqs	= uart2_mpu_irqs,
+	.mpu_irqs	= omap2_uart2_mpu_irqs,
 	.sdma_reqs	= uart2_sdma_reqs,
 	.sdma_reqs_cnt	= ARRAY_SIZE(uart2_sdma_reqs),
 	.main_clk	= "uart2_fck",
@@ -951,11 +892,6 @@ static struct omap_hwmod omap2420_uart2_hwmod = {
 
 /* UART3 */
 
-static struct omap_hwmod_irq_info uart3_mpu_irqs[] = {
-	{ .irq = INT_24XX_UART3_IRQ, },
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_dma_info uart3_sdma_reqs[] = {
 	{ .name = "rx",	.dma_req = OMAP24XX_DMA_UART3_RX, },
 	{ .name = "tx",	.dma_req = OMAP24XX_DMA_UART3_TX, },
@@ -967,7 +903,7 @@ static struct omap_hwmod_ocp_if *omap2420_uart3_slaves[] = {
 
 static struct omap_hwmod omap2420_uart3_hwmod = {
 	.name		= "uart3",
-	.mpu_irqs	= uart3_mpu_irqs,
+	.mpu_irqs	= omap2_uart3_mpu_irqs,
 	.sdma_reqs	= uart3_sdma_reqs,
 	.sdma_reqs_cnt	= ARRAY_SIZE(uart3_sdma_reqs),
 	.main_clk	= "uart3_fck",
@@ -1085,11 +1021,6 @@ static struct omap_hwmod_class omap2420_dispc_hwmod_class = {
 	.sysc = &omap2420_dispc_sysc,
 };
 
-static struct omap_hwmod_irq_info omap2420_dispc_irqs[] = {
-	{ .irq = 25 },
-	{ .irq = -1 }
-};
-
 /* l4_core -> dss_dispc */
 static struct omap_hwmod_ocp_if omap2420_l4_core__dss_dispc = {
 	.master		= &omap2420_l4_core_hwmod,
@@ -1113,7 +1044,7 @@ static struct omap_hwmod_ocp_if *omap2420_dss_dispc_slaves[] = {
 static struct omap_hwmod omap2420_dss_dispc_hwmod = {
 	.name		= "dss_dispc",
 	.class		= &omap2420_dispc_hwmod_class,
-	.mpu_irqs	= omap2420_dispc_irqs,
+	.mpu_irqs	= omap2_dispc_irqs,
 	.main_clk	= "dss1_fck",
 	.prcm		= {
 		.omap2 = {
@@ -1252,11 +1183,6 @@ static struct omap_i2c_dev_attr i2c_dev_attr;
 
 /* I2C1 */
 
-static struct omap_hwmod_irq_info i2c1_mpu_irqs[] = {
-	{ .irq = INT_24XX_I2C1_IRQ, },
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_dma_info i2c1_sdma_reqs[] = {
 	{ .name = "tx", .dma_req = OMAP24XX_DMA_I2C1_TX },
 	{ .name = "rx", .dma_req = OMAP24XX_DMA_I2C1_RX },
@@ -1268,7 +1194,7 @@ static struct omap_hwmod_ocp_if *omap2420_i2c1_slaves[] = {
 
 static struct omap_hwmod omap2420_i2c1_hwmod = {
 	.name		= "i2c1",
-	.mpu_irqs	= i2c1_mpu_irqs,
+	.mpu_irqs	= omap2_i2c1_mpu_irqs,
 	.sdma_reqs	= i2c1_sdma_reqs,
 	.sdma_reqs_cnt	= ARRAY_SIZE(i2c1_sdma_reqs),
 	.main_clk	= "i2c1_fck",
@@ -1291,11 +1217,6 @@ static struct omap_hwmod omap2420_i2c1_hwmod = {
 
 /* I2C2 */
 
-static struct omap_hwmod_irq_info i2c2_mpu_irqs[] = {
-	{ .irq = INT_24XX_I2C2_IRQ, },
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_dma_info i2c2_sdma_reqs[] = {
 	{ .name = "tx", .dma_req = OMAP24XX_DMA_I2C2_TX },
 	{ .name = "rx", .dma_req = OMAP24XX_DMA_I2C2_RX },
@@ -1307,7 +1228,7 @@ static struct omap_hwmod_ocp_if *omap2420_i2c2_slaves[] = {
 
 static struct omap_hwmod omap2420_i2c2_hwmod = {
 	.name		= "i2c2",
-	.mpu_irqs	= i2c2_mpu_irqs,
+	.mpu_irqs	= omap2_i2c2_mpu_irqs,
 	.sdma_reqs	= i2c2_sdma_reqs,
 	.sdma_reqs_cnt	= ARRAY_SIZE(i2c2_sdma_reqs),
 	.main_clk	= "i2c2_fck",
@@ -1428,11 +1349,6 @@ static struct omap_hwmod_class omap242x_gpio_hwmod_class = {
 };
 
 /* gpio1 */
-static struct omap_hwmod_irq_info omap242x_gpio1_irqs[] = {
-	{ .irq = 29 }, /* INT_24XX_GPIO_BANK1 */
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_ocp_if *omap2420_gpio1_slaves[] = {
 	&omap2420_l4_wkup__gpio1,
 };
@@ -1440,7 +1356,7 @@ static struct omap_hwmod_ocp_if *omap2420_gpio1_slaves[] = {
 static struct omap_hwmod omap2420_gpio1_hwmod = {
 	.name		= "gpio1",
 	.flags		= HWMOD_CONTROL_OPT_CLKS_IN_RESET,
-	.mpu_irqs	= omap242x_gpio1_irqs,
+	.mpu_irqs	= omap2_gpio1_irqs,
 	.main_clk	= "gpios_fck",
 	.prcm		= {
 		.omap2 = {
@@ -1459,11 +1375,6 @@ static struct omap_hwmod omap2420_gpio1_hwmod = {
 };
 
 /* gpio2 */
-static struct omap_hwmod_irq_info omap242x_gpio2_irqs[] = {
-	{ .irq = 30 }, /* INT_24XX_GPIO_BANK2 */
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_ocp_if *omap2420_gpio2_slaves[] = {
 	&omap2420_l4_wkup__gpio2,
 };
@@ -1471,7 +1382,7 @@ static struct omap_hwmod_ocp_if *omap2420_gpio2_slaves[] = {
 static struct omap_hwmod omap2420_gpio2_hwmod = {
 	.name		= "gpio2",
 	.flags		= HWMOD_CONTROL_OPT_CLKS_IN_RESET,
-	.mpu_irqs	= omap242x_gpio2_irqs,
+	.mpu_irqs	= omap2_gpio2_irqs,
 	.main_clk	= "gpios_fck",
 	.prcm		= {
 		.omap2 = {
@@ -1490,11 +1401,6 @@ static struct omap_hwmod omap2420_gpio2_hwmod = {
 };
 
 /* gpio3 */
-static struct omap_hwmod_irq_info omap242x_gpio3_irqs[] = {
-	{ .irq = 31 }, /* INT_24XX_GPIO_BANK3 */
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_ocp_if *omap2420_gpio3_slaves[] = {
 	&omap2420_l4_wkup__gpio3,
 };
@@ -1502,7 +1408,7 @@ static struct omap_hwmod_ocp_if *omap2420_gpio3_slaves[] = {
 static struct omap_hwmod omap2420_gpio3_hwmod = {
 	.name		= "gpio3",
 	.flags		= HWMOD_CONTROL_OPT_CLKS_IN_RESET,
-	.mpu_irqs	= omap242x_gpio3_irqs,
+	.mpu_irqs	= omap2_gpio3_irqs,
 	.main_clk	= "gpios_fck",
 	.prcm		= {
 		.omap2 = {
@@ -1521,11 +1427,6 @@ static struct omap_hwmod omap2420_gpio3_hwmod = {
 };
 
 /* gpio4 */
-static struct omap_hwmod_irq_info omap242x_gpio4_irqs[] = {
-	{ .irq = 32 }, /* INT_24XX_GPIO_BANK4 */
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_ocp_if *omap2420_gpio4_slaves[] = {
 	&omap2420_l4_wkup__gpio4,
 };
@@ -1533,7 +1434,7 @@ static struct omap_hwmod_ocp_if *omap2420_gpio4_slaves[] = {
 static struct omap_hwmod omap2420_gpio4_hwmod = {
 	.name		= "gpio4",
 	.flags		= HWMOD_CONTROL_OPT_CLKS_IN_RESET,
-	.mpu_irqs	= omap242x_gpio4_irqs,
+	.mpu_irqs	= omap2_gpio4_irqs,
 	.main_clk	= "gpios_fck",
 	.prcm		= {
 		.omap2 = {
@@ -1575,14 +1476,6 @@ static struct omap_dma_dev_attr dma_dev_attr = {
 	.lch_count = 32,
 };
 
-static struct omap_hwmod_irq_info omap2420_dma_system_irqs[] = {
-	{ .name = "0", .irq = 12 }, /* INT_24XX_SDMA_IRQ0 */
-	{ .name = "1", .irq = 13 }, /* INT_24XX_SDMA_IRQ1 */
-	{ .name = "2", .irq = 14 }, /* INT_24XX_SDMA_IRQ2 */
-	{ .name = "3", .irq = 15 }, /* INT_24XX_SDMA_IRQ3 */
-	{ .irq = -1 }
-};
-
 /* dma_system -> L3 */
 static struct omap_hwmod_ocp_if omap2420_dma_system__l3 = {
 	.master		= &omap2420_dma_system_hwmod,
@@ -1613,7 +1506,7 @@ static struct omap_hwmod_ocp_if *omap2420_dma_system_slaves[] = {
 static struct omap_hwmod omap2420_dma_system_hwmod = {
 	.name		= "dma",
 	.class		= &omap2420_dma_hwmod_class,
-	.mpu_irqs	= omap2420_dma_system_irqs,
+	.mpu_irqs	= omap2_dma_system_irqs,
 	.main_clk	= "core_l3_ck",
 	.slaves		= omap2420_dma_system_slaves,
 	.slaves_cnt	= ARRAY_SIZE(omap2420_dma_system_slaves),
@@ -1709,11 +1602,6 @@ static struct omap_hwmod_class omap2420_mcspi_class = {
 };
 
 /* mcspi1 */
-static struct omap_hwmod_irq_info omap2420_mcspi1_mpu_irqs[] = {
-	{ .irq = 65 },
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_dma_info omap2420_mcspi1_sdma_reqs[] = {
 	{ .name = "tx0", .dma_req = 35 }, /* DMA_SPI1_TX0 */
 	{ .name = "rx0", .dma_req = 36 }, /* DMA_SPI1_RX0 */
@@ -1735,7 +1623,7 @@ static struct omap2_mcspi_dev_attr omap_mcspi1_dev_attr = {
 
 static struct omap_hwmod omap2420_mcspi1_hwmod = {
 	.name		= "mcspi1_hwmod",
-	.mpu_irqs	= omap2420_mcspi1_mpu_irqs,
+	.mpu_irqs	= omap2_mcspi1_mpu_irqs,
 	.sdma_reqs	= omap2420_mcspi1_sdma_reqs,
 	.sdma_reqs_cnt	= ARRAY_SIZE(omap2420_mcspi1_sdma_reqs),
 	.main_clk	= "mcspi1_fck",
@@ -1756,11 +1644,6 @@ static struct omap_hwmod omap2420_mcspi1_hwmod = {
 };
 
 /* mcspi2 */
-static struct omap_hwmod_irq_info omap2420_mcspi2_mpu_irqs[] = {
-	{ .irq = 66 },
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_dma_info omap2420_mcspi2_sdma_reqs[] = {
 	{ .name = "tx0", .dma_req = 43 }, /* DMA_SPI2_TX0 */
 	{ .name = "rx0", .dma_req = 44 }, /* DMA_SPI2_RX0 */
@@ -1778,7 +1661,7 @@ static struct omap2_mcspi_dev_attr omap_mcspi2_dev_attr = {
 
 static struct omap_hwmod omap2420_mcspi2_hwmod = {
 	.name		= "mcspi2_hwmod",
-	.mpu_irqs	= omap2420_mcspi2_mpu_irqs,
+	.mpu_irqs	= omap2_mcspi2_mpu_irqs,
 	.sdma_reqs	= omap2420_mcspi2_sdma_reqs,
 	.sdma_reqs_cnt	= ARRAY_SIZE(omap2420_mcspi2_sdma_reqs),
 	.main_clk	= "mcspi2_fck",
diff --git a/arch/arm/mach-omap2/omap_hwmod_2430_data.c b/arch/arm/mach-omap2/omap_hwmod_2430_data.c
index 2c28468..62ecc68 100644
--- a/arch/arm/mach-omap2/omap_hwmod_2430_data.c
+++ b/arch/arm/mach-omap2/omap_hwmod_2430_data.c
@@ -367,10 +367,6 @@ static struct omap_hwmod_class omap2430_timer_hwmod_class = {
 
 /* timer1 */
 static struct omap_hwmod omap2430_timer1_hwmod;
-static struct omap_hwmod_irq_info omap2430_timer1_mpu_irqs[] = {
-	{ .irq = 37, },
-	{ .irq = -1 }
-};
 
 static struct omap_hwmod_addr_space omap2430_timer1_addrs[] = {
 	{
@@ -398,7 +394,7 @@ static struct omap_hwmod_ocp_if *omap2430_timer1_slaves[] = {
 /* timer1 hwmod */
 static struct omap_hwmod omap2430_timer1_hwmod = {
 	.name		= "timer1",
-	.mpu_irqs	= omap2430_timer1_mpu_irqs,
+	.mpu_irqs	= omap2_timer1_mpu_irqs,
 	.main_clk	= "gpt1_fck",
 	.prcm		= {
 		.omap2 = {
@@ -417,10 +413,6 @@ static struct omap_hwmod omap2430_timer1_hwmod = {
 
 /* timer2 */
 static struct omap_hwmod omap2430_timer2_hwmod;
-static struct omap_hwmod_irq_info omap2430_timer2_mpu_irqs[] = {
-	{ .irq = 38, },
-	{ .irq = -1 }
-};
 
 /* l4_core -> timer2 */
 static struct omap_hwmod_ocp_if omap2430_l4_core__timer2 = {
@@ -439,7 +431,7 @@ static struct omap_hwmod_ocp_if *omap2430_timer2_slaves[] = {
 /* timer2 hwmod */
 static struct omap_hwmod omap2430_timer2_hwmod = {
 	.name		= "timer2",
-	.mpu_irqs	= omap2430_timer2_mpu_irqs,
+	.mpu_irqs	= omap2_timer2_mpu_irqs,
 	.main_clk	= "gpt2_fck",
 	.prcm		= {
 		.omap2 = {
@@ -458,10 +450,6 @@ static struct omap_hwmod omap2430_timer2_hwmod = {
 
 /* timer3 */
 static struct omap_hwmod omap2430_timer3_hwmod;
-static struct omap_hwmod_irq_info omap2430_timer3_mpu_irqs[] = {
-	{ .irq = 39, },
-	{ .irq = -1 }
-};
 
 /* l4_core -> timer3 */
 static struct omap_hwmod_ocp_if omap2430_l4_core__timer3 = {
@@ -480,7 +468,7 @@ static struct omap_hwmod_ocp_if *omap2430_timer3_slaves[] = {
 /* timer3 hwmod */
 static struct omap_hwmod omap2430_timer3_hwmod = {
 	.name		= "timer3",
-	.mpu_irqs	= omap2430_timer3_mpu_irqs,
+	.mpu_irqs	= omap2_timer3_mpu_irqs,
 	.main_clk	= "gpt3_fck",
 	.prcm		= {
 		.omap2 = {
@@ -499,10 +487,6 @@ static struct omap_hwmod omap2430_timer3_hwmod = {
 
 /* timer4 */
 static struct omap_hwmod omap2430_timer4_hwmod;
-static struct omap_hwmod_irq_info omap2430_timer4_mpu_irqs[] = {
-	{ .irq = 40, },
-	{ .irq = -1 }
-};
 
 /* l4_core -> timer4 */
 static struct omap_hwmod_ocp_if omap2430_l4_core__timer4 = {
@@ -521,7 +505,7 @@ static struct omap_hwmod_ocp_if *omap2430_timer4_slaves[] = {
 /* timer4 hwmod */
 static struct omap_hwmod omap2430_timer4_hwmod = {
 	.name		= "timer4",
-	.mpu_irqs	= omap2430_timer4_mpu_irqs,
+	.mpu_irqs	= omap2_timer4_mpu_irqs,
 	.main_clk	= "gpt4_fck",
 	.prcm		= {
 		.omap2 = {
@@ -540,10 +524,6 @@ static struct omap_hwmod omap2430_timer4_hwmod = {
 
 /* timer5 */
 static struct omap_hwmod omap2430_timer5_hwmod;
-static struct omap_hwmod_irq_info omap2430_timer5_mpu_irqs[] = {
-	{ .irq = 41, },
-	{ .irq = -1 }
-};
 
 /* l4_core -> timer5 */
 static struct omap_hwmod_ocp_if omap2430_l4_core__timer5 = {
@@ -562,7 +542,7 @@ static struct omap_hwmod_ocp_if *omap2430_timer5_slaves[] = {
 /* timer5 hwmod */
 static struct omap_hwmod omap2430_timer5_hwmod = {
 	.name		= "timer5",
-	.mpu_irqs	= omap2430_timer5_mpu_irqs,
+	.mpu_irqs	= omap2_timer5_mpu_irqs,
 	.main_clk	= "gpt5_fck",
 	.prcm		= {
 		.omap2 = {
@@ -581,10 +561,6 @@ static struct omap_hwmod omap2430_timer5_hwmod = {
 
 /* timer6 */
 static struct omap_hwmod omap2430_timer6_hwmod;
-static struct omap_hwmod_irq_info omap2430_timer6_mpu_irqs[] = {
-	{ .irq = 42, },
-	{ .irq = -1 }
-};
 
 /* l4_core -> timer6 */
 static struct omap_hwmod_ocp_if omap2430_l4_core__timer6 = {
@@ -603,7 +579,7 @@ static struct omap_hwmod_ocp_if *omap2430_timer6_slaves[] = {
 /* timer6 hwmod */
 static struct omap_hwmod omap2430_timer6_hwmod = {
 	.name		= "timer6",
-	.mpu_irqs	= omap2430_timer6_mpu_irqs,
+	.mpu_irqs	= omap2_timer6_mpu_irqs,
 	.main_clk	= "gpt6_fck",
 	.prcm		= {
 		.omap2 = {
@@ -622,10 +598,6 @@ static struct omap_hwmod omap2430_timer6_hwmod = {
 
 /* timer7 */
 static struct omap_hwmod omap2430_timer7_hwmod;
-static struct omap_hwmod_irq_info omap2430_timer7_mpu_irqs[] = {
-	{ .irq = 43, },
-	{ .irq = -1 }
-};
 
 /* l4_core -> timer7 */
 static struct omap_hwmod_ocp_if omap2430_l4_core__timer7 = {
@@ -644,7 +616,7 @@ static struct omap_hwmod_ocp_if *omap2430_timer7_slaves[] = {
 /* timer7 hwmod */
 static struct omap_hwmod omap2430_timer7_hwmod = {
 	.name		= "timer7",
-	.mpu_irqs	= omap2430_timer7_mpu_irqs,
+	.mpu_irqs	= omap2_timer7_mpu_irqs,
 	.main_clk	= "gpt7_fck",
 	.prcm		= {
 		.omap2 = {
@@ -663,10 +635,6 @@ static struct omap_hwmod omap2430_timer7_hwmod = {
 
 /* timer8 */
 static struct omap_hwmod omap2430_timer8_hwmod;
-static struct omap_hwmod_irq_info omap2430_timer8_mpu_irqs[] = {
-	{ .irq = 44, },
-	{ .irq = -1 }
-};
 
 /* l4_core -> timer8 */
 static struct omap_hwmod_ocp_if omap2430_l4_core__timer8 = {
@@ -685,7 +653,7 @@ static struct omap_hwmod_ocp_if *omap2430_timer8_slaves[] = {
 /* timer8 hwmod */
 static struct omap_hwmod omap2430_timer8_hwmod = {
 	.name		= "timer8",
-	.mpu_irqs	= omap2430_timer8_mpu_irqs,
+	.mpu_irqs	= omap2_timer8_mpu_irqs,
 	.main_clk	= "gpt8_fck",
 	.prcm		= {
 		.omap2 = {
@@ -704,10 +672,6 @@ static struct omap_hwmod omap2430_timer8_hwmod = {
 
 /* timer9 */
 static struct omap_hwmod omap2430_timer9_hwmod;
-static struct omap_hwmod_irq_info omap2430_timer9_mpu_irqs[] = {
-	{ .irq = 45, },
-	{ .irq = -1 }
-};
 
 /* l4_core -> timer9 */
 static struct omap_hwmod_ocp_if omap2430_l4_core__timer9 = {
@@ -726,7 +690,7 @@ static struct omap_hwmod_ocp_if *omap2430_timer9_slaves[] = {
 /* timer9 hwmod */
 static struct omap_hwmod omap2430_timer9_hwmod = {
 	.name		= "timer9",
-	.mpu_irqs	= omap2430_timer9_mpu_irqs,
+	.mpu_irqs	= omap2_timer9_mpu_irqs,
 	.main_clk	= "gpt9_fck",
 	.prcm		= {
 		.omap2 = {
@@ -745,10 +709,6 @@ static struct omap_hwmod omap2430_timer9_hwmod = {
 
 /* timer10 */
 static struct omap_hwmod omap2430_timer10_hwmod;
-static struct omap_hwmod_irq_info omap2430_timer10_mpu_irqs[] = {
-	{ .irq = 46, },
-	{ .irq = -1 }
-};
 
 /* l4_core -> timer10 */
 static struct omap_hwmod_ocp_if omap2430_l4_core__timer10 = {
@@ -767,7 +727,7 @@ static struct omap_hwmod_ocp_if *omap2430_timer10_slaves[] = {
 /* timer10 hwmod */
 static struct omap_hwmod omap2430_timer10_hwmod = {
 	.name		= "timer10",
-	.mpu_irqs	= omap2430_timer10_mpu_irqs,
+	.mpu_irqs	= omap2_timer10_mpu_irqs,
 	.main_clk	= "gpt10_fck",
 	.prcm		= {
 		.omap2 = {
@@ -786,10 +746,6 @@ static struct omap_hwmod omap2430_timer10_hwmod = {
 
 /* timer11 */
 static struct omap_hwmod omap2430_timer11_hwmod;
-static struct omap_hwmod_irq_info omap2430_timer11_mpu_irqs[] = {
-	{ .irq = 47, },
-	{ .irq = -1 }
-};
 
 /* l4_core -> timer11 */
 static struct omap_hwmod_ocp_if omap2430_l4_core__timer11 = {
@@ -808,7 +764,7 @@ static struct omap_hwmod_ocp_if *omap2430_timer11_slaves[] = {
 /* timer11 hwmod */
 static struct omap_hwmod omap2430_timer11_hwmod = {
 	.name		= "timer11",
-	.mpu_irqs	= omap2430_timer11_mpu_irqs,
+	.mpu_irqs	= omap2_timer11_mpu_irqs,
 	.main_clk	= "gpt11_fck",
 	.prcm		= {
 		.omap2 = {
@@ -827,10 +783,6 @@ static struct omap_hwmod omap2430_timer11_hwmod = {
 
 /* timer12 */
 static struct omap_hwmod omap2430_timer12_hwmod;
-static struct omap_hwmod_irq_info omap2430_timer12_mpu_irqs[] = {
-	{ .irq = 48, },
-	{ .irq = -1 }
-};
 
 /* l4_core -> timer12 */
 static struct omap_hwmod_ocp_if omap2430_l4_core__timer12 = {
@@ -849,7 +801,7 @@ static struct omap_hwmod_ocp_if *omap2430_timer12_slaves[] = {
 /* timer12 hwmod */
 static struct omap_hwmod omap2430_timer12_hwmod = {
 	.name		= "timer12",
-	.mpu_irqs	= omap2430_timer12_mpu_irqs,
+	.mpu_irqs	= omap2xxx_timer12_mpu_irqs,
 	.main_clk	= "gpt12_fck",
 	.prcm		= {
 		.omap2 = {
@@ -948,11 +900,6 @@ static struct omap_hwmod_class uart_class = {
 
 /* UART1 */
 
-static struct omap_hwmod_irq_info uart1_mpu_irqs[] = {
-	{ .irq = INT_24XX_UART1_IRQ, },
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_dma_info uart1_sdma_reqs[] = {
 	{ .name = "rx",	.dma_req = OMAP24XX_DMA_UART1_RX, },
 	{ .name = "tx",	.dma_req = OMAP24XX_DMA_UART1_TX, },
@@ -964,7 +911,7 @@ static struct omap_hwmod_ocp_if *omap2430_uart1_slaves[] = {
 
 static struct omap_hwmod omap2430_uart1_hwmod = {
 	.name		= "uart1",
-	.mpu_irqs	= uart1_mpu_irqs,
+	.mpu_irqs	= omap2_uart1_mpu_irqs,
 	.sdma_reqs	= uart1_sdma_reqs,
 	.sdma_reqs_cnt	= ARRAY_SIZE(uart1_sdma_reqs),
 	.main_clk	= "uart1_fck",
@@ -985,11 +932,6 @@ static struct omap_hwmod omap2430_uart1_hwmod = {
 
 /* UART2 */
 
-static struct omap_hwmod_irq_info uart2_mpu_irqs[] = {
-	{ .irq = INT_24XX_UART2_IRQ, },
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_dma_info uart2_sdma_reqs[] = {
 	{ .name = "rx",	.dma_req = OMAP24XX_DMA_UART2_RX, },
 	{ .name = "tx",	.dma_req = OMAP24XX_DMA_UART2_TX, },
@@ -1001,7 +943,7 @@ static struct omap_hwmod_ocp_if *omap2430_uart2_slaves[] = {
 
 static struct omap_hwmod omap2430_uart2_hwmod = {
 	.name		= "uart2",
-	.mpu_irqs	= uart2_mpu_irqs,
+	.mpu_irqs	= omap2_uart2_mpu_irqs,
 	.sdma_reqs	= uart2_sdma_reqs,
 	.sdma_reqs_cnt	= ARRAY_SIZE(uart2_sdma_reqs),
 	.main_clk	= "uart2_fck",
@@ -1022,11 +964,6 @@ static struct omap_hwmod omap2430_uart2_hwmod = {
 
 /* UART3 */
 
-static struct omap_hwmod_irq_info uart3_mpu_irqs[] = {
-	{ .irq = INT_24XX_UART3_IRQ, },
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_dma_info uart3_sdma_reqs[] = {
 	{ .name = "rx",	.dma_req = OMAP24XX_DMA_UART3_RX, },
 	{ .name = "tx",	.dma_req = OMAP24XX_DMA_UART3_TX, },
@@ -1038,7 +975,7 @@ static struct omap_hwmod_ocp_if *omap2430_uart3_slaves[] = {
 
 static struct omap_hwmod omap2430_uart3_hwmod = {
 	.name		= "uart3",
-	.mpu_irqs	= uart3_mpu_irqs,
+	.mpu_irqs	= omap2_uart3_mpu_irqs,
 	.sdma_reqs	= uart3_sdma_reqs,
 	.sdma_reqs_cnt	= ARRAY_SIZE(uart3_sdma_reqs),
 	.main_clk	= "uart3_fck",
@@ -1150,11 +1087,6 @@ static struct omap_hwmod_class omap2430_dispc_hwmod_class = {
 	.sysc = &omap2430_dispc_sysc,
 };
 
-static struct omap_hwmod_irq_info omap2430_dispc_irqs[] = {
-	{ .irq = 25 },
-	{ .irq = -1 }
-};
-
 /* l4_core -> dss_dispc */
 static struct omap_hwmod_ocp_if omap2430_l4_core__dss_dispc = {
 	.master		= &omap2430_l4_core_hwmod,
@@ -1172,7 +1104,7 @@ static struct omap_hwmod_ocp_if *omap2430_dss_dispc_slaves[] = {
 static struct omap_hwmod omap2430_dss_dispc_hwmod = {
 	.name		= "dss_dispc",
 	.class		= &omap2430_dispc_hwmod_class,
-	.mpu_irqs	= omap2430_dispc_irqs,
+	.mpu_irqs	= omap2_dispc_irqs,
 	.main_clk	= "dss1_fck",
 	.prcm		= {
 		.omap2 = {
@@ -1302,11 +1234,6 @@ static struct omap_i2c_dev_attr i2c_dev_attr = {
 
 /* I2C1 */
 
-static struct omap_hwmod_irq_info i2c1_mpu_irqs[] = {
-	{ .irq = INT_24XX_I2C1_IRQ, },
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_dma_info i2c1_sdma_reqs[] = {
 	{ .name = "tx", .dma_req = OMAP24XX_DMA_I2C1_TX },
 	{ .name = "rx", .dma_req = OMAP24XX_DMA_I2C1_RX },
@@ -1318,7 +1245,7 @@ static struct omap_hwmod_ocp_if *omap2430_i2c1_slaves[] = {
 
 static struct omap_hwmod omap2430_i2c1_hwmod = {
 	.name		= "i2c1",
-	.mpu_irqs	= i2c1_mpu_irqs,
+	.mpu_irqs	= omap2_i2c1_mpu_irqs,
 	.sdma_reqs	= i2c1_sdma_reqs,
 	.sdma_reqs_cnt	= ARRAY_SIZE(i2c1_sdma_reqs),
 	.main_clk	= "i2chs1_fck",
@@ -1348,11 +1275,6 @@ static struct omap_hwmod omap2430_i2c1_hwmod = {
 
 /* I2C2 */
 
-static struct omap_hwmod_irq_info i2c2_mpu_irqs[] = {
-	{ .irq = INT_24XX_I2C2_IRQ, },
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_dma_info i2c2_sdma_reqs[] = {
 	{ .name = "tx", .dma_req = OMAP24XX_DMA_I2C2_TX },
 	{ .name = "rx", .dma_req = OMAP24XX_DMA_I2C2_RX },
@@ -1364,7 +1286,7 @@ static struct omap_hwmod_ocp_if *omap2430_i2c2_slaves[] = {
 
 static struct omap_hwmod omap2430_i2c2_hwmod = {
 	.name		= "i2c2",
-	.mpu_irqs	= i2c2_mpu_irqs,
+	.mpu_irqs	= omap2_i2c2_mpu_irqs,
 	.sdma_reqs	= i2c2_sdma_reqs,
 	.sdma_reqs_cnt	= ARRAY_SIZE(i2c2_sdma_reqs),
 	.main_clk	= "i2chs2_fck",
@@ -1502,11 +1424,6 @@ static struct omap_hwmod_class omap243x_gpio_hwmod_class = {
 };
 
 /* gpio1 */
-static struct omap_hwmod_irq_info omap243x_gpio1_irqs[] = {
-	{ .irq = 29 }, /* INT_24XX_GPIO_BANK1 */
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_ocp_if *omap2430_gpio1_slaves[] = {
 	&omap2430_l4_wkup__gpio1,
 };
@@ -1514,7 +1431,7 @@ static struct omap_hwmod_ocp_if *omap2430_gpio1_slaves[] = {
 static struct omap_hwmod omap2430_gpio1_hwmod = {
 	.name		= "gpio1",
 	.flags		= HWMOD_CONTROL_OPT_CLKS_IN_RESET,
-	.mpu_irqs	= omap243x_gpio1_irqs,
+	.mpu_irqs	= omap2_gpio1_irqs,
 	.main_clk	= "gpios_fck",
 	.prcm		= {
 		.omap2 = {
@@ -1533,11 +1450,6 @@ static struct omap_hwmod omap2430_gpio1_hwmod = {
 };
 
 /* gpio2 */
-static struct omap_hwmod_irq_info omap243x_gpio2_irqs[] = {
-	{ .irq = 30 }, /* INT_24XX_GPIO_BANK2 */
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_ocp_if *omap2430_gpio2_slaves[] = {
 	&omap2430_l4_wkup__gpio2,
 };
@@ -1545,7 +1457,7 @@ static struct omap_hwmod_ocp_if *omap2430_gpio2_slaves[] = {
 static struct omap_hwmod omap2430_gpio2_hwmod = {
 	.name		= "gpio2",
 	.flags		= HWMOD_CONTROL_OPT_CLKS_IN_RESET,
-	.mpu_irqs	= omap243x_gpio2_irqs,
+	.mpu_irqs	= omap2_gpio2_irqs,
 	.main_clk	= "gpios_fck",
 	.prcm		= {
 		.omap2 = {
@@ -1564,11 +1476,6 @@ static struct omap_hwmod omap2430_gpio2_hwmod = {
 };
 
 /* gpio3 */
-static struct omap_hwmod_irq_info omap243x_gpio3_irqs[] = {
-	{ .irq = 31 }, /* INT_24XX_GPIO_BANK3 */
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_ocp_if *omap2430_gpio3_slaves[] = {
 	&omap2430_l4_wkup__gpio3,
 };
@@ -1576,7 +1483,7 @@ static struct omap_hwmod_ocp_if *omap2430_gpio3_slaves[] = {
 static struct omap_hwmod omap2430_gpio3_hwmod = {
 	.name		= "gpio3",
 	.flags		= HWMOD_CONTROL_OPT_CLKS_IN_RESET,
-	.mpu_irqs	= omap243x_gpio3_irqs,
+	.mpu_irqs	= omap2_gpio3_irqs,
 	.main_clk	= "gpios_fck",
 	.prcm		= {
 		.omap2 = {
@@ -1595,11 +1502,6 @@ static struct omap_hwmod omap2430_gpio3_hwmod = {
 };
 
 /* gpio4 */
-static struct omap_hwmod_irq_info omap243x_gpio4_irqs[] = {
-	{ .irq = 32 }, /* INT_24XX_GPIO_BANK4 */
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_ocp_if *omap2430_gpio4_slaves[] = {
 	&omap2430_l4_wkup__gpio4,
 };
@@ -1607,7 +1509,7 @@ static struct omap_hwmod_ocp_if *omap2430_gpio4_slaves[] = {
 static struct omap_hwmod omap2430_gpio4_hwmod = {
 	.name		= "gpio4",
 	.flags		= HWMOD_CONTROL_OPT_CLKS_IN_RESET,
-	.mpu_irqs	= omap243x_gpio4_irqs,
+	.mpu_irqs	= omap2_gpio4_irqs,
 	.main_clk	= "gpios_fck",
 	.prcm		= {
 		.omap2 = {
@@ -1680,14 +1582,6 @@ static struct omap_dma_dev_attr dma_dev_attr = {
 	.lch_count = 32,
 };
 
-static struct omap_hwmod_irq_info omap2430_dma_system_irqs[] = {
-	{ .name = "0", .irq = 12 }, /* INT_24XX_SDMA_IRQ0 */
-	{ .name = "1", .irq = 13 }, /* INT_24XX_SDMA_IRQ1 */
-	{ .name = "2", .irq = 14 }, /* INT_24XX_SDMA_IRQ2 */
-	{ .name = "3", .irq = 15 }, /* INT_24XX_SDMA_IRQ3 */
-	{ .irq = -1 }
-};
-
 /* dma_system -> L3 */
 static struct omap_hwmod_ocp_if omap2430_dma_system__l3 = {
 	.master		= &omap2430_dma_system_hwmod,
@@ -1718,7 +1612,7 @@ static struct omap_hwmod_ocp_if *omap2430_dma_system_slaves[] = {
 static struct omap_hwmod omap2430_dma_system_hwmod = {
 	.name		= "dma",
 	.class		= &omap2430_dma_hwmod_class,
-	.mpu_irqs	= omap2430_dma_system_irqs,
+	.mpu_irqs	= omap2_dma_system_irqs,
 	.main_clk	= "core_l3_ck",
 	.slaves		= omap2430_dma_system_slaves,
 	.slaves_cnt	= ARRAY_SIZE(omap2430_dma_system_slaves),
@@ -1813,11 +1707,6 @@ static struct omap_hwmod_class omap2430_mcspi_class = {
 };
 
 /* mcspi1 */
-static struct omap_hwmod_irq_info omap2430_mcspi1_mpu_irqs[] = {
-	{ .irq = 65 },
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_dma_info omap2430_mcspi1_sdma_reqs[] = {
 	{ .name = "tx0", .dma_req = 35 }, /* DMA_SPI1_TX0 */
 	{ .name = "rx0", .dma_req = 36 }, /* DMA_SPI1_RX0 */
@@ -1839,7 +1728,7 @@ static struct omap2_mcspi_dev_attr omap_mcspi1_dev_attr = {
 
 static struct omap_hwmod omap2430_mcspi1_hwmod = {
 	.name		= "mcspi1_hwmod",
-	.mpu_irqs	= omap2430_mcspi1_mpu_irqs,
+	.mpu_irqs	= omap2_mcspi1_mpu_irqs,
 	.sdma_reqs	= omap2430_mcspi1_sdma_reqs,
 	.sdma_reqs_cnt	= ARRAY_SIZE(omap2430_mcspi1_sdma_reqs),
 	.main_clk	= "mcspi1_fck",
@@ -1860,11 +1749,6 @@ static struct omap_hwmod omap2430_mcspi1_hwmod = {
 };
 
 /* mcspi2 */
-static struct omap_hwmod_irq_info omap2430_mcspi2_mpu_irqs[] = {
-	{ .irq = 66 },
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_dma_info omap2430_mcspi2_sdma_reqs[] = {
 	{ .name = "tx0", .dma_req = 43 }, /* DMA_SPI2_TX0 */
 	{ .name = "rx0", .dma_req = 44 }, /* DMA_SPI2_RX0 */
@@ -1882,7 +1766,7 @@ static struct omap2_mcspi_dev_attr omap_mcspi2_dev_attr = {
 
 static struct omap_hwmod omap2430_mcspi2_hwmod = {
 	.name		= "mcspi2_hwmod",
-	.mpu_irqs	= omap2430_mcspi2_mpu_irqs,
+	.mpu_irqs	= omap2_mcspi2_mpu_irqs,
 	.sdma_reqs	= omap2430_mcspi2_sdma_reqs,
 	.sdma_reqs_cnt	= ARRAY_SIZE(omap2430_mcspi2_sdma_reqs),
 	.main_clk	= "mcspi2_fck",
diff --git a/arch/arm/mach-omap2/omap_hwmod_2xxx_3xxx_ipblock_data.c b/arch/arm/mach-omap2/omap_hwmod_2xxx_3xxx_ipblock_data.c
new file mode 100644
index 0000000..245294b
--- /dev/null
+++ b/arch/arm/mach-omap2/omap_hwmod_2xxx_3xxx_ipblock_data.c
@@ -0,0 +1,142 @@
+/*
+ * omap_hwmod_2xxx_3xxx_ipblock_data.c - common IP block data for OMAP2/3
+ *
+ * Copyright (C) 2011 Nokia Corporation
+ * Paul Walmsley
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+#include <plat/omap_hwmod.h>
+#include <plat/serial.h>
+
+#include <mach/irqs.h>
+
+#include "omap_hwmod_common_data.h"
+
+struct omap_hwmod_irq_info omap2_timer1_mpu_irqs[] = {
+	{ .irq = 37, },
+	{ .irq = -1 }
+};
+
+struct omap_hwmod_irq_info omap2_timer2_mpu_irqs[] = {
+	{ .irq = 38, },
+	{ .irq = -1 }
+};
+
+struct omap_hwmod_irq_info omap2_timer3_mpu_irqs[] = {
+	{ .irq = 39, },
+	{ .irq = -1 }
+};
+
+struct omap_hwmod_irq_info omap2_timer4_mpu_irqs[] = {
+	{ .irq = 40, },
+	{ .irq = -1 }
+};
+
+struct omap_hwmod_irq_info omap2_timer5_mpu_irqs[] = {
+	{ .irq = 41, },
+	{ .irq = -1 }
+};
+
+struct omap_hwmod_irq_info omap2_timer6_mpu_irqs[] = {
+	{ .irq = 42, },
+	{ .irq = -1 }
+};
+
+struct omap_hwmod_irq_info omap2_timer7_mpu_irqs[] = {
+	{ .irq = 43, },
+	{ .irq = -1 }
+};
+
+struct omap_hwmod_irq_info omap2_timer8_mpu_irqs[] = {
+	{ .irq = 44, },
+	{ .irq = -1 }
+};
+
+struct omap_hwmod_irq_info omap2_timer9_mpu_irqs[] = {
+	{ .irq = 45, },
+	{ .irq = -1 }
+};
+
+struct omap_hwmod_irq_info omap2_timer10_mpu_irqs[] = {
+	{ .irq = 46, },
+	{ .irq = -1 }
+};
+
+struct omap_hwmod_irq_info omap2_timer11_mpu_irqs[] = {
+	{ .irq = 47, },
+	{ .irq = -1 }
+};
+
+struct omap_hwmod_irq_info omap2_uart1_mpu_irqs[] = {
+	{ .irq = INT_24XX_UART1_IRQ, },
+	{ .irq = -1 }
+};
+
+struct omap_hwmod_irq_info omap2_uart2_mpu_irqs[] = {
+	{ .irq = INT_24XX_UART2_IRQ, },
+	{ .irq = -1 }
+};
+
+struct omap_hwmod_irq_info omap2_uart3_mpu_irqs[] = {
+	{ .irq = INT_24XX_UART3_IRQ, },
+	{ .irq = -1 }
+};
+
+struct omap_hwmod_irq_info omap2_dispc_irqs[] = {
+	{ .irq = 25 },
+	{ .irq = -1 }
+};
+
+struct omap_hwmod_irq_info omap2_i2c1_mpu_irqs[] = {
+	{ .irq = INT_24XX_I2C1_IRQ, },
+	{ .irq = -1 }
+};
+
+struct omap_hwmod_irq_info omap2_i2c2_mpu_irqs[] = {
+	{ .irq = INT_24XX_I2C2_IRQ, },
+	{ .irq = -1 }
+};
+
+struct omap_hwmod_irq_info omap2_gpio1_irqs[] = {
+	{ .irq = 29 }, /* INT_24XX_GPIO_BANK1 */
+	{ .irq = -1 }
+};
+
+struct omap_hwmod_irq_info omap2_gpio2_irqs[] = {
+	{ .irq = 30 }, /* INT_24XX_GPIO_BANK2 */
+	{ .irq = -1 }
+};
+
+struct omap_hwmod_irq_info omap2_gpio3_irqs[] = {
+	{ .irq = 31 }, /* INT_24XX_GPIO_BANK3 */
+	{ .irq = -1 }
+};
+
+struct omap_hwmod_irq_info omap2_gpio4_irqs[] = {
+	{ .irq = 32 }, /* INT_24XX_GPIO_BANK4 */
+	{ .irq = -1 }
+};
+
+struct omap_hwmod_irq_info omap2_dma_system_irqs[] = {
+	{ .name = "0", .irq = 12 }, /* INT_24XX_SDMA_IRQ0 */
+	{ .name = "1", .irq = 13 }, /* INT_24XX_SDMA_IRQ1 */
+	{ .name = "2", .irq = 14 }, /* INT_24XX_SDMA_IRQ2 */
+	{ .name = "3", .irq = 15 }, /* INT_24XX_SDMA_IRQ3 */
+	{ .irq = -1 }
+};
+
+struct omap_hwmod_irq_info omap2_mcspi1_mpu_irqs[] = {
+	{ .irq = 65 },
+	{ .irq = -1 }
+};
+
+struct omap_hwmod_irq_info omap2_mcspi2_mpu_irqs[] = {
+	{ .irq = 66 },
+	{ .irq = -1 }
+};
+
+
+
diff --git a/arch/arm/mach-omap2/omap_hwmod_2xxx_ipblock_data.c b/arch/arm/mach-omap2/omap_hwmod_2xxx_ipblock_data.c
new file mode 100644
index 0000000..5a078a6
--- /dev/null
+++ b/arch/arm/mach-omap2/omap_hwmod_2xxx_ipblock_data.c
@@ -0,0 +1,21 @@
+/*
+ * omap_hwmod_2xxx_ipblock_data.c - common IP block data for OMAP2xxx
+ *
+ * Copyright (C) 2011 Nokia Corporation
+ * Paul Walmsley
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+#include <plat/omap_hwmod.h>
+#include <plat/serial.h>
+
+#include <mach/irqs.h>
+
+#include "omap_hwmod_common_data.h"
+
+struct omap_hwmod_irq_info omap2xxx_timer12_mpu_irqs[] = {
+	{ .irq = 48, },
+	{ .irq = -1 }
+};
diff --git a/arch/arm/mach-omap2/omap_hwmod_3xxx_data.c b/arch/arm/mach-omap2/omap_hwmod_3xxx_data.c
index cc178b5..6bac4bb 100644
--- a/arch/arm/mach-omap2/omap_hwmod_3xxx_data.c
+++ b/arch/arm/mach-omap2/omap_hwmod_3xxx_data.c
@@ -151,7 +151,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_l3_main_masters[] = {
 static struct omap_hwmod omap3xxx_l3_main_hwmod = {
 	.name		= "l3_main",
 	.class		= &l3_hwmod_class,
-	.mpu_irqs       = omap3xxx_l3_main_irqs,
+	.mpu_irqs	= omap3xxx_l3_main_irqs,
 	.masters	= omap3xxx_l3_main_masters,
 	.masters_cnt	= ARRAY_SIZE(omap3xxx_l3_main_masters),
 	.slaves		= omap3xxx_l3_main_slaves,
@@ -572,10 +572,6 @@ static struct omap_hwmod_class omap3xxx_timer_hwmod_class = {
 
 /* timer1 */
 static struct omap_hwmod omap3xxx_timer1_hwmod;
-static struct omap_hwmod_irq_info omap3xxx_timer1_mpu_irqs[] = {
-	{ .irq = 37, },
-	{ .irq = -1 }
-};
 
 static struct omap_hwmod_addr_space omap3xxx_timer1_addrs[] = {
 	{
@@ -603,7 +599,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_timer1_slaves[] = {
 /* timer1 hwmod */
 static struct omap_hwmod omap3xxx_timer1_hwmod = {
 	.name		= "timer1",
-	.mpu_irqs	= omap3xxx_timer1_mpu_irqs,
+	.mpu_irqs	= omap2_timer1_mpu_irqs,
 	.main_clk	= "gpt1_fck",
 	.prcm		= {
 		.omap2 = {
@@ -622,10 +618,6 @@ static struct omap_hwmod omap3xxx_timer1_hwmod = {
 
 /* timer2 */
 static struct omap_hwmod omap3xxx_timer2_hwmod;
-static struct omap_hwmod_irq_info omap3xxx_timer2_mpu_irqs[] = {
-	{ .irq = 38, },
-	{ .irq = -1 }
-};
 
 static struct omap_hwmod_addr_space omap3xxx_timer2_addrs[] = {
 	{
@@ -653,7 +645,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_timer2_slaves[] = {
 /* timer2 hwmod */
 static struct omap_hwmod omap3xxx_timer2_hwmod = {
 	.name		= "timer2",
-	.mpu_irqs	= omap3xxx_timer2_mpu_irqs,
+	.mpu_irqs	= omap2_timer2_mpu_irqs,
 	.main_clk	= "gpt2_fck",
 	.prcm		= {
 		.omap2 = {
@@ -672,10 +664,6 @@ static struct omap_hwmod omap3xxx_timer2_hwmod = {
 
 /* timer3 */
 static struct omap_hwmod omap3xxx_timer3_hwmod;
-static struct omap_hwmod_irq_info omap3xxx_timer3_mpu_irqs[] = {
-	{ .irq = 39, },
-	{ .irq = -1 }
-};
 
 static struct omap_hwmod_addr_space omap3xxx_timer3_addrs[] = {
 	{
@@ -703,7 +691,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_timer3_slaves[] = {
 /* timer3 hwmod */
 static struct omap_hwmod omap3xxx_timer3_hwmod = {
 	.name		= "timer3",
-	.mpu_irqs	= omap3xxx_timer3_mpu_irqs,
+	.mpu_irqs	= omap2_timer3_mpu_irqs,
 	.main_clk	= "gpt3_fck",
 	.prcm		= {
 		.omap2 = {
@@ -722,10 +710,6 @@ static struct omap_hwmod omap3xxx_timer3_hwmod = {
 
 /* timer4 */
 static struct omap_hwmod omap3xxx_timer4_hwmod;
-static struct omap_hwmod_irq_info omap3xxx_timer4_mpu_irqs[] = {
-	{ .irq = 40, },
-	{ .irq = -1 }
-};
 
 static struct omap_hwmod_addr_space omap3xxx_timer4_addrs[] = {
 	{
@@ -753,7 +737,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_timer4_slaves[] = {
 /* timer4 hwmod */
 static struct omap_hwmod omap3xxx_timer4_hwmod = {
 	.name		= "timer4",
-	.mpu_irqs	= omap3xxx_timer4_mpu_irqs,
+	.mpu_irqs	= omap2_timer4_mpu_irqs,
 	.main_clk	= "gpt4_fck",
 	.prcm		= {
 		.omap2 = {
@@ -772,10 +756,6 @@ static struct omap_hwmod omap3xxx_timer4_hwmod = {
 
 /* timer5 */
 static struct omap_hwmod omap3xxx_timer5_hwmod;
-static struct omap_hwmod_irq_info omap3xxx_timer5_mpu_irqs[] = {
-	{ .irq = 41, },
-	{ .irq = -1 }
-};
 
 static struct omap_hwmod_addr_space omap3xxx_timer5_addrs[] = {
 	{
@@ -803,7 +783,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_timer5_slaves[] = {
 /* timer5 hwmod */
 static struct omap_hwmod omap3xxx_timer5_hwmod = {
 	.name		= "timer5",
-	.mpu_irqs	= omap3xxx_timer5_mpu_irqs,
+	.mpu_irqs	= omap2_timer5_mpu_irqs,
 	.main_clk	= "gpt5_fck",
 	.prcm		= {
 		.omap2 = {
@@ -822,10 +802,6 @@ static struct omap_hwmod omap3xxx_timer5_hwmod = {
 
 /* timer6 */
 static struct omap_hwmod omap3xxx_timer6_hwmod;
-static struct omap_hwmod_irq_info omap3xxx_timer6_mpu_irqs[] = {
-	{ .irq = 42, },
-	{ .irq = -1 }
-};
 
 static struct omap_hwmod_addr_space omap3xxx_timer6_addrs[] = {
 	{
@@ -853,7 +829,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_timer6_slaves[] = {
 /* timer6 hwmod */
 static struct omap_hwmod omap3xxx_timer6_hwmod = {
 	.name		= "timer6",
-	.mpu_irqs	= omap3xxx_timer6_mpu_irqs,
+	.mpu_irqs	= omap2_timer6_mpu_irqs,
 	.main_clk	= "gpt6_fck",
 	.prcm		= {
 		.omap2 = {
@@ -872,10 +848,6 @@ static struct omap_hwmod omap3xxx_timer6_hwmod = {
 
 /* timer7 */
 static struct omap_hwmod omap3xxx_timer7_hwmod;
-static struct omap_hwmod_irq_info omap3xxx_timer7_mpu_irqs[] = {
-	{ .irq = 43, },
-	{ .irq = -1 }
-};
 
 static struct omap_hwmod_addr_space omap3xxx_timer7_addrs[] = {
 	{
@@ -903,7 +875,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_timer7_slaves[] = {
 /* timer7 hwmod */
 static struct omap_hwmod omap3xxx_timer7_hwmod = {
 	.name		= "timer7",
-	.mpu_irqs	= omap3xxx_timer7_mpu_irqs,
+	.mpu_irqs	= omap2_timer7_mpu_irqs,
 	.main_clk	= "gpt7_fck",
 	.prcm		= {
 		.omap2 = {
@@ -922,10 +894,6 @@ static struct omap_hwmod omap3xxx_timer7_hwmod = {
 
 /* timer8 */
 static struct omap_hwmod omap3xxx_timer8_hwmod;
-static struct omap_hwmod_irq_info omap3xxx_timer8_mpu_irqs[] = {
-	{ .irq = 44, },
-	{ .irq = -1 }
-};
 
 static struct omap_hwmod_addr_space omap3xxx_timer8_addrs[] = {
 	{
@@ -953,7 +921,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_timer8_slaves[] = {
 /* timer8 hwmod */
 static struct omap_hwmod omap3xxx_timer8_hwmod = {
 	.name		= "timer8",
-	.mpu_irqs	= omap3xxx_timer8_mpu_irqs,
+	.mpu_irqs	= omap2_timer8_mpu_irqs,
 	.main_clk	= "gpt8_fck",
 	.prcm		= {
 		.omap2 = {
@@ -972,10 +940,6 @@ static struct omap_hwmod omap3xxx_timer8_hwmod = {
 
 /* timer9 */
 static struct omap_hwmod omap3xxx_timer9_hwmod;
-static struct omap_hwmod_irq_info omap3xxx_timer9_mpu_irqs[] = {
-	{ .irq = 45, },
-	{ .irq = -1 }
-};
 
 static struct omap_hwmod_addr_space omap3xxx_timer9_addrs[] = {
 	{
@@ -1003,7 +967,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_timer9_slaves[] = {
 /* timer9 hwmod */
 static struct omap_hwmod omap3xxx_timer9_hwmod = {
 	.name		= "timer9",
-	.mpu_irqs	= omap3xxx_timer9_mpu_irqs,
+	.mpu_irqs	= omap2_timer9_mpu_irqs,
 	.main_clk	= "gpt9_fck",
 	.prcm		= {
 		.omap2 = {
@@ -1022,10 +986,6 @@ static struct omap_hwmod omap3xxx_timer9_hwmod = {
 
 /* timer10 */
 static struct omap_hwmod omap3xxx_timer10_hwmod;
-static struct omap_hwmod_irq_info omap3xxx_timer10_mpu_irqs[] = {
-	{ .irq = 46, },
-	{ .irq = -1 }
-};
 
 /* l4_core -> timer10 */
 static struct omap_hwmod_ocp_if omap3xxx_l4_core__timer10 = {
@@ -1044,7 +1004,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_timer10_slaves[] = {
 /* timer10 hwmod */
 static struct omap_hwmod omap3xxx_timer10_hwmod = {
 	.name		= "timer10",
-	.mpu_irqs	= omap3xxx_timer10_mpu_irqs,
+	.mpu_irqs	= omap2_timer10_mpu_irqs,
 	.main_clk	= "gpt10_fck",
 	.prcm		= {
 		.omap2 = {
@@ -1063,10 +1023,6 @@ static struct omap_hwmod omap3xxx_timer10_hwmod = {
 
 /* timer11 */
 static struct omap_hwmod omap3xxx_timer11_hwmod;
-static struct omap_hwmod_irq_info omap3xxx_timer11_mpu_irqs[] = {
-	{ .irq = 47, },
-	{ .irq = -1 }
-};
 
 /* l4_core -> timer11 */
 static struct omap_hwmod_ocp_if omap3xxx_l4_core__timer11 = {
@@ -1085,7 +1041,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_timer11_slaves[] = {
 /* timer11 hwmod */
 static struct omap_hwmod omap3xxx_timer11_hwmod = {
 	.name		= "timer11",
-	.mpu_irqs	= omap3xxx_timer11_mpu_irqs,
+	.mpu_irqs	= omap2_timer11_mpu_irqs,
 	.main_clk	= "gpt11_fck",
 	.prcm		= {
 		.omap2 = {
@@ -1254,11 +1210,6 @@ static struct omap_hwmod_class uart_class = {
 
 /* UART1 */
 
-static struct omap_hwmod_irq_info uart1_mpu_irqs[] = {
-	{ .irq = INT_24XX_UART1_IRQ, },
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_dma_info uart1_sdma_reqs[] = {
 	{ .name = "tx",	.dma_req = OMAP24XX_DMA_UART1_TX, },
 	{ .name = "rx",	.dma_req = OMAP24XX_DMA_UART1_RX, },
@@ -1270,7 +1221,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_uart1_slaves[] = {
 
 static struct omap_hwmod omap3xxx_uart1_hwmod = {
 	.name		= "uart1",
-	.mpu_irqs	= uart1_mpu_irqs,
+	.mpu_irqs	= omap2_uart1_mpu_irqs,
 	.sdma_reqs	= uart1_sdma_reqs,
 	.sdma_reqs_cnt	= ARRAY_SIZE(uart1_sdma_reqs),
 	.main_clk	= "uart1_fck",
@@ -1291,11 +1242,6 @@ static struct omap_hwmod omap3xxx_uart1_hwmod = {
 
 /* UART2 */
 
-static struct omap_hwmod_irq_info uart2_mpu_irqs[] = {
-	{ .irq = INT_24XX_UART2_IRQ, },
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_dma_info uart2_sdma_reqs[] = {
 	{ .name = "tx",	.dma_req = OMAP24XX_DMA_UART2_TX, },
 	{ .name = "rx",	.dma_req = OMAP24XX_DMA_UART2_RX, },
@@ -1307,7 +1253,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_uart2_slaves[] = {
 
 static struct omap_hwmod omap3xxx_uart2_hwmod = {
 	.name		= "uart2",
-	.mpu_irqs	= uart2_mpu_irqs,
+	.mpu_irqs	= omap2_uart2_mpu_irqs,
 	.sdma_reqs	= uart2_sdma_reqs,
 	.sdma_reqs_cnt	= ARRAY_SIZE(uart2_sdma_reqs),
 	.main_clk	= "uart2_fck",
@@ -1328,11 +1274,6 @@ static struct omap_hwmod omap3xxx_uart2_hwmod = {
 
 /* UART3 */
 
-static struct omap_hwmod_irq_info uart3_mpu_irqs[] = {
-	{ .irq = INT_24XX_UART3_IRQ, },
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_dma_info uart3_sdma_reqs[] = {
 	{ .name = "tx",	.dma_req = OMAP24XX_DMA_UART3_TX, },
 	{ .name = "rx",	.dma_req = OMAP24XX_DMA_UART3_RX, },
@@ -1344,7 +1285,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_uart3_slaves[] = {
 
 static struct omap_hwmod omap3xxx_uart3_hwmod = {
 	.name		= "uart3",
-	.mpu_irqs	= uart3_mpu_irqs,
+	.mpu_irqs	= omap2_uart3_mpu_irqs,
 	.sdma_reqs	= uart3_sdma_reqs,
 	.sdma_reqs_cnt	= ARRAY_SIZE(uart3_sdma_reqs),
 	.main_clk	= "uart3_fck",
@@ -1555,11 +1496,6 @@ static struct omap_hwmod_class omap3xxx_dispc_hwmod_class = {
 	.sysc = &omap3xxx_dispc_sysc,
 };
 
-static struct omap_hwmod_irq_info omap3xxx_dispc_irqs[] = {
-	{ .irq = 25 },
-	{ .irq = -1 }
-};
-
 /* l4_core -> dss_dispc */
 static struct omap_hwmod_ocp_if omap3xxx_l4_core__dss_dispc = {
 	.master		= &omap3xxx_l4_core_hwmod,
@@ -1584,7 +1520,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_dss_dispc_slaves[] = {
 static struct omap_hwmod omap3xxx_dss_dispc_hwmod = {
 	.name		= "dss_dispc",
 	.class		= &omap3xxx_dispc_hwmod_class,
-	.mpu_irqs	= omap3xxx_dispc_irqs,
+	.mpu_irqs	= omap2_dispc_irqs,
 	.main_clk	= "dss1_alwon_fck",
 	.prcm		= {
 		.omap2 = {
@@ -1781,11 +1717,6 @@ static struct omap_i2c_dev_attr i2c1_dev_attr = {
 	.fifo_depth	= 8, /* bytes */
 };
 
-static struct omap_hwmod_irq_info i2c1_mpu_irqs[] = {
-	{ .irq = INT_24XX_I2C1_IRQ, },
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_dma_info i2c1_sdma_reqs[] = {
 	{ .name = "tx", .dma_req = OMAP24XX_DMA_I2C1_TX },
 	{ .name = "rx", .dma_req = OMAP24XX_DMA_I2C1_RX },
@@ -1797,7 +1728,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_i2c1_slaves[] = {
 
 static struct omap_hwmod omap3xxx_i2c1_hwmod = {
 	.name		= "i2c1",
-	.mpu_irqs	= i2c1_mpu_irqs,
+	.mpu_irqs	= omap2_i2c1_mpu_irqs,
 	.sdma_reqs	= i2c1_sdma_reqs,
 	.sdma_reqs_cnt	= ARRAY_SIZE(i2c1_sdma_reqs),
 	.main_clk	= "i2c1_fck",
@@ -1823,11 +1754,6 @@ static struct omap_i2c_dev_attr i2c2_dev_attr = {
 	.fifo_depth	= 8, /* bytes */
 };
 
-static struct omap_hwmod_irq_info i2c2_mpu_irqs[] = {
-	{ .irq = INT_24XX_I2C2_IRQ, },
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_dma_info i2c2_sdma_reqs[] = {
 	{ .name = "tx", .dma_req = OMAP24XX_DMA_I2C2_TX },
 	{ .name = "rx", .dma_req = OMAP24XX_DMA_I2C2_RX },
@@ -1839,7 +1765,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_i2c2_slaves[] = {
 
 static struct omap_hwmod omap3xxx_i2c2_hwmod = {
 	.name		= "i2c2",
-	.mpu_irqs	= i2c2_mpu_irqs,
+	.mpu_irqs	= omap2_i2c2_mpu_irqs,
 	.sdma_reqs	= i2c2_sdma_reqs,
 	.sdma_reqs_cnt	= ARRAY_SIZE(i2c2_sdma_reqs),
 	.main_clk	= "i2c2_fck",
@@ -2032,11 +1958,6 @@ static struct omap_gpio_dev_attr gpio_dev_attr = {
 };
 
 /* gpio1 */
-static struct omap_hwmod_irq_info omap3xxx_gpio1_irqs[] = {
-	{ .irq = 29 }, /* INT_34XX_GPIO_BANK1 */
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_opt_clk gpio1_opt_clks[] = {
 	{ .role = "dbclk", .clk = "gpio1_dbck", },
 };
@@ -2048,7 +1969,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_gpio1_slaves[] = {
 static struct omap_hwmod omap3xxx_gpio1_hwmod = {
 	.name		= "gpio1",
 	.flags		= HWMOD_CONTROL_OPT_CLKS_IN_RESET,
-	.mpu_irqs	= omap3xxx_gpio1_irqs,
+	.mpu_irqs	= omap2_gpio1_irqs,
 	.main_clk	= "gpio1_ick",
 	.opt_clks	= gpio1_opt_clks,
 	.opt_clks_cnt	= ARRAY_SIZE(gpio1_opt_clks),
@@ -2069,11 +1990,6 @@ static struct omap_hwmod omap3xxx_gpio1_hwmod = {
 };
 
 /* gpio2 */
-static struct omap_hwmod_irq_info omap3xxx_gpio2_irqs[] = {
-	{ .irq = 30 }, /* INT_34XX_GPIO_BANK2 */
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_opt_clk gpio2_opt_clks[] = {
 	{ .role = "dbclk", .clk = "gpio2_dbck", },
 };
@@ -2085,7 +2001,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_gpio2_slaves[] = {
 static struct omap_hwmod omap3xxx_gpio2_hwmod = {
 	.name		= "gpio2",
 	.flags		= HWMOD_CONTROL_OPT_CLKS_IN_RESET,
-	.mpu_irqs	= omap3xxx_gpio2_irqs,
+	.mpu_irqs	= omap2_gpio2_irqs,
 	.main_clk	= "gpio2_ick",
 	.opt_clks	= gpio2_opt_clks,
 	.opt_clks_cnt	= ARRAY_SIZE(gpio2_opt_clks),
@@ -2106,11 +2022,6 @@ static struct omap_hwmod omap3xxx_gpio2_hwmod = {
 };
 
 /* gpio3 */
-static struct omap_hwmod_irq_info omap3xxx_gpio3_irqs[] = {
-	{ .irq = 31 }, /* INT_34XX_GPIO_BANK3 */
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_opt_clk gpio3_opt_clks[] = {
 	{ .role = "dbclk", .clk = "gpio3_dbck", },
 };
@@ -2122,7 +2033,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_gpio3_slaves[] = {
 static struct omap_hwmod omap3xxx_gpio3_hwmod = {
 	.name		= "gpio3",
 	.flags		= HWMOD_CONTROL_OPT_CLKS_IN_RESET,
-	.mpu_irqs	= omap3xxx_gpio3_irqs,
+	.mpu_irqs	= omap2_gpio3_irqs,
 	.main_clk	= "gpio3_ick",
 	.opt_clks	= gpio3_opt_clks,
 	.opt_clks_cnt	= ARRAY_SIZE(gpio3_opt_clks),
@@ -2143,11 +2054,6 @@ static struct omap_hwmod omap3xxx_gpio3_hwmod = {
 };
 
 /* gpio4 */
-static struct omap_hwmod_irq_info omap3xxx_gpio4_irqs[] = {
-	{ .irq = 32 }, /* INT_34XX_GPIO_BANK4 */
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_opt_clk gpio4_opt_clks[] = {
 	{ .role = "dbclk", .clk = "gpio4_dbck", },
 };
@@ -2159,7 +2065,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_gpio4_slaves[] = {
 static struct omap_hwmod omap3xxx_gpio4_hwmod = {
 	.name		= "gpio4",
 	.flags		= HWMOD_CONTROL_OPT_CLKS_IN_RESET,
-	.mpu_irqs	= omap3xxx_gpio4_irqs,
+	.mpu_irqs	= omap2_gpio4_irqs,
 	.main_clk	= "gpio4_ick",
 	.opt_clks	= gpio4_opt_clks,
 	.opt_clks_cnt	= ARRAY_SIZE(gpio4_opt_clks),
@@ -2287,14 +2193,6 @@ static struct omap_hwmod_class omap3xxx_dma_hwmod_class = {
 };
 
 /* dma_system */
-static struct omap_hwmod_irq_info omap3xxx_dma_system_irqs[] = {
-	{ .name = "0", .irq = 12 }, /* INT_24XX_SDMA_IRQ0 */
-	{ .name = "1", .irq = 13 }, /* INT_24XX_SDMA_IRQ1 */
-	{ .name = "2", .irq = 14 }, /* INT_24XX_SDMA_IRQ2 */
-	{ .name = "3", .irq = 15 }, /* INT_24XX_SDMA_IRQ3 */
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_addr_space omap3xxx_dma_system_addrs[] = {
 	{
 		.pa_start	= 0x48056000,
@@ -2326,7 +2224,7 @@ static struct omap_hwmod_ocp_if *omap3xxx_dma_system_slaves[] = {
 static struct omap_hwmod omap3xxx_dma_system_hwmod = {
 	.name		= "dma",
 	.class		= &omap3xxx_dma_hwmod_class,
-	.mpu_irqs	= omap3xxx_dma_system_irqs,
+	.mpu_irqs	= omap2_dma_system_irqs,
 	.main_clk	= "core_l3_ick",
 	.prcm = {
 		.omap2 = {
@@ -3044,11 +2942,6 @@ static struct omap_hwmod_class omap34xx_mcspi_class = {
 };
 
 /* mcspi1 */
-static struct omap_hwmod_irq_info omap34xx_mcspi1_mpu_irqs[] = {
-	{ .name = "irq", .irq = 65 },
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_dma_info omap34xx_mcspi1_sdma_reqs[] = {
 	{ .name = "tx0", .dma_req = 35 },
 	{ .name = "rx0", .dma_req = 36 },
@@ -3070,7 +2963,7 @@ static struct omap2_mcspi_dev_attr omap_mcspi1_dev_attr = {
 
 static struct omap_hwmod omap34xx_mcspi1 = {
 	.name		= "mcspi1",
-	.mpu_irqs	= omap34xx_mcspi1_mpu_irqs,
+	.mpu_irqs	= omap2_mcspi1_mpu_irqs,
 	.sdma_reqs	= omap34xx_mcspi1_sdma_reqs,
 	.sdma_reqs_cnt	= ARRAY_SIZE(omap34xx_mcspi1_sdma_reqs),
 	.main_clk	= "mcspi1_fck",
@@ -3091,11 +2984,6 @@ static struct omap_hwmod omap34xx_mcspi1 = {
 };
 
 /* mcspi2 */
-static struct omap_hwmod_irq_info omap34xx_mcspi2_mpu_irqs[] = {
-	{ .name = "irq", .irq = 66 },
-	{ .irq = -1 }
-};
-
 static struct omap_hwmod_dma_info omap34xx_mcspi2_sdma_reqs[] = {
 	{ .name = "tx0", .dma_req = 43 },
 	{ .name = "rx0", .dma_req = 44 },
@@ -3113,7 +3001,7 @@ static struct omap2_mcspi_dev_attr omap_mcspi2_dev_attr = {
 
 static struct omap_hwmod omap34xx_mcspi2 = {
 	.name		= "mcspi2",
-	.mpu_irqs	= omap34xx_mcspi2_mpu_irqs,
+	.mpu_irqs	= omap2_mcspi2_mpu_irqs,
 	.sdma_reqs	= omap34xx_mcspi2_sdma_reqs,
 	.sdma_reqs_cnt	= ARRAY_SIZE(omap34xx_mcspi2_sdma_reqs),
 	.main_clk	= "mcspi2_fck",
diff --git a/arch/arm/mach-omap2/omap_hwmod_common_data.h b/arch/arm/mach-omap2/omap_hwmod_common_data.h
index 76a2f11..1ac878c 100644
--- a/arch/arm/mach-omap2/omap_hwmod_common_data.h
+++ b/arch/arm/mach-omap2/omap_hwmod_common_data.h
@@ -49,6 +49,35 @@ extern struct omap_hwmod_addr_space omap2_dma_system_addrs[];
 extern struct omap_hwmod_addr_space omap2_mailbox_addrs[];
 extern struct omap_hwmod_addr_space omap2_mcbsp1_addrs[];
 
+/* Common IP block data across OMAP2xxx */
+extern struct omap_hwmod_irq_info omap2xxx_timer12_mpu_irqs[];
+
+/* Common IP block data across OMAP2/3 */
+extern struct omap_hwmod_irq_info omap2_timer1_mpu_irqs[];
+extern struct omap_hwmod_irq_info omap2_timer2_mpu_irqs[];
+extern struct omap_hwmod_irq_info omap2_timer3_mpu_irqs[];
+extern struct omap_hwmod_irq_info omap2_timer4_mpu_irqs[];
+extern struct omap_hwmod_irq_info omap2_timer5_mpu_irqs[];
+extern struct omap_hwmod_irq_info omap2_timer6_mpu_irqs[];
+extern struct omap_hwmod_irq_info omap2_timer7_mpu_irqs[];
+extern struct omap_hwmod_irq_info omap2_timer8_mpu_irqs[];
+extern struct omap_hwmod_irq_info omap2_timer9_mpu_irqs[];
+extern struct omap_hwmod_irq_info omap2_timer10_mpu_irqs[];
+extern struct omap_hwmod_irq_info omap2_timer11_mpu_irqs[];
+extern struct omap_hwmod_irq_info omap2_uart1_mpu_irqs[];
+extern struct omap_hwmod_irq_info omap2_uart2_mpu_irqs[];
+extern struct omap_hwmod_irq_info omap2_uart3_mpu_irqs[];
+extern struct omap_hwmod_irq_info omap2_dispc_irqs[];
+extern struct omap_hwmod_irq_info omap2_i2c1_mpu_irqs[];
+extern struct omap_hwmod_irq_info omap2_i2c2_mpu_irqs[];
+extern struct omap_hwmod_irq_info omap2_gpio1_irqs[];
+extern struct omap_hwmod_irq_info omap2_gpio2_irqs[];
+extern struct omap_hwmod_irq_info omap2_gpio3_irqs[];
+extern struct omap_hwmod_irq_info omap2_gpio4_irqs[];
+extern struct omap_hwmod_irq_info omap2_dma_system_irqs[];
+extern struct omap_hwmod_irq_info omap2_mcspi1_mpu_irqs[];
+extern struct omap_hwmod_irq_info omap2_mcspi2_mpu_irqs[];
+
 /* OMAP hwmod classes - forward declarations */
 extern struct omap_hwmod_class l3_hwmod_class;
 extern struct omap_hwmod_class l4_hwmod_class;
-- 
1.6.6.1

