From 9ccd5395ba746bff2eb4a5053f5b41297efe70a5 Mon Sep 17 00:00:00 2001
From: Kevin Hilman <khilman@ti.com>
Date: Mon, 4 Apr 2011 17:22:28 -0700
Subject: [PATCH 131/149] OMAP3+: VP: move SoC-specific sys clock rate retreival late init

Add sys clock name and rate to struct voltage domain.  SoC specific
voltagedomain init code initializes sys clock name.  After clock
framework is initialized, voltage late init will then use use the
sys_clk rate to calculate the various timing that depend on that rate.

Signed-off-by: Kevin Hilman <khilman@ti.com>
---
 arch/arm/mach-omap2/voltage.c                 |   47 +++++++++----------------
 arch/arm/mach-omap2/voltage.h                 |    5 +++
 arch/arm/mach-omap2/voltagedomains3xxx_data.c |    8 ++++
 arch/arm/mach-omap2/voltagedomains44xx_data.c |    8 ++++
 4 files changed, 38 insertions(+), 30 deletions(-)

diff --git a/arch/arm/mach-omap2/voltage.c b/arch/arm/mach-omap2/voltage.c
index 5b16fd1..533ea38 100644
--- a/arch/arm/mach-omap2/voltage.c
+++ b/arch/arm/mach-omap2/voltage.c
@@ -21,10 +21,10 @@
 
 #include <linux/delay.h>
 #include <linux/io.h>
-#include <linux/clk.h>
 #include <linux/err.h>
 #include <linux/debugfs.h>
 #include <linux/slab.h>
+#include <linux/clk.h>
 
 #include <plat/common.h>
 
@@ -45,36 +45,12 @@ static LIST_HEAD(voltdm_list);
 
 static int __init _config_common_vdd_data(struct voltagedomain *voltdm)
 {
-	char *sys_ck_name;
-	struct clk *sys_ck;
-	u32 sys_clk_speed, timeout_val, waittime;
 	struct omap_vdd_info *vdd = voltdm->vdd;
+	u32 sys_clk_rate, timeout_val, waittime;
 
-	/*
-	 * XXX Clockfw should handle this, or this should be in a
-	 * struct record
-	 */
-	if (cpu_is_omap24xx() || cpu_is_omap34xx())
-		sys_ck_name = "sys_ck";
-	else if (cpu_is_omap44xx())
-		sys_ck_name = "sys_clkin_ck";
-	else
-		return -EINVAL;
-
-	/*
-	 * Sys clk rate is require to calculate vp timeout value and
-	 * smpswaittimemin and smpswaittimemax.
-	 */
-	sys_ck = clk_get(NULL, sys_ck_name);
-	if (IS_ERR(sys_ck)) {
-		pr_warning("%s: Could not get the sys clk to calculate"
-			"various vdd_%s params\n", __func__, voltdm->name);
-		return -EINVAL;
-	}
-	sys_clk_speed = clk_get_rate(sys_ck);
-	clk_put(sys_ck);
 	/* Divide to avoid overflow */
-	sys_clk_speed /= 1000;
+	sys_clk_rate = voltdm->sys_clk.rate / 1000;
+	WARN_ON(!sys_clk_rate);
 
 	/* Generic voltage parameters */
 	vdd->volt_scale = omap_vp_forceupdate_scale;
@@ -84,13 +60,13 @@ static int __init _config_common_vdd_data(struct voltagedomain *voltdm)
 		(voltdm->pmic->vp_erroroffset <<
 		 __ffs(voltdm->vp->common->vpconfig_erroroffset_mask));
 
-	timeout_val = (sys_clk_speed * voltdm->pmic->vp_timeout_us) / 1000;
+	timeout_val = (sys_clk_rate * voltdm->pmic->vp_timeout_us) / 1000;
 	vdd->vp_rt_data.vlimitto_timeout = timeout_val;
 	vdd->vp_rt_data.vlimitto_vddmin = voltdm->pmic->vp_vddmin;
 	vdd->vp_rt_data.vlimitto_vddmax = voltdm->pmic->vp_vddmax;
 
 	waittime = ((voltdm->pmic->step_size / voltdm->pmic->slew_rate) *
-				sys_clk_speed) / 1000;
+		    sys_clk_rate) / 1000;
 	vdd->vp_rt_data.vstepmin_smpswaittimemin = waittime;
 	vdd->vp_rt_data.vstepmax_smpswaittimemax = waittime;
 	vdd->vp_rt_data.vstepmin_stepmin = voltdm->pmic->vp_vstepmin;
@@ -346,9 +322,20 @@ int __init omap_voltage_late_init(void)
 	}
 
 	list_for_each_entry(voltdm, &voltdm_list, node) {
+		struct clk *sys_ck;
+
 		if (!voltdm->scalable)
 			continue;
 
+		sys_ck = clk_get(NULL, voltdm->sys_clk.name);
+		if (IS_ERR(sys_ck)) {
+			pr_warning("%s: Could not get sys clk.\n", __func__);
+			return -EINVAL;
+		}
+		voltdm->sys_clk.rate = clk_get_rate(sys_ck);
+		WARN_ON(!voltdm->sys_clk.rate);
+		clk_put(sys_ck);
+
 		if (voltdm->vc) {
 			voltdm->vdd->volt_scale = omap_vc_bypass_scale;
 			omap_vc_init_channel(voltdm);
diff --git a/arch/arm/mach-omap2/voltage.h b/arch/arm/mach-omap2/voltage.h
index 5261703..d73c956 100644
--- a/arch/arm/mach-omap2/voltage.h
+++ b/arch/arm/mach-omap2/voltage.h
@@ -76,6 +76,11 @@ struct voltagedomain {
 	void (*write) (u32 val, u8 offset);
 	u32 (*rmw)(u32 mask, u32 bits, u8 offset);
 
+	union {
+		const char *name;
+		u32 rate;
+	} sys_clk;
+
 	struct omap_vdd_info *vdd;
 };
 
diff --git a/arch/arm/mach-omap2/voltagedomains3xxx_data.c b/arch/arm/mach-omap2/voltagedomains3xxx_data.c
index 4db2c6c..e7a0be1 100644
--- a/arch/arm/mach-omap2/voltagedomains3xxx_data.c
+++ b/arch/arm/mach-omap2/voltagedomains3xxx_data.c
@@ -82,8 +82,13 @@ static struct voltagedomain *voltagedomains_omap3[] __initdata = {
 	NULL,
 };
 
+static const char *sys_clk_name __initdata = "sys_ck";
+
 void __init omap3xxx_voltagedomains_init(void)
 {
+	struct voltagedomain *voltdm;
+	int i;
+
 	/*
 	 * XXX Will depend on the process, validation, and binning
 	 * for the currently-running IC
@@ -96,5 +101,8 @@ void __init omap3xxx_voltagedomains_init(void)
 		omap3_vdd2_info.volt_data = omap34xx_vddcore_volt_data;
 	}
 
+	for (i = 0; voltdm = voltagedomains_omap3[i], voltdm; i++)
+		voltdm->sys_clk.name = sys_clk_name;
+
 	voltdm_init(voltagedomains_omap3);
 };
diff --git a/arch/arm/mach-omap2/voltagedomains44xx_data.c b/arch/arm/mach-omap2/voltagedomains44xx_data.c
index 3e7cb4e..9c20fbb 100644
--- a/arch/arm/mach-omap2/voltagedomains44xx_data.c
+++ b/arch/arm/mach-omap2/voltagedomains44xx_data.c
@@ -98,8 +98,13 @@ static struct voltagedomain *voltagedomains_omap4[] __initdata = {
 	NULL,
 };
 
+static const char *sys_clk_name __initdata = "sys_clkin_ck";
+
 void __init omap44xx_voltagedomains_init(void)
 {
+	struct voltagedomain *voltdm;
+	int i;
+
 	/*
 	 * XXX Will depend on the process, validation, and binning
 	 * for the currently-running IC
@@ -108,5 +113,8 @@ void __init omap44xx_voltagedomains_init(void)
 	omap4_vdd_iva_info.volt_data = omap44xx_vdd_iva_volt_data;
 	omap4_vdd_core_info.volt_data = omap44xx_vdd_core_volt_data;
 
+	for (i = 0; voltdm = voltagedomains_omap4[i], voltdm; i++)
+		voltdm->sys_clk.name = sys_clk_name;
+
 	voltdm_init(voltagedomains_omap4);
 };
-- 
1.6.6.1

