From 1ae58f6d2ec41a1b7d0cdeca4de4b9d9760195bf Mon Sep 17 00:00:00 2001
From: Sergio Aguirre <saaguirre@ti.com>
Date: Thu, 24 Jun 2010 14:27:39 -0500
Subject: [PATCH 15/75] Revert "DEBUG: omap3beagle: camera: Force mode0 in cam_xclka"

This reverts commit 158e14b3d449dde2c6aa9f8cddb86fbbee2d2cd7.
---
 arch/arm/mach-omap2/board-omap3beagle-camera.c |    3 ---
 1 files changed, 0 insertions(+), 3 deletions(-)

diff --git a/arch/arm/mach-omap2/board-omap3beagle-camera.c b/arch/arm/mach-omap2/board-omap3beagle-camera.c
index 77f9469..1652f15 100644
--- a/arch/arm/mach-omap2/board-omap3beagle-camera.c
+++ b/arch/arm/mach-omap2/board-omap3beagle-camera.c
@@ -34,7 +34,6 @@
 
 #include <plat/mux.h>
 #include <plat/board.h>
-#include <plat/control.h>
 
 #include <media/v4l2-int-device.h>
 #include <media/mt9t111.h>
@@ -161,7 +160,6 @@ static int mt9t111_power_set(struct v4l2_int_device *s, enum v4l2_power power)
 	switch (power) {
 	case V4L2_POWER_OFF:
 	case V4L2_POWER_STANDBY:
-		omap_ctrl_writew(0x0, 0x110); /* Control XCLKA output mux */
 		isp_set_xclk(vdev->cam->isp, 0, CAM_USE_XCLKA);
 
 		if (regulator_is_enabled(beagle_mt9t111_reg1))
@@ -171,7 +169,6 @@ static int mt9t111_power_set(struct v4l2_int_device *s, enum v4l2_power power)
 		break;
 
 	case V4L2_POWER_ON:
-		omap_ctrl_writew(0x0, 0x110); /* Control XCLKA output mux */
 		isp_set_xclk(vdev->cam->isp, MT9T111_CLK_MIN, CAM_USE_XCLKA);
 
 #if defined(CONFIG_VIDEO_OMAP3) || defined(CONFIG_VIDEO_OMAP3_MODULE)
-- 
1.6.6.1

