From 857c12d206f68fb02ec55be89bf6e351df1dc71f Mon Sep 17 00:00:00 2001
From: Kevin Hilman <khilman@ti.com>
Date: Mon, 18 Jul 2011 16:24:17 -0700
Subject: [PATCH 144/149] OMAP3+: voltage: update nominal voltage in voltdm_scale() not VC post-scale

Currently, the nominal voltage is updated in the VC post-scale function
which is common to both scaling methods.  However, this has readabiliy
problems as this update is not where it might be expected.  Instead, move
the updated into voltdm_scale() upon a successful return of voltdm->scale()

Signed-off-by: Kevin Hilman <khilman@ti.com>
---
 arch/arm/mach-omap2/vc.c      |    2 --
 arch/arm/mach-omap2/voltage.c |    6 +++++-
 2 files changed, 5 insertions(+), 3 deletions(-)

diff --git a/arch/arm/mach-omap2/vc.c b/arch/arm/mach-omap2/vc.c
index 3233c69..16fa912 100644
--- a/arch/arm/mach-omap2/vc.c
+++ b/arch/arm/mach-omap2/vc.c
@@ -143,8 +143,6 @@ void omap_vc_post_scale(struct voltagedomain *voltdm,
 	smps_delay = ((smps_steps * voltdm->pmic->step_size) /
 			voltdm->pmic->slew_rate) + 2;
 	udelay(smps_delay);
-
-	voltdm->nominal_volt = target_volt;
 }
 
 /* vc_bypass_scale - VC bypass method of voltage scaling */
diff --git a/arch/arm/mach-omap2/voltage.c b/arch/arm/mach-omap2/voltage.c
index 031f6bf..cebc8b1 100644
--- a/arch/arm/mach-omap2/voltage.c
+++ b/arch/arm/mach-omap2/voltage.c
@@ -85,7 +85,11 @@ int voltdm_scale(struct voltagedomain *voltdm,
 		return -ENODATA;
 	}
 
-	return voltdm->scale(voltdm, target_volt);
+	ret = voltdm->scale(voltdm, target_volt);
+	if (!ret)
+		voltdm->nominal_volt = target_volt;
+
+	return ret;
 }
 
 /**
-- 
1.6.6.1

