From 820390a8f9a05965bf59597efe13f3f0d4fee0ec Mon Sep 17 00:00:00 2001
From: Benoit Cousson <b-cousson@ti.com>
Date: Sun, 10 Jul 2011 05:56:31 -0600
Subject: [PATCH 082/149] OMAP4: prm: Replace warm reset API with the offset based version

The warm reset function was still using the obsolete API.
Replace it by the new one and move the file to the proper c file.

Change the function names to stick to the file convention as
suggested by Paul Walmsley <paul@pwsan.com>:
prm_xxx -> prminst_xxx

Signed-off-by: Benoit Cousson <b-cousson@ti.com>
Cc: Paul Walmsley <paul@pwsan.com>
Cc: Rajendra Nayak <rnayak@ti.com>
Signed-off-by: Paul Walmsley <paul@pwsan.com>
---
 arch/arm/mach-omap2/prcm.c        |    2 +-
 arch/arm/mach-omap2/prm44xx.c     |   15 ---------------
 arch/arm/mach-omap2/prm44xx.h     |    2 --
 arch/arm/mach-omap2/prminst44xx.c |   19 +++++++++++++++++++
 arch/arm/mach-omap2/prminst44xx.h |    8 ++++----
 5 files changed, 24 insertions(+), 22 deletions(-)

diff --git a/arch/arm/mach-omap2/prcm.c b/arch/arm/mach-omap2/prcm.c
index 6be1438..2e40a5c 100644
--- a/arch/arm/mach-omap2/prcm.c
+++ b/arch/arm/mach-omap2/prcm.c
@@ -70,7 +70,7 @@ static void omap_prcm_arch_reset(char mode, const char *cmd)
 		prcm_offs = OMAP3430_GR_MOD;
 		omap3_ctrl_write_boot_mode((cmd ? (u8)*cmd : 0));
 	} else if (cpu_is_omap44xx()) {
-		omap4_prm_global_warm_sw_reset(); /* never returns */
+		omap4_prminst_global_warm_sw_reset(); /* never returns */
 	} else {
 		WARN_ON(1);
 	}
diff --git a/arch/arm/mach-omap2/prm44xx.c b/arch/arm/mach-omap2/prm44xx.c
index faec860..f815329 100644
--- a/arch/arm/mach-omap2/prm44xx.c
+++ b/arch/arm/mach-omap2/prm44xx.c
@@ -87,18 +87,3 @@ u32 omap4_prm_clear_inst_reg_bits(u32 bits, s16 inst, s16 reg)
 {
 	return omap4_prm_rmw_inst_reg_bits(bits, 0x0, inst, reg);
 }
-
-void omap4_prm_global_warm_sw_reset(void)
-{
-	u32 v;
-
-	v = omap4_prm_read_inst_reg(OMAP4430_PRM_DEVICE_INST,
-				    OMAP4_RM_RSTCTRL);
-	v |= OMAP4430_RST_GLOBAL_WARM_SW_MASK;
-	omap4_prm_write_inst_reg(v, OMAP4430_PRM_DEVICE_INST,
-				 OMAP4_RM_RSTCTRL);
-
-	/* OCP barrier */
-	v = omap4_prm_read_inst_reg(OMAP4430_PRM_DEVICE_INST,
-				    OMAP4_RM_RSTCTRL);
-}
diff --git a/arch/arm/mach-omap2/prm44xx.h b/arch/arm/mach-omap2/prm44xx.h
index 3732e02..725a6a8 100644
--- a/arch/arm/mach-omap2/prm44xx.h
+++ b/arch/arm/mach-omap2/prm44xx.h
@@ -755,8 +755,6 @@ extern u32 omap4_prm_set_inst_reg_bits(u32 bits, s16 inst, s16 idx);
 extern u32 omap4_prm_clear_inst_reg_bits(u32 bits, s16 inst, s16 idx);
 extern u32 omap4_prm_read_bits_shift(void __iomem *reg, u32 mask);
 
-extern void omap4_prm_global_warm_sw_reset(void);
-
 # endif
 
 #endif
diff --git a/arch/arm/mach-omap2/prminst44xx.c b/arch/arm/mach-omap2/prminst44xx.c
index 35e02aa..3a7bab1 100644
--- a/arch/arm/mach-omap2/prminst44xx.c
+++ b/arch/arm/mach-omap2/prminst44xx.c
@@ -155,3 +155,22 @@ int omap4_prminst_deassert_hardreset(u8 shift, u8 part, s16 inst,
 
 	return (c == MAX_MODULE_HARDRESET_WAIT) ? -EBUSY : 0;
 }
+
+
+void omap4_prminst_global_warm_sw_reset(void)
+{
+	u32 v;
+
+	v = omap4_prminst_read_inst_reg(OMAP4430_PRM_PARTITION,
+				    OMAP4430_PRM_DEVICE_INST,
+				    OMAP4_PRM_RSTCTRL_OFFSET);
+	v |= OMAP4430_RST_GLOBAL_WARM_SW_MASK;
+	omap4_prminst_write_inst_reg(v, OMAP4430_PRM_PARTITION,
+				 OMAP4430_PRM_DEVICE_INST,
+				 OMAP4_PRM_RSTCTRL_OFFSET);
+
+	/* OCP barrier */
+	v = omap4_prminst_read_inst_reg(OMAP4430_PRM_PARTITION,
+				    OMAP4430_PRM_DEVICE_INST,
+				    OMAP4_PRM_RSTCTRL_OFFSET);
+}
diff --git a/arch/arm/mach-omap2/prminst44xx.h b/arch/arm/mach-omap2/prminst44xx.h
index c14ae29..46f2efb 100644
--- a/arch/arm/mach-omap2/prminst44xx.h
+++ b/arch/arm/mach-omap2/prminst44xx.h
@@ -21,13 +21,13 @@ extern void omap4_prminst_write_inst_reg(u32 val, u8 part, s16 inst, u16 idx);
 extern u32 omap4_prminst_rmw_inst_reg_bits(u32 mask, u32 bits, u8 part,
 					   s16 inst, u16 idx);
 
-extern void omap4_prm_global_warm_sw_reset(void);
+extern void omap4_prminst_global_warm_sw_reset(void);
 
 extern int omap4_prminst_is_hardreset_asserted(u8 shift, u8 part, s16 inst,
-					   u16 rstctrl_offs);
+					       u16 rstctrl_offs);
 extern int omap4_prminst_assert_hardreset(u8 shift, u8 part, s16 inst,
-				      u16 rstctrl_offs);
+					  u16 rstctrl_offs);
 extern int omap4_prminst_deassert_hardreset(u8 shift, u8 part, s16 inst,
-					u16 rstctrl_offs);
+					    u16 rstctrl_offs);
 
 #endif
-- 
1.6.6.1

