From 13238be1e612ab4113413cf21e83307ea9e18f1e Mon Sep 17 00:00:00 2001
From: Sergio Aguirre <saaguirre@ti.com>
Date: Thu, 1 Jul 2010 13:57:26 -0500
Subject: [PATCH 56/75] omap34xxcam: Fix multi pixel format negotiation

Signed-off-by: Sergio Aguirre <saaguirre@ti.com>
---
 drivers/media/video/omap34xxcam.c |    2 +-
 1 files changed, 1 insertions(+), 1 deletions(-)

diff --git a/drivers/media/video/omap34xxcam.c b/drivers/media/video/omap34xxcam.c
index 2e8153b..051c6a7 100644
--- a/drivers/media/video/omap34xxcam.c
+++ b/drivers/media/video/omap34xxcam.c
@@ -544,7 +544,7 @@ static int try_pix_parm(struct omap34xxcam_videodev *vdev,
 				pix_tmp_out.height = pix_tmp_in.height;
 			rval = isp_try_fmt_cap(isp, &pix_tmp_in, &pix_tmp_out);
 			if (rval)
-				return rval;
+				break;
 
 			dev_dbg(&vdev->vfd->dev, "this w %d\th %d\tfmt %8.8x\t"
 				"-> w %d\th %d\t fmt %8.8x"
-- 
1.6.6.1

