From 02243f13eec816e11d16676a131bc04b8a0666ab Mon Sep 17 00:00:00 2001
From: Tomi Valkeinen <tomi.valkeinen@nokia.com>
Date: Wed, 11 Feb 2009 16:33:02 +0200
Subject: [PATCH] OMAPFB: move omapfb.h to include/linux/

This is needed so that omapfb.h is automatically exported to user space.

omapfb.h should be cleaned up later. Some stuff can probably be moved
to omapfb's private include file.

Signed-off-by: Tomi Valkeinen <tomi.valkeinen@nokia.com>
---
 arch/arm/mach-omap1/board-nokia770.c     |    2 +-
 arch/arm/mach-omap2/board-n800.c         |    2 +-
 arch/arm/mach-omap2/io.c                 |    2 +-
 arch/arm/plat-omap/fb.c                  |    2 +-
 arch/arm/plat-omap/include/mach/omapfb.h |  398 ------------------------------
 drivers/video/omap/blizzard.c            |    2 +-
 drivers/video/omap/dispc.c               |    2 +-
 drivers/video/omap/hwa742.c              |    2 +-
 drivers/video/omap/lcd_2430sdp.c         |    2 +-
 drivers/video/omap/lcd_ams_delta.c       |    2 +-
 drivers/video/omap/lcd_apollon.c         |    2 +-
 drivers/video/omap/lcd_h3.c              |    2 +-
 drivers/video/omap/lcd_h4.c              |    3 +-
 drivers/video/omap/lcd_inn1510.c         |    2 +-
 drivers/video/omap/lcd_inn1610.c         |    2 +-
 drivers/video/omap/lcd_ldp.c             |    2 +-
 drivers/video/omap/lcd_mipid.c           |    2 +-
 drivers/video/omap/lcd_omap2evm.c        |    2 +-
 drivers/video/omap/lcd_omap3beagle.c     |    2 +-
 drivers/video/omap/lcd_omap3evm.c        |    2 +-
 drivers/video/omap/lcd_osk.c             |    2 +-
 drivers/video/omap/lcd_overo.c           |    2 +-
 drivers/video/omap/lcd_p2.c              |    2 +-
 drivers/video/omap/lcd_palmte.c          |    2 +-
 drivers/video/omap/lcd_palmtt.c          |    2 +-
 drivers/video/omap/lcd_palmz71.c         |    3 +-
 drivers/video/omap/lcdc.c                |    2 +-
 drivers/video/omap/omapfb_main.c         |    2 +-
 drivers/video/omap/rfbi.c                |    3 +-
 drivers/video/omap/sossi.c               |    2 +-
 include/linux/omapfb.h                   |  398 ++++++++++++++++++++++++++++++
 31 files changed, 427 insertions(+), 430 deletions(-)
 delete mode 100644 arch/arm/plat-omap/include/mach/omapfb.h
 create mode 100644 include/linux/omapfb.h

diff --git a/arch/arm/mach-omap1/board-nokia770.c b/arch/arm/mach-omap1/board-nokia770.c
index 8780ca6..ca4680a 100644
--- a/arch/arm/mach-omap1/board-nokia770.c
+++ b/arch/arm/mach-omap1/board-nokia770.c
@@ -18,6 +18,7 @@
 #include <linux/spi/spi.h>
 #include <linux/spi/ads7846.h>
 #include <linux/workqueue.h>
+#include <linux/omapfb.h>
 #include <linux/delay.h>
 
 #include <mach/hardware.h>
@@ -32,7 +33,6 @@
 #include <mach/keypad.h>
 #include <mach/common.h>
 #include <mach/dsp_common.h>
-#include <mach/omapfb.h>
 #include <mach/lcd_mipid.h>
 #include <mach/mmc.h>
 #include <mach/usb.h>
diff --git a/arch/arm/mach-omap2/board-n800.c b/arch/arm/mach-omap2/board-n800.c
index cb32b61..f6f6571 100644
--- a/arch/arm/mach-omap2/board-n800.c
+++ b/arch/arm/mach-omap2/board-n800.c
@@ -27,6 +27,7 @@
 #include <linux/i2c/lm8323.h>
 #include <linux/i2c/menelaus.h>
 #include <linux/i2c/lp5521.h>
+#include <linux/omapfb.h>
 #include <mach/hardware.h>
 #include <asm/mach-types.h>
 #include <asm/mach/arch.h>
@@ -39,7 +40,6 @@
 #include <mach/lcd_mipid.h>
 #include <mach/clock.h>
 #include <mach/gpio-switch.h>
-#include <mach/omapfb.h>
 #include <mach/blizzard.h>
 
 #include <../drivers/cbus/tahvo.h>
diff --git a/arch/arm/mach-omap2/io.c b/arch/arm/mach-omap2/io.c
index adbe21f..a04e3ee 100644
--- a/arch/arm/mach-omap2/io.c
+++ b/arch/arm/mach-omap2/io.c
@@ -18,13 +18,13 @@
 #include <linux/module.h>
 #include <linux/kernel.h>
 #include <linux/init.h>
+#include <linux/omapfb.h>
 #include <linux/io.h>
 
 #include <asm/tlb.h>
 
 #include <asm/mach/map.h>
 #include <mach/mux.h>
-#include <mach/omapfb.h>
 #include <mach/sram.h>
 #include <mach/sdrc.h>
 #include <mach/gpmc.h>
diff --git a/arch/arm/plat-omap/fb.c b/arch/arm/plat-omap/fb.c
index 3746222..40615a6 100644
--- a/arch/arm/plat-omap/fb.c
+++ b/arch/arm/plat-omap/fb.c
@@ -28,13 +28,13 @@
 #include <linux/platform_device.h>
 #include <linux/bootmem.h>
 #include <linux/io.h>
+#include <linux/omapfb.h>
 
 #include <mach/hardware.h>
 #include <asm/mach/map.h>
 
 #include <mach/board.h>
 #include <mach/sram.h>
-#include <mach/omapfb.h>
 
 #if defined(CONFIG_FB_OMAP) || defined(CONFIG_FB_OMAP_MODULE)
 
diff --git a/arch/arm/plat-omap/include/mach/omapfb.h b/arch/arm/plat-omap/include/mach/omapfb.h
deleted file mode 100644
index b226bdf..0000000
--- a/arch/arm/plat-omap/include/mach/omapfb.h
+++ /dev/null
@@ -1,398 +0,0 @@
-/*
- * File: arch/arm/plat-omap/include/mach/omapfb.h
- *
- * Framebuffer driver for TI OMAP boards
- *
- * Copyright (C) 2004 Nokia Corporation
- * Author: Imre Deak <imre.deak@nokia.com>
- *
- * This program is free software; you can redistribute it and/or modify it
- * under the terms of the GNU General Public License as published by the
- * Free Software Foundation; either version 2 of the License, or (at your
- * option) any later version.
- *
- * This program is distributed in the hope that it will be useful, but
- * WITHOUT ANY WARRANTY; without even the implied warranty of
- * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU
- * General Public License for more details.
- *
- * You should have received a copy of the GNU General Public License along
- * with this program; if not, write to the Free Software Foundation, Inc.,
- * 59 Temple Place - Suite 330, Boston, MA  02111-1307, USA.
- */
-
-#ifndef __OMAPFB_H
-#define __OMAPFB_H
-
-#include <asm/ioctl.h>
-#include <asm/types.h>
-
-/* IOCTL commands. */
-
-#define OMAP_IOW(num, dtype)	_IOW('O', num, dtype)
-#define OMAP_IOR(num, dtype)	_IOR('O', num, dtype)
-#define OMAP_IOWR(num, dtype)	_IOWR('O', num, dtype)
-#define OMAP_IO(num)		_IO('O', num)
-
-#define OMAPFB_MIRROR		OMAP_IOW(31, int)
-#define OMAPFB_SYNC_GFX		OMAP_IO(37)
-#define OMAPFB_VSYNC		OMAP_IO(38)
-#define OMAPFB_SET_UPDATE_MODE	OMAP_IOW(40, int)
-#define OMAPFB_GET_CAPS		OMAP_IOR(42, struct omapfb_caps)
-#define OMAPFB_GET_UPDATE_MODE	OMAP_IOW(43, int)
-#define OMAPFB_LCD_TEST		OMAP_IOW(45, int)
-#define OMAPFB_CTRL_TEST	OMAP_IOW(46, int)
-#define OMAPFB_UPDATE_WINDOW_OLD OMAP_IOW(47, struct omapfb_update_window_old)
-#define OMAPFB_SET_COLOR_KEY	OMAP_IOW(50, struct omapfb_color_key)
-#define OMAPFB_GET_COLOR_KEY	OMAP_IOW(51, struct omapfb_color_key)
-#define OMAPFB_SETUP_PLANE	OMAP_IOW(52, struct omapfb_plane_info)
-#define OMAPFB_QUERY_PLANE	OMAP_IOW(53, struct omapfb_plane_info)
-#define OMAPFB_UPDATE_WINDOW	OMAP_IOW(54, struct omapfb_update_window)
-#define OMAPFB_SETUP_MEM	OMAP_IOW(55, struct omapfb_mem_info)
-#define OMAPFB_QUERY_MEM	OMAP_IOW(56, struct omapfb_mem_info)
-
-#define OMAPFB_CAPS_GENERIC_MASK	0x00000fff
-#define OMAPFB_CAPS_LCDC_MASK		0x00fff000
-#define OMAPFB_CAPS_PANEL_MASK		0xff000000
-
-#define OMAPFB_CAPS_MANUAL_UPDATE	0x00001000
-#define OMAPFB_CAPS_TEARSYNC		0x00002000
-#define OMAPFB_CAPS_PLANE_RELOCATE_MEM	0x00004000
-#define OMAPFB_CAPS_PLANE_SCALE		0x00008000
-#define OMAPFB_CAPS_WINDOW_PIXEL_DOUBLE	0x00010000
-#define OMAPFB_CAPS_WINDOW_SCALE	0x00020000
-#define OMAPFB_CAPS_WINDOW_OVERLAY	0x00040000
-#define OMAPFB_CAPS_WINDOW_ROTATE	0x00080000
-#define OMAPFB_CAPS_SET_BACKLIGHT	0x01000000
-
-/* Values from DSP must map to lower 16-bits */
-#define OMAPFB_FORMAT_MASK		0x00ff
-#define OMAPFB_FORMAT_FLAG_DOUBLE	0x0100
-#define OMAPFB_FORMAT_FLAG_TEARSYNC	0x0200
-#define OMAPFB_FORMAT_FLAG_FORCE_VSYNC	0x0400
-#define OMAPFB_FORMAT_FLAG_ENABLE_OVERLAY	0x0800
-#define OMAPFB_FORMAT_FLAG_DISABLE_OVERLAY	0x1000
-
-#define OMAPFB_EVENT_READY	1
-#define OMAPFB_EVENT_DISABLED	2
-
-#define OMAPFB_MEMTYPE_SDRAM		0
-#define OMAPFB_MEMTYPE_SRAM		1
-#define OMAPFB_MEMTYPE_MAX		1
-
-enum omapfb_color_format {
-	OMAPFB_COLOR_RGB565 = 0,
-	OMAPFB_COLOR_YUV422,
-	OMAPFB_COLOR_YUV420,
-	OMAPFB_COLOR_CLUT_8BPP,
-	OMAPFB_COLOR_CLUT_4BPP,
-	OMAPFB_COLOR_CLUT_2BPP,
-	OMAPFB_COLOR_CLUT_1BPP,
-	OMAPFB_COLOR_RGB444,
-	OMAPFB_COLOR_YUY422,
-};
-
-struct omapfb_update_window {
-	__u32 x, y;
-	__u32 width, height;
-	__u32 format;
-	__u32 out_x, out_y;
-	__u32 out_width, out_height;
-	__u32 reserved[8];
-};
-
-struct omapfb_update_window_old {
-	__u32 x, y;
-	__u32 width, height;
-	__u32 format;
-};
-
-enum omapfb_plane {
-	OMAPFB_PLANE_GFX = 0,
-	OMAPFB_PLANE_VID1,
-	OMAPFB_PLANE_VID2,
-};
-
-enum omapfb_channel_out {
-	OMAPFB_CHANNEL_OUT_LCD = 0,
-	OMAPFB_CHANNEL_OUT_DIGIT,
-};
-
-struct omapfb_plane_info {
-	__u32 pos_x;
-	__u32 pos_y;
-	__u8  enabled;
-	__u8  channel_out;
-	__u8  mirror;
-	__u8  reserved1;
-	__u32 out_width;
-	__u32 out_height;
-	__u32 reserved2[12];
-};
-
-struct omapfb_mem_info {
-	__u32 size;
-	__u8  type;
-	__u8  reserved[3];
-};
-
-struct omapfb_caps {
-	__u32 ctrl;
-	__u32 plane_color;
-	__u32 wnd_color;
-};
-
-enum omapfb_color_key_type {
-	OMAPFB_COLOR_KEY_DISABLED = 0,
-	OMAPFB_COLOR_KEY_GFX_DST,
-	OMAPFB_COLOR_KEY_VID_SRC,
-};
-
-struct omapfb_color_key {
-	__u8  channel_out;
-	__u32 background;
-	__u32 trans_key;
-	__u8  key_type;
-};
-
-enum omapfb_update_mode {
-	OMAPFB_UPDATE_DISABLED = 0,
-	OMAPFB_AUTO_UPDATE,
-	OMAPFB_MANUAL_UPDATE
-};
-
-#ifdef __KERNEL__
-
-#include <linux/completion.h>
-#include <linux/interrupt.h>
-#include <linux/fb.h>
-#include <linux/mutex.h>
-
-#include <mach/board.h>
-
-#define OMAP_LCDC_INV_VSYNC             0x0001
-#define OMAP_LCDC_INV_HSYNC             0x0002
-#define OMAP_LCDC_INV_PIX_CLOCK         0x0004
-#define OMAP_LCDC_INV_OUTPUT_EN         0x0008
-#define OMAP_LCDC_HSVS_RISING_EDGE      0x0010
-#define OMAP_LCDC_HSVS_OPPOSITE         0x0020
-
-#define OMAP_LCDC_SIGNAL_MASK		0x003f
-
-#define OMAP_LCDC_PANEL_TFT		0x0100
-
-#define OMAPFB_PLANE_XRES_MIN		8
-#define OMAPFB_PLANE_YRES_MIN		8
-
-#ifdef CONFIG_ARCH_OMAP1
-#define OMAPFB_PLANE_NUM		1
-#else
-#define OMAPFB_PLANE_NUM		3
-#endif
-
-struct omapfb_device;
-
-struct lcd_panel {
-	const char	*name;
-	int		config;		/* TFT/STN, signal inversion */
-	int		bpp;		/* Pixel format in fb mem */
-	int		data_lines;	/* Lines on LCD HW interface */
-
-	int		x_res, y_res;
-	int		pixel_clock;	/* In kHz */
-	int		hsw;		/* Horizontal synchronization
-					   pulse width */
-	int		hfp;		/* Horizontal front porch */
-	int		hbp;		/* Horizontal back porch */
-	int		vsw;		/* Vertical synchronization
-					   pulse width */
-	int		vfp;		/* Vertical front porch */
-	int		vbp;		/* Vertical back porch */
-	int		acb;		/* ac-bias pin frequency */
-	int		pcd;		/* pixel clock divider.
-					   Obsolete use pixel_clock instead */
-
-	int		(*init)		(struct lcd_panel *panel,
-					 struct omapfb_device *fbdev);
-	void		(*cleanup)	(struct lcd_panel *panel);
-	int		(*enable)	(struct lcd_panel *panel);
-	void		(*disable)	(struct lcd_panel *panel);
-	unsigned long	(*get_caps)	(struct lcd_panel *panel);
-	int		(*set_bklight_level)(struct lcd_panel *panel,
-					     unsigned int level);
-	unsigned int	(*get_bklight_level)(struct lcd_panel *panel);
-	unsigned int	(*get_bklight_max)  (struct lcd_panel *panel);
-	int		(*run_test)	(struct lcd_panel *panel, int test_num);
-};
-
-struct extif_timings {
-	int cs_on_time;
-	int cs_off_time;
-	int we_on_time;
-	int we_off_time;
-	int re_on_time;
-	int re_off_time;
-	int we_cycle_time;
-	int re_cycle_time;
-	int cs_pulse_width;
-	int access_time;
-
-	int clk_div;
-
-	u32 tim[5];		/* set by extif->convert_timings */
-
-	int converted;
-};
-
-struct lcd_ctrl_extif {
-	int  (*init)		(struct omapfb_device *fbdev);
-	void (*cleanup)		(void);
-	void (*get_clk_info)	(u32 *clk_period, u32 *max_clk_div);
-	unsigned long (*get_max_tx_rate)(void);
-	int  (*convert_timings)	(struct extif_timings *timings);
-	void (*set_timings)	(const struct extif_timings *timings);
-	void (*set_bits_per_cycle)(int bpc);
-	void (*write_command)	(const void *buf, unsigned int len);
-	void (*read_data)	(void *buf, unsigned int len);
-	void (*write_data)	(const void *buf, unsigned int len);
-	void (*transfer_area)	(int width, int height,
-				 void (callback)(void * data), void *data);
-	int  (*setup_tearsync)	(unsigned pin_cnt,
-				 unsigned hs_pulse_time, unsigned vs_pulse_time,
-				 int hs_pol_inv, int vs_pol_inv, int div);
-	int  (*enable_tearsync) (int enable, unsigned line);
-
-	unsigned long		max_transmit_size;
-};
-
-struct omapfb_notifier_block {
-	struct notifier_block	nb;
-	void			*data;
-	int			plane_idx;
-};
-
-typedef int (*omapfb_notifier_callback_t)(struct notifier_block *,
-					  unsigned long event,
-					  void *fbi);
-
-struct omapfb_mem_region {
-	u32		paddr;
-	void __iomem	*vaddr;
-	unsigned long	size;
-	u8		type;		/* OMAPFB_PLANE_MEM_* */
-	unsigned	alloc:1;	/* allocated by the driver */
-	unsigned	map:1;		/* kernel mapped by the driver */
-};
-
-struct omapfb_mem_desc {
-	int				region_cnt;
-	struct omapfb_mem_region	region[OMAPFB_PLANE_NUM];
-};
-
-struct lcd_ctrl {
-	const char	*name;
-	void		*data;
-
-	int		(*init)		  (struct omapfb_device *fbdev,
-					   int ext_mode,
-					   struct omapfb_mem_desc *req_md);
-	void		(*cleanup)	  (void);
-	void		(*bind_client)	  (struct omapfb_notifier_block *nb);
-	void		(*get_caps)	  (int plane, struct omapfb_caps *caps);
-	int		(*set_update_mode)(enum omapfb_update_mode mode);
-	enum omapfb_update_mode (*get_update_mode)(void);
-	int		(*setup_plane)	  (int plane, int channel_out,
-					   unsigned long offset,
-					   int screen_width,
-					   int pos_x, int pos_y, int width,
-					   int height, int color_mode);
-	int		(*set_rotate)	  (int angle);
-	int		(*setup_mem)	  (int plane, size_t size,
-					   int mem_type, unsigned long *paddr);
-	int		(*mmap)		  (struct fb_info *info,
-					   struct vm_area_struct *vma);
-	int		(*set_scale)	  (int plane,
-					   int orig_width, int orig_height,
-					   int out_width, int out_height);
-	int		(*enable_plane)	  (int plane, int enable);
-	int		(*update_window)  (struct fb_info *fbi,
-					   struct omapfb_update_window *win,
-					   void (*callback)(void *),
-					   void *callback_data);
-	void		(*sync)		  (void);
-	void		(*suspend)	  (void);
-	void		(*resume)	  (void);
-	int		(*run_test)	  (int test_num);
-	int		(*setcolreg)	  (u_int regno, u16 red, u16 green,
-					   u16 blue, u16 transp,
-					   int update_hw_mem);
-	int		(*set_color_key)  (struct omapfb_color_key *ck);
-	int		(*get_color_key)  (struct omapfb_color_key *ck);
-};
-
-enum omapfb_state {
-	OMAPFB_DISABLED	= 0,
-	OMAPFB_SUSPENDED= 99,
-	OMAPFB_ACTIVE	= 100
-};
-
-struct omapfb_plane_struct {
-	int				idx;
-	struct omapfb_plane_info	info;
-	enum omapfb_color_format	color_mode;
-	struct omapfb_device		*fbdev;
-};
-
-struct omapfb_device {
-	int			state;
-	int                     ext_lcdc;               /* Using external
-                                                           LCD controller */
-	struct mutex		rqueue_mutex;
-
-	int			palette_size;
-	u32			pseudo_palette[17];
-
-	struct lcd_panel	*panel;			/* LCD panel */
-	const struct lcd_ctrl	*ctrl;			/* LCD controller */
-	const struct lcd_ctrl	*int_ctrl;		/* internal LCD ctrl */
-	struct lcd_ctrl_extif	*ext_if;		/* LCD ctrl external
-							   interface */
-	struct device		*dev;
-	struct fb_var_screeninfo	new_var;	/* for mode changes */
-
-	struct omapfb_mem_desc		mem_desc;
-	struct fb_info			*fb_info[OMAPFB_PLANE_NUM];
-};
-
-struct omapfb_platform_data {
-	struct omap_lcd_config		lcd;
-	struct omapfb_mem_desc		mem_desc;
-	void				*ctrl_platform_data;
-};
-
-#ifdef CONFIG_ARCH_OMAP1
-extern struct lcd_ctrl omap1_lcd_ctrl;
-#else
-extern struct lcd_ctrl omap2_disp_ctrl;
-#endif
-
-extern void omapfb_reserve_sdram(void);
-extern void omapfb_register_panel(struct lcd_panel *panel);
-extern void omapfb_write_first_pixel(struct omapfb_device *fbdev, u16 pixval);
-extern void omapfb_notify_clients(struct omapfb_device *fbdev,
-				  unsigned long event);
-extern int  omapfb_register_client(struct omapfb_notifier_block *nb,
-				   omapfb_notifier_callback_t callback,
-				   void *callback_data);
-extern int  omapfb_unregister_client(struct omapfb_notifier_block *nb);
-extern int  omapfb_update_window_async(struct fb_info *fbi,
-				       struct omapfb_update_window *win,
-				       void (*callback)(void *),
-				       void *callback_data);
-
-/* in arch/arm/plat-omap/fb.c */
-extern void omapfb_set_ctrl_platform_data(void *pdata);
-
-#endif /* __KERNEL__ */
-
-#endif /* __OMAPFB_H */
diff --git a/drivers/video/omap/blizzard.c b/drivers/video/omap/blizzard.c
index f60a233..8121c09 100644
--- a/drivers/video/omap/blizzard.c
+++ b/drivers/video/omap/blizzard.c
@@ -25,9 +25,9 @@
 #include <linux/fb.h>
 #include <linux/delay.h>
 #include <linux/clk.h>
+#include <linux/omapfb.h>
 
 #include <mach/dma.h>
-#include <mach/omapfb.h>
 #include <mach/blizzard.h>
 
 #include "dispc.h"
diff --git a/drivers/video/omap/dispc.c b/drivers/video/omap/dispc.c
index c140c21..1915af5 100644
--- a/drivers/video/omap/dispc.c
+++ b/drivers/video/omap/dispc.c
@@ -24,9 +24,9 @@
 #include <linux/vmalloc.h>
 #include <linux/clk.h>
 #include <linux/io.h>
+#include <linux/omapfb.h>
 
 #include <mach/sram.h>
-#include <mach/omapfb.h>
 #include <mach/board.h>
 
 #include "dispc.h"
diff --git a/drivers/video/omap/hwa742.c b/drivers/video/omap/hwa742.c
index f24df0b..9b4c506 100644
--- a/drivers/video/omap/hwa742.c
+++ b/drivers/video/omap/hwa742.c
@@ -25,9 +25,9 @@
 #include <linux/fb.h>
 #include <linux/delay.h>
 #include <linux/clk.h>
+#include <linux/omapfb.h>
 
 #include <mach/dma.h>
-#include <mach/omapfb.h>
 #include <mach/hwa742.h>
 
 #define HWA742_REV_CODE_REG       0x0
diff --git a/drivers/video/omap/lcd_2430sdp.c b/drivers/video/omap/lcd_2430sdp.c
index a22b452..1252cc3 100644
--- a/drivers/video/omap/lcd_2430sdp.c
+++ b/drivers/video/omap/lcd_2430sdp.c
@@ -26,9 +26,9 @@
 #include <linux/delay.h>
 #include <linux/gpio.h>
 #include <linux/i2c/twl4030.h>
+#include <linux/omapfb.h>
 
 #include <mach/mux.h>
-#include <mach/omapfb.h>
 #include <asm/mach-types.h>
 
 #define SDP2430_LCD_PANEL_BACKLIGHT_GPIO	91
diff --git a/drivers/video/omap/lcd_ams_delta.c b/drivers/video/omap/lcd_ams_delta.c
index 3fd5342..4d54725 100644
--- a/drivers/video/omap/lcd_ams_delta.c
+++ b/drivers/video/omap/lcd_ams_delta.c
@@ -24,13 +24,13 @@
 
 #include <linux/module.h>
 #include <linux/platform_device.h>
+#include <linux/omapfb.h>
 
 #include <asm/delay.h>
 #include <asm/io.h>
 
 #include <mach/board-ams-delta.h>
 #include <mach/hardware.h>
-#include <mach/omapfb.h>
 
 #define AMS_DELTA_DEFAULT_CONTRAST	112
 
diff --git a/drivers/video/omap/lcd_apollon.c b/drivers/video/omap/lcd_apollon.c
index beae5d9..e3b2224 100644
--- a/drivers/video/omap/lcd_apollon.c
+++ b/drivers/video/omap/lcd_apollon.c
@@ -23,10 +23,10 @@
 
 #include <linux/module.h>
 #include <linux/platform_device.h>
+#include <linux/omapfb.h>
 
 #include <mach/gpio.h>
 #include <mach/mux.h>
-#include <mach/omapfb.h>
 
 /* #define USE_35INCH_LCD 1 */
 
diff --git a/drivers/video/omap/lcd_h3.c b/drivers/video/omap/lcd_h3.c
index 2486237..f7264ea 100644
--- a/drivers/video/omap/lcd_h3.c
+++ b/drivers/video/omap/lcd_h3.c
@@ -22,9 +22,9 @@
 #include <linux/module.h>
 #include <linux/platform_device.h>
 #include <linux/i2c/tps65010.h>
+#include <linux/omapfb.h>
 
 #include <mach/gpio.h>
-#include <mach/omapfb.h>
 
 #define MODULE_NAME	"omapfb-lcd_h3"
 
diff --git a/drivers/video/omap/lcd_h4.c b/drivers/video/omap/lcd_h4.c
index 6ff5643..d72df0c 100644
--- a/drivers/video/omap/lcd_h4.c
+++ b/drivers/video/omap/lcd_h4.c
@@ -21,8 +21,7 @@
 
 #include <linux/module.h>
 #include <linux/platform_device.h>
-
-#include <mach/omapfb.h>
+#include <linux/omapfb.h>
 
 static int h4_panel_init(struct lcd_panel *panel, struct omapfb_device *fbdev)
 {
diff --git a/drivers/video/omap/lcd_inn1510.c b/drivers/video/omap/lcd_inn1510.c
index 6953ed4..f6e05d7 100644
--- a/drivers/video/omap/lcd_inn1510.c
+++ b/drivers/video/omap/lcd_inn1510.c
@@ -22,9 +22,9 @@
 #include <linux/module.h>
 #include <linux/platform_device.h>
 #include <linux/io.h>
+#include <linux/omapfb.h>
 
 #include <mach/fpga.h>
-#include <mach/omapfb.h>
 
 static int innovator1510_panel_init(struct lcd_panel *panel,
 				    struct omapfb_device *fbdev)
diff --git a/drivers/video/omap/lcd_inn1610.c b/drivers/video/omap/lcd_inn1610.c
index 4c4f7ee..c599e41 100644
--- a/drivers/video/omap/lcd_inn1610.c
+++ b/drivers/video/omap/lcd_inn1610.c
@@ -21,9 +21,9 @@
 
 #include <linux/module.h>
 #include <linux/platform_device.h>
+#include <linux/omapfb.h>
 
 #include <mach/gpio.h>
-#include <mach/omapfb.h>
 
 #define MODULE_NAME	"omapfb-lcd_h3"
 
diff --git a/drivers/video/omap/lcd_ldp.c b/drivers/video/omap/lcd_ldp.c
index 8925230..1c25186 100644
--- a/drivers/video/omap/lcd_ldp.c
+++ b/drivers/video/omap/lcd_ldp.c
@@ -25,10 +25,10 @@
 #include <linux/platform_device.h>
 #include <linux/delay.h>
 #include <linux/i2c/twl4030.h>
+#include <linux/omapfb.h>
 
 #include <mach/gpio.h>
 #include <mach/mux.h>
-#include <mach/omapfb.h>
 #include <asm/mach-types.h>
 
 #define LCD_PANEL_BACKLIGHT_GPIO 	(15 + OMAP_MAX_GPIO_LINES)
diff --git a/drivers/video/omap/lcd_mipid.c b/drivers/video/omap/lcd_mipid.c
index 1895997..4b28005 100644
--- a/drivers/video/omap/lcd_mipid.c
+++ b/drivers/video/omap/lcd_mipid.c
@@ -22,8 +22,8 @@
 #include <linux/delay.h>
 #include <linux/workqueue.h>
 #include <linux/spi/spi.h>
+#include <linux/omapfb.h>
 
-#include <mach/omapfb.h>
 #include <mach/lcd_mipid.h>
 
 #include "../../cbus/tahvo.h"
diff --git a/drivers/video/omap/lcd_omap2evm.c b/drivers/video/omap/lcd_omap2evm.c
index 2fc46c2..1908a2b 100644
--- a/drivers/video/omap/lcd_omap2evm.c
+++ b/drivers/video/omap/lcd_omap2evm.c
@@ -25,9 +25,9 @@
 #include <linux/platform_device.h>
 #include <linux/gpio.h>
 #include <linux/i2c/twl4030.h>
+#include <linux/omapfb.h>
 
 #include <mach/mux.h>
-#include <mach/omapfb.h>
 #include <asm/mach-types.h>
 
 #define LCD_PANEL_ENABLE_GPIO	154
diff --git a/drivers/video/omap/lcd_omap3beagle.c b/drivers/video/omap/lcd_omap3beagle.c
index eae43e4..6be117e 100644
--- a/drivers/video/omap/lcd_omap3beagle.c
+++ b/drivers/video/omap/lcd_omap3beagle.c
@@ -24,9 +24,9 @@
 #include <linux/platform_device.h>
 #include <linux/gpio.h>
 #include <linux/i2c/twl4030.h>
+#include <linux/omapfb.h>
 
 #include <mach/mux.h>
-#include <mach/omapfb.h>
 #include <asm/mach-types.h>
 
 #define LCD_PANEL_ENABLE_GPIO       170
diff --git a/drivers/video/omap/lcd_omap3evm.c b/drivers/video/omap/lcd_omap3evm.c
index 1c3d814..10ba48c 100644
--- a/drivers/video/omap/lcd_omap3evm.c
+++ b/drivers/video/omap/lcd_omap3evm.c
@@ -24,9 +24,9 @@
 #include <linux/platform_device.h>
 #include <linux/gpio.h>
 #include <linux/i2c/twl4030.h>
+#include <linux/omapfb.h>
 
 #include <mach/mux.h>
-#include <mach/omapfb.h>
 #include <asm/mach-types.h>
 
 #define LCD_PANEL_ENABLE_GPIO       153
diff --git a/drivers/video/omap/lcd_osk.c b/drivers/video/omap/lcd_osk.c
index 379c96d..d6b193e 100644
--- a/drivers/video/omap/lcd_osk.c
+++ b/drivers/video/omap/lcd_osk.c
@@ -22,10 +22,10 @@
 
 #include <linux/module.h>
 #include <linux/platform_device.h>
+#include <linux/omapfb.h>
 
 #include <mach/gpio.h>
 #include <mach/mux.h>
-#include <mach/omapfb.h>
 
 static int osk_panel_init(struct lcd_panel *panel, struct omapfb_device *fbdev)
 {
diff --git a/drivers/video/omap/lcd_overo.c b/drivers/video/omap/lcd_overo.c
index 2bc5c92..40c2026 100644
--- a/drivers/video/omap/lcd_overo.c
+++ b/drivers/video/omap/lcd_overo.c
@@ -22,10 +22,10 @@
 #include <linux/module.h>
 #include <linux/platform_device.h>
 #include <linux/i2c/twl4030.h>
+#include <linux/omapfb.h>
 
 #include <mach/gpio.h>
 #include <mach/mux.h>
-#include <mach/omapfb.h>
 #include <asm/mach-types.h>
 
 #define LCD_ENABLE       144
diff --git a/drivers/video/omap/lcd_p2.c b/drivers/video/omap/lcd_p2.c
index dd40fd7..bc5abef 100644
--- a/drivers/video/omap/lcd_p2.c
+++ b/drivers/video/omap/lcd_p2.c
@@ -24,10 +24,10 @@
 #include <linux/module.h>
 #include <linux/delay.h>
 #include <linux/platform_device.h>
+#include <linux/omapfb.h>
 
 #include <mach/mux.h>
 #include <mach/gpio.h>
-#include <mach/omapfb.h>
 
 /*
  * File: epson-md-tft.h
diff --git a/drivers/video/omap/lcd_palmte.c b/drivers/video/omap/lcd_palmte.c
index 2183173..dcb456c 100644
--- a/drivers/video/omap/lcd_palmte.c
+++ b/drivers/video/omap/lcd_palmte.c
@@ -22,9 +22,9 @@
 #include <linux/module.h>
 #include <linux/platform_device.h>
 #include <linux/io.h>
+#include <linux/omapfb.h>
 
 #include <mach/fpga.h>
-#include <mach/omapfb.h>
 
 static int palmte_panel_init(struct lcd_panel *panel,
 				struct omapfb_device *fbdev)
diff --git a/drivers/video/omap/lcd_palmtt.c b/drivers/video/omap/lcd_palmtt.c
index 57b0f6c..e8adab8 100644
--- a/drivers/video/omap/lcd_palmtt.c
+++ b/drivers/video/omap/lcd_palmtt.c
@@ -28,9 +28,9 @@ GPIO13 - screen blanking
 #include <linux/platform_device.h>
 #include <linux/module.h>
 #include <linux/io.h>
+#include <linux/omapfb.h>
 
 #include <mach/gpio.h>
-#include <mach/omapfb.h>
 
 static int palmtt_panel_init(struct lcd_panel *panel,
 	struct omapfb_device *fbdev)
diff --git a/drivers/video/omap/lcd_palmz71.c b/drivers/video/omap/lcd_palmz71.c
index d33d78b..d5b3f82 100644
--- a/drivers/video/omap/lcd_palmz71.c
+++ b/drivers/video/omap/lcd_palmz71.c
@@ -23,8 +23,7 @@
 #include <linux/module.h>
 #include <linux/platform_device.h>
 #include <linux/io.h>
-
-#include <mach/omapfb.h>
+#include <linux/omapfb.h>
 
 static int palmz71_panel_init(struct lcd_panel *panel,
 			      struct omapfb_device *fbdev)
diff --git a/drivers/video/omap/lcdc.c b/drivers/video/omap/lcdc.c
index ab39492..633e33c 100644
--- a/drivers/video/omap/lcdc.c
+++ b/drivers/video/omap/lcdc.c
@@ -28,9 +28,9 @@
 #include <linux/dma-mapping.h>
 #include <linux/vmalloc.h>
 #include <linux/clk.h>
+#include <linux/omapfb.h>
 
 #include <mach/dma.h>
-#include <mach/omapfb.h>
 
 #include <asm/mach-types.h>
 
diff --git a/drivers/video/omap/omapfb_main.c b/drivers/video/omap/omapfb_main.c
index 3bb4247..c6306af 100644
--- a/drivers/video/omap/omapfb_main.c
+++ b/drivers/video/omap/omapfb_main.c
@@ -27,9 +27,9 @@
 #include <linux/platform_device.h>
 #include <linux/mm.h>
 #include <linux/uaccess.h>
+#include <linux/omapfb.h>
 
 #include <mach/dma.h>
-#include <mach/omapfb.h>
 
 #include "lcdc.h"
 #include "dispc.h"
diff --git a/drivers/video/omap/rfbi.c b/drivers/video/omap/rfbi.c
index 29fa368..118cfa9 100644
--- a/drivers/video/omap/rfbi.c
+++ b/drivers/video/omap/rfbi.c
@@ -26,8 +26,7 @@
 #include <linux/interrupt.h>
 #include <linux/clk.h>
 #include <linux/io.h>
-
-#include <mach/omapfb.h>
+#include <linux/omapfb.h>
 
 #include "dispc.h"
 
diff --git a/drivers/video/omap/sossi.c b/drivers/video/omap/sossi.c
index cc697cc..ff9dd71 100644
--- a/drivers/video/omap/sossi.c
+++ b/drivers/video/omap/sossi.c
@@ -23,9 +23,9 @@
 #include <linux/clk.h>
 #include <linux/irq.h>
 #include <linux/io.h>
+#include <linux/omapfb.h>
 
 #include <mach/dma.h>
-#include <mach/omapfb.h>
 
 #include "lcdc.h"
 
diff --git a/include/linux/omapfb.h b/include/linux/omapfb.h
new file mode 100644
index 0000000..b226bdf
--- /dev/null
+++ b/include/linux/omapfb.h
@@ -0,0 +1,398 @@
+/*
+ * File: arch/arm/plat-omap/include/mach/omapfb.h
+ *
+ * Framebuffer driver for TI OMAP boards
+ *
+ * Copyright (C) 2004 Nokia Corporation
+ * Author: Imre Deak <imre.deak@nokia.com>
+ *
+ * This program is free software; you can redistribute it and/or modify it
+ * under the terms of the GNU General Public License as published by the
+ * Free Software Foundation; either version 2 of the License, or (at your
+ * option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful, but
+ * WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU
+ * General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License along
+ * with this program; if not, write to the Free Software Foundation, Inc.,
+ * 59 Temple Place - Suite 330, Boston, MA  02111-1307, USA.
+ */
+
+#ifndef __OMAPFB_H
+#define __OMAPFB_H
+
+#include <asm/ioctl.h>
+#include <asm/types.h>
+
+/* IOCTL commands. */
+
+#define OMAP_IOW(num, dtype)	_IOW('O', num, dtype)
+#define OMAP_IOR(num, dtype)	_IOR('O', num, dtype)
+#define OMAP_IOWR(num, dtype)	_IOWR('O', num, dtype)
+#define OMAP_IO(num)		_IO('O', num)
+
+#define OMAPFB_MIRROR		OMAP_IOW(31, int)
+#define OMAPFB_SYNC_GFX		OMAP_IO(37)
+#define OMAPFB_VSYNC		OMAP_IO(38)
+#define OMAPFB_SET_UPDATE_MODE	OMAP_IOW(40, int)
+#define OMAPFB_GET_CAPS		OMAP_IOR(42, struct omapfb_caps)
+#define OMAPFB_GET_UPDATE_MODE	OMAP_IOW(43, int)
+#define OMAPFB_LCD_TEST		OMAP_IOW(45, int)
+#define OMAPFB_CTRL_TEST	OMAP_IOW(46, int)
+#define OMAPFB_UPDATE_WINDOW_OLD OMAP_IOW(47, struct omapfb_update_window_old)
+#define OMAPFB_SET_COLOR_KEY	OMAP_IOW(50, struct omapfb_color_key)
+#define OMAPFB_GET_COLOR_KEY	OMAP_IOW(51, struct omapfb_color_key)
+#define OMAPFB_SETUP_PLANE	OMAP_IOW(52, struct omapfb_plane_info)
+#define OMAPFB_QUERY_PLANE	OMAP_IOW(53, struct omapfb_plane_info)
+#define OMAPFB_UPDATE_WINDOW	OMAP_IOW(54, struct omapfb_update_window)
+#define OMAPFB_SETUP_MEM	OMAP_IOW(55, struct omapfb_mem_info)
+#define OMAPFB_QUERY_MEM	OMAP_IOW(56, struct omapfb_mem_info)
+
+#define OMAPFB_CAPS_GENERIC_MASK	0x00000fff
+#define OMAPFB_CAPS_LCDC_MASK		0x00fff000
+#define OMAPFB_CAPS_PANEL_MASK		0xff000000
+
+#define OMAPFB_CAPS_MANUAL_UPDATE	0x00001000
+#define OMAPFB_CAPS_TEARSYNC		0x00002000
+#define OMAPFB_CAPS_PLANE_RELOCATE_MEM	0x00004000
+#define OMAPFB_CAPS_PLANE_SCALE		0x00008000
+#define OMAPFB_CAPS_WINDOW_PIXEL_DOUBLE	0x00010000
+#define OMAPFB_CAPS_WINDOW_SCALE	0x00020000
+#define OMAPFB_CAPS_WINDOW_OVERLAY	0x00040000
+#define OMAPFB_CAPS_WINDOW_ROTATE	0x00080000
+#define OMAPFB_CAPS_SET_BACKLIGHT	0x01000000
+
+/* Values from DSP must map to lower 16-bits */
+#define OMAPFB_FORMAT_MASK		0x00ff
+#define OMAPFB_FORMAT_FLAG_DOUBLE	0x0100
+#define OMAPFB_FORMAT_FLAG_TEARSYNC	0x0200
+#define OMAPFB_FORMAT_FLAG_FORCE_VSYNC	0x0400
+#define OMAPFB_FORMAT_FLAG_ENABLE_OVERLAY	0x0800
+#define OMAPFB_FORMAT_FLAG_DISABLE_OVERLAY	0x1000
+
+#define OMAPFB_EVENT_READY	1
+#define OMAPFB_EVENT_DISABLED	2
+
+#define OMAPFB_MEMTYPE_SDRAM		0
+#define OMAPFB_MEMTYPE_SRAM		1
+#define OMAPFB_MEMTYPE_MAX		1
+
+enum omapfb_color_format {
+	OMAPFB_COLOR_RGB565 = 0,
+	OMAPFB_COLOR_YUV422,
+	OMAPFB_COLOR_YUV420,
+	OMAPFB_COLOR_CLUT_8BPP,
+	OMAPFB_COLOR_CLUT_4BPP,
+	OMAPFB_COLOR_CLUT_2BPP,
+	OMAPFB_COLOR_CLUT_1BPP,
+	OMAPFB_COLOR_RGB444,
+	OMAPFB_COLOR_YUY422,
+};
+
+struct omapfb_update_window {
+	__u32 x, y;
+	__u32 width, height;
+	__u32 format;
+	__u32 out_x, out_y;
+	__u32 out_width, out_height;
+	__u32 reserved[8];
+};
+
+struct omapfb_update_window_old {
+	__u32 x, y;
+	__u32 width, height;
+	__u32 format;
+};
+
+enum omapfb_plane {
+	OMAPFB_PLANE_GFX = 0,
+	OMAPFB_PLANE_VID1,
+	OMAPFB_PLANE_VID2,
+};
+
+enum omapfb_channel_out {
+	OMAPFB_CHANNEL_OUT_LCD = 0,
+	OMAPFB_CHANNEL_OUT_DIGIT,
+};
+
+struct omapfb_plane_info {
+	__u32 pos_x;
+	__u32 pos_y;
+	__u8  enabled;
+	__u8  channel_out;
+	__u8  mirror;
+	__u8  reserved1;
+	__u32 out_width;
+	__u32 out_height;
+	__u32 reserved2[12];
+};
+
+struct omapfb_mem_info {
+	__u32 size;
+	__u8  type;
+	__u8  reserved[3];
+};
+
+struct omapfb_caps {
+	__u32 ctrl;
+	__u32 plane_color;
+	__u32 wnd_color;
+};
+
+enum omapfb_color_key_type {
+	OMAPFB_COLOR_KEY_DISABLED = 0,
+	OMAPFB_COLOR_KEY_GFX_DST,
+	OMAPFB_COLOR_KEY_VID_SRC,
+};
+
+struct omapfb_color_key {
+	__u8  channel_out;
+	__u32 background;
+	__u32 trans_key;
+	__u8  key_type;
+};
+
+enum omapfb_update_mode {
+	OMAPFB_UPDATE_DISABLED = 0,
+	OMAPFB_AUTO_UPDATE,
+	OMAPFB_MANUAL_UPDATE
+};
+
+#ifdef __KERNEL__
+
+#include <linux/completion.h>
+#include <linux/interrupt.h>
+#include <linux/fb.h>
+#include <linux/mutex.h>
+
+#include <mach/board.h>
+
+#define OMAP_LCDC_INV_VSYNC             0x0001
+#define OMAP_LCDC_INV_HSYNC             0x0002
+#define OMAP_LCDC_INV_PIX_CLOCK         0x0004
+#define OMAP_LCDC_INV_OUTPUT_EN         0x0008
+#define OMAP_LCDC_HSVS_RISING_EDGE      0x0010
+#define OMAP_LCDC_HSVS_OPPOSITE         0x0020
+
+#define OMAP_LCDC_SIGNAL_MASK		0x003f
+
+#define OMAP_LCDC_PANEL_TFT		0x0100
+
+#define OMAPFB_PLANE_XRES_MIN		8
+#define OMAPFB_PLANE_YRES_MIN		8
+
+#ifdef CONFIG_ARCH_OMAP1
+#define OMAPFB_PLANE_NUM		1
+#else
+#define OMAPFB_PLANE_NUM		3
+#endif
+
+struct omapfb_device;
+
+struct lcd_panel {
+	const char	*name;
+	int		config;		/* TFT/STN, signal inversion */
+	int		bpp;		/* Pixel format in fb mem */
+	int		data_lines;	/* Lines on LCD HW interface */
+
+	int		x_res, y_res;
+	int		pixel_clock;	/* In kHz */
+	int		hsw;		/* Horizontal synchronization
+					   pulse width */
+	int		hfp;		/* Horizontal front porch */
+	int		hbp;		/* Horizontal back porch */
+	int		vsw;		/* Vertical synchronization
+					   pulse width */
+	int		vfp;		/* Vertical front porch */
+	int		vbp;		/* Vertical back porch */
+	int		acb;		/* ac-bias pin frequency */
+	int		pcd;		/* pixel clock divider.
+					   Obsolete use pixel_clock instead */
+
+	int		(*init)		(struct lcd_panel *panel,
+					 struct omapfb_device *fbdev);
+	void		(*cleanup)	(struct lcd_panel *panel);
+	int		(*enable)	(struct lcd_panel *panel);
+	void		(*disable)	(struct lcd_panel *panel);
+	unsigned long	(*get_caps)	(struct lcd_panel *panel);
+	int		(*set_bklight_level)(struct lcd_panel *panel,
+					     unsigned int level);
+	unsigned int	(*get_bklight_level)(struct lcd_panel *panel);
+	unsigned int	(*get_bklight_max)  (struct lcd_panel *panel);
+	int		(*run_test)	(struct lcd_panel *panel, int test_num);
+};
+
+struct extif_timings {
+	int cs_on_time;
+	int cs_off_time;
+	int we_on_time;
+	int we_off_time;
+	int re_on_time;
+	int re_off_time;
+	int we_cycle_time;
+	int re_cycle_time;
+	int cs_pulse_width;
+	int access_time;
+
+	int clk_div;
+
+	u32 tim[5];		/* set by extif->convert_timings */
+
+	int converted;
+};
+
+struct lcd_ctrl_extif {
+	int  (*init)		(struct omapfb_device *fbdev);
+	void (*cleanup)		(void);
+	void (*get_clk_info)	(u32 *clk_period, u32 *max_clk_div);
+	unsigned long (*get_max_tx_rate)(void);
+	int  (*convert_timings)	(struct extif_timings *timings);
+	void (*set_timings)	(const struct extif_timings *timings);
+	void (*set_bits_per_cycle)(int bpc);
+	void (*write_command)	(const void *buf, unsigned int len);
+	void (*read_data)	(void *buf, unsigned int len);
+	void (*write_data)	(const void *buf, unsigned int len);
+	void (*transfer_area)	(int width, int height,
+				 void (callback)(void * data), void *data);
+	int  (*setup_tearsync)	(unsigned pin_cnt,
+				 unsigned hs_pulse_time, unsigned vs_pulse_time,
+				 int hs_pol_inv, int vs_pol_inv, int div);
+	int  (*enable_tearsync) (int enable, unsigned line);
+
+	unsigned long		max_transmit_size;
+};
+
+struct omapfb_notifier_block {
+	struct notifier_block	nb;
+	void			*data;
+	int			plane_idx;
+};
+
+typedef int (*omapfb_notifier_callback_t)(struct notifier_block *,
+					  unsigned long event,
+					  void *fbi);
+
+struct omapfb_mem_region {
+	u32		paddr;
+	void __iomem	*vaddr;
+	unsigned long	size;
+	u8		type;		/* OMAPFB_PLANE_MEM_* */
+	unsigned	alloc:1;	/* allocated by the driver */
+	unsigned	map:1;		/* kernel mapped by the driver */
+};
+
+struct omapfb_mem_desc {
+	int				region_cnt;
+	struct omapfb_mem_region	region[OMAPFB_PLANE_NUM];
+};
+
+struct lcd_ctrl {
+	const char	*name;
+	void		*data;
+
+	int		(*init)		  (struct omapfb_device *fbdev,
+					   int ext_mode,
+					   struct omapfb_mem_desc *req_md);
+	void		(*cleanup)	  (void);
+	void		(*bind_client)	  (struct omapfb_notifier_block *nb);
+	void		(*get_caps)	  (int plane, struct omapfb_caps *caps);
+	int		(*set_update_mode)(enum omapfb_update_mode mode);
+	enum omapfb_update_mode (*get_update_mode)(void);
+	int		(*setup_plane)	  (int plane, int channel_out,
+					   unsigned long offset,
+					   int screen_width,
+					   int pos_x, int pos_y, int width,
+					   int height, int color_mode);
+	int		(*set_rotate)	  (int angle);
+	int		(*setup_mem)	  (int plane, size_t size,
+					   int mem_type, unsigned long *paddr);
+	int		(*mmap)		  (struct fb_info *info,
+					   struct vm_area_struct *vma);
+	int		(*set_scale)	  (int plane,
+					   int orig_width, int orig_height,
+					   int out_width, int out_height);
+	int		(*enable_plane)	  (int plane, int enable);
+	int		(*update_window)  (struct fb_info *fbi,
+					   struct omapfb_update_window *win,
+					   void (*callback)(void *),
+					   void *callback_data);
+	void		(*sync)		  (void);
+	void		(*suspend)	  (void);
+	void		(*resume)	  (void);
+	int		(*run_test)	  (int test_num);
+	int		(*setcolreg)	  (u_int regno, u16 red, u16 green,
+					   u16 blue, u16 transp,
+					   int update_hw_mem);
+	int		(*set_color_key)  (struct omapfb_color_key *ck);
+	int		(*get_color_key)  (struct omapfb_color_key *ck);
+};
+
+enum omapfb_state {
+	OMAPFB_DISABLED	= 0,
+	OMAPFB_SUSPENDED= 99,
+	OMAPFB_ACTIVE	= 100
+};
+
+struct omapfb_plane_struct {
+	int				idx;
+	struct omapfb_plane_info	info;
+	enum omapfb_color_format	color_mode;
+	struct omapfb_device		*fbdev;
+};
+
+struct omapfb_device {
+	int			state;
+	int                     ext_lcdc;               /* Using external
+                                                           LCD controller */
+	struct mutex		rqueue_mutex;
+
+	int			palette_size;
+	u32			pseudo_palette[17];
+
+	struct lcd_panel	*panel;			/* LCD panel */
+	const struct lcd_ctrl	*ctrl;			/* LCD controller */
+	const struct lcd_ctrl	*int_ctrl;		/* internal LCD ctrl */
+	struct lcd_ctrl_extif	*ext_if;		/* LCD ctrl external
+							   interface */
+	struct device		*dev;
+	struct fb_var_screeninfo	new_var;	/* for mode changes */
+
+	struct omapfb_mem_desc		mem_desc;
+	struct fb_info			*fb_info[OMAPFB_PLANE_NUM];
+};
+
+struct omapfb_platform_data {
+	struct omap_lcd_config		lcd;
+	struct omapfb_mem_desc		mem_desc;
+	void				*ctrl_platform_data;
+};
+
+#ifdef CONFIG_ARCH_OMAP1
+extern struct lcd_ctrl omap1_lcd_ctrl;
+#else
+extern struct lcd_ctrl omap2_disp_ctrl;
+#endif
+
+extern void omapfb_reserve_sdram(void);
+extern void omapfb_register_panel(struct lcd_panel *panel);
+extern void omapfb_write_first_pixel(struct omapfb_device *fbdev, u16 pixval);
+extern void omapfb_notify_clients(struct omapfb_device *fbdev,
+				  unsigned long event);
+extern int  omapfb_register_client(struct omapfb_notifier_block *nb,
+				   omapfb_notifier_callback_t callback,
+				   void *callback_data);
+extern int  omapfb_unregister_client(struct omapfb_notifier_block *nb);
+extern int  omapfb_update_window_async(struct fb_info *fbi,
+				       struct omapfb_update_window *win,
+				       void (*callback)(void *),
+				       void *callback_data);
+
+/* in arch/arm/plat-omap/fb.c */
+extern void omapfb_set_ctrl_platform_data(void *pdata);
+
+#endif /* __KERNEL__ */
+
+#endif /* __OMAPFB_H */
-- 
1.5.6.5

