From f9ca8154cf395ec00129f12016697ef610a826ff Mon Sep 17 00:00:00 2001
From: Sergei Shtylyov <sshtylyov-hkdhdckH98+B+jHODAdFcQ@public.gmane.org>
Date: Fri, 27 Mar 2009 12:55:16 -0700
Subject: [PATCH] musb_host: factor out musb_ep_{get|set}_qh()

Factor out the often used code to get/set the active 'qh'
pointer for the hardware endpoint.  Change the way the case
of a shared FIFO is handled by setting *both* 'in_qh' and
'out_qh' fields of 'struct musb_hw_ep'.  That seems more
consistent and makes getting to the current 'qh' easy when
the code knows the direction beforehand.

While at it, turn some assignments into intializers and
fix declaration style in the vicinity.

Signed-off-by: Sergei Shtylyov <sshtylyov-hkdhdckH98+B+jHODAdFcQ@public.gmane.org>
Signed-off-by: David Brownell <dbrownell-Rn4VEauK+AKRv+LV9MX5uipxlwaOVQ5f@public.gmane.org>
---
 drivers/usb/musb/musb_host.c |   56 ++++++++++++++++-------------------------
 1 files changed, 22 insertions(+), 34 deletions(-)

diff --git a/drivers/usb/musb/musb_host.c b/drivers/usb/musb/musb_host.c
index dc32ce4..bc89079 100644
--- a/drivers/usb/musb/musb_host.c
+++ b/drivers/usb/musb/musb_host.c
@@ -178,6 +178,19 @@ static inline void cppi_host_txdma_start(struct musb_hw_ep *ep)
 	musb_writew(ep->regs, MUSB_TXCSR, txcsr);
 }
 
+static void musb_ep_set_qh(struct musb_hw_ep *ep, int is_in, struct musb_qh *qh)
+{
+	if (is_in != 0 || ep->is_shared_fifo)
+		ep->in_qh  = qh;
+	if (is_in == 0 || ep->is_shared_fifo)
+		ep->out_qh = qh;
+}
+
+static struct musb_qh *musb_ep_get_qh(struct musb_hw_ep *ep, int is_in)
+{
+	return is_in ? ep->in_qh : ep->out_qh;
+}
+
 /*
  * Start the URB at the front of an endpoint's queue
  * end must be claimed from the caller.
@@ -207,7 +220,6 @@ musb_start_urb(struct musb *musb, int is_in, struct musb_qh *qh)
 	case USB_ENDPOINT_XFER_CONTROL:
 		/* control transfers always start with SETUP */
 		is_in = 0;
-		hw_ep->out_qh = qh;
 		musb->ep0_stage = MUSB_EP0_START;
 		buf = urb->setup_packet;
 		len = 8;
@@ -236,10 +248,7 @@ musb_start_urb(struct musb *musb, int is_in, struct musb_qh *qh)
 			epnum, buf + offset, len);
 
 	/* Configure endpoint */
-	if (is_in || hw_ep->is_shared_fifo)
-		hw_ep->in_qh = qh;
-	else
-		hw_ep->out_qh = qh;
+	musb_ep_set_qh(hw_ep, is_in, qh);
 	musb_ep_program(musb, epnum, urb, !is_in, buf, offset, len);
 
 	/* transmit may have more work: start it when it is time */
@@ -374,11 +383,8 @@ musb_giveback(struct musb_qh *qh, struct urb *urb, int status)
 		else
 			ep->tx_reinit = 1;
 
-		/* clobber old pointers to this qh */
-		if (is_in || ep->is_shared_fifo)
-			ep->in_qh = NULL;
-		else
-			ep->out_qh = NULL;
+		/* Clobber old pointers to this qh */
+		musb_ep_set_qh(ep, is_in, NULL);
 		qh->hep->hcpriv = NULL;
 
 		switch (qh->type) {
@@ -421,12 +427,7 @@ static void
 musb_advance_schedule(struct musb *musb, struct urb *urb,
 		struct musb_hw_ep *hw_ep, int is_in)
 {
-	struct musb_qh	*qh;
-
-	if (is_in || hw_ep->is_shared_fifo)
-		qh = hw_ep->in_qh;
-	else
-		qh = hw_ep->out_qh;
+	struct musb_qh		*qh = musb_ep_get_qh(hw_ep, is_in);
 
 	if (urb->status == -EINPROGRESS)
 		qh = musb_giveback(qh, urb, 0);
@@ -689,15 +690,8 @@ static void musb_ep_program(struct musb *musb, u8 epnum,
 	void __iomem		*mbase = musb->mregs;
 	struct musb_hw_ep	*hw_ep = musb->endpoints + epnum;
 	void __iomem		*epio = hw_ep->regs;
-	struct musb_qh		*qh;
-	u16			packet_sz;
-
-	if (!is_out || hw_ep->is_shared_fifo)
-		qh = hw_ep->in_qh;
-	else
-		qh = hw_ep->out_qh;
-
-	packet_sz = qh->maxpacket;
+	struct musb_qh		*qh = musb_ep_get_qh(hw_ep, !is_out);
+	u16			packet_sz = qh->maxpacket;
 
 	DBG(3, "%s hw%d urb %p spd%d dev%d ep%d%s "
 				"h_addr%02x h_port%02x bytes %d\n",
@@ -1114,17 +1108,14 @@ void musb_host_tx(struct musb *musb, u8 epnum)
 	u16			tx_csr;
 	size_t			length = 0;
 	size_t			offset = 0;
-	struct urb		*urb;
 	struct musb_hw_ep	*hw_ep = musb->endpoints + epnum;
 	void __iomem		*epio = hw_ep->regs;
-	struct musb_qh		*qh = hw_ep->is_shared_fifo ? hw_ep->in_qh
-							    : hw_ep->out_qh;
+	struct musb_qh		*qh = hw_ep->out_qh;
+	struct urb		*urb = next_urb(qh);
 	u32			status = 0;
 	void __iomem		*mbase = musb->mregs;
 	struct dma_channel	*dma;
 
-	urb = next_urb(qh);
-
 	musb_ep_select(mbase, epnum);
 	tx_csr = musb_readw(epio, MUSB_TXCSR);
 
@@ -1741,10 +1732,7 @@ static int musb_schedule(
 			epnum++, hw_ep++) {
 		int	diff;
 
-		if (is_in || hw_ep->is_shared_fifo) {
-			if (hw_ep->in_qh  != NULL)
-				continue;
-		} else	if (hw_ep->out_qh != NULL)
+		if (musb_ep_get_qh(hw_ep, is_in) != NULL)
 			continue;
 
 		if (hw_ep == musb->bulk_ep)
-- 
1.6.0.4

