From 2377c3d6cf49c057bd2237fbabf429a9b243c663 Mon Sep 17 00:00:00 2001
From: Roger Quadros <roger.quadros@nokia.com>
Date: Wed, 10 Mar 2010 15:30:05 +0200
Subject: [PATCH 4/10] OMAP: RX51: Add LCD Panel support

From: Roger Quadros <roger.quadros@nokia.com>

Patch-mainline: 2.6.35?
Git-repo: http://www.gitorious.org/linux-omap-dss2/linux/commit/c296146d9fe00624cbb34da56c6b2927ef9bbbad

Adds basic support for LCD Panel on Nokia N900

Signed-off-by: Roger Quadros <roger.quadros@nokia.com>
---
 arch/arm/mach-omap2/Makefile                 |    1 +
 arch/arm/mach-omap2/board-rx51-peripherals.c |   13 +++
 arch/arm/mach-omap2/board-rx51-video.c       |  107 ++++++++++++++++++++++++++
 arch/arm/mach-omap2/board-rx51.c             |    2 +
 4 files changed, 123 insertions(+), 0 deletions(-)
 create mode 100644 arch/arm/mach-omap2/board-rx51-video.c

diff --git a/arch/arm/mach-omap2/Makefile b/arch/arm/mach-omap2/Makefile
index b32678b..05e7c9c 100644
--- a/arch/arm/mach-omap2/Makefile
+++ b/arch/arm/mach-omap2/Makefile
@@ -89,6 +89,7 @@ obj-$(CONFIG_MACH_NOKIA_N8X0)		+= board-n8x0.o
 obj-$(CONFIG_MACH_NOKIA_RX51)		+= board-rx51.o \
 					   board-rx51-sdram.o \
 					   board-rx51-peripherals.o \
+					   board-rx51-video.o \
 					   mmc-twl4030.o
 obj-$(CONFIG_MACH_OMAP_ZOOM2)		+= board-zoom2.o \
 					   board-zoom-peripherals.o \
diff --git a/arch/arm/mach-omap2/board-rx51-peripherals.c b/arch/arm/mach-omap2/board-rx51-peripherals.c
index acafdbc..7bae364 100644
--- a/arch/arm/mach-omap2/board-rx51-peripherals.c
+++ b/arch/arm/mach-omap2/board-rx51-peripherals.c
@@ -45,6 +45,7 @@
 /* list all spi devices here */
 enum {
 	RX51_SPI_WL1251,
+	RX51_SPI_MIPID,		/* LCD panel */
 };
 
 static struct wl12xx_platform_data wl1251_pdata;
@@ -54,6 +55,11 @@ static struct omap2_mcspi_device_config wl1251_mcspi_config = {
 	.single_channel	= 1,
 };
 
+static struct omap2_mcspi_device_config mipid_mcspi_config = {
+	.turbo_mode	= 0,
+	.single_channel	= 1,
+};
+
 static struct spi_board_info rx51_peripherals_spi_board_info[] __initdata = {
 	[RX51_SPI_WL1251] = {
 		.modalias		= "wl1251",
@@ -64,6 +70,13 @@ static struct spi_board_info rx51_peripherals_spi_board_info[] __initdata = {
 		.controller_data	= &wl1251_mcspi_config,
 		.platform_data		= &wl1251_pdata,
 	},
+	[RX51_SPI_MIPID] = {
+		.modalias		= "acx565akm",
+		.bus_num		= 1,
+		.chip_select		= 2,
+		.max_speed_hz		= 6000000,
+		.controller_data	= &mipid_mcspi_config,
+	},
 };
 
 #if defined(CONFIG_KEYBOARD_GPIO) || defined(CONFIG_KEYBOARD_GPIO_MODULE)
diff --git a/arch/arm/mach-omap2/board-rx51-video.c b/arch/arm/mach-omap2/board-rx51-video.c
new file mode 100644
index 0000000..e4a9d4c
--- /dev/null
+++ b/arch/arm/mach-omap2/board-rx51-video.c
@@ -0,0 +1,107 @@
+/*
+ * linux/arch/arm/mach-omap2/board-rx51-video.c
+ *
+ * Copyright (C) 2010 Nokia
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+#include <linux/kernel.h>
+#include <linux/init.h>
+#include <linux/platform_device.h>
+#include <linux/gpio.h>
+#include <linux/spi/spi.h>
+#include <linux/mm.h>
+
+#include <asm/mach-types.h>
+#include <plat/mux.h>
+#include <plat/display.h>
+#include <plat/vram.h>
+#include <plat/mcspi.h>
+
+#include "mux.h"
+
+#define RX51_LCD_RESET_GPIO	90
+
+#if defined(CONFIG_FB_OMAP2) || defined(CONFIG_FB_OMAP2_MODULE)
+
+static int rx51_lcd_enable(struct omap_dss_device *dssdev)
+{
+	gpio_set_value(dssdev->reset_gpio, 1);
+	return 0;
+}
+
+static void rx51_lcd_disable(struct omap_dss_device *dssdev)
+{
+	gpio_set_value(dssdev->reset_gpio, 0);
+}
+
+static struct omap_dss_device rx51_lcd_device = {
+	.name			= "lcd",
+	.driver_name		= "panel-acx565akm",
+	.type			= OMAP_DISPLAY_TYPE_SDI,
+	.phy.sdi.datapairs	= 2,
+	.reset_gpio		= RX51_LCD_RESET_GPIO,
+	.platform_enable	= rx51_lcd_enable,
+	.platform_disable	= rx51_lcd_disable,
+};
+
+static struct omap_dss_device *rx51_dss_devices[] = {
+	&rx51_lcd_device,
+};
+
+static struct omap_dss_board_info rx51_dss_board_info = {
+	.num_devices	= ARRAY_SIZE(rx51_dss_devices),
+	.devices	= rx51_dss_devices,
+	.default_device	= &rx51_lcd_device,
+};
+
+struct platform_device rx51_display_device = {
+	.name	= "omapdss",
+	.id	= -1,
+	.dev	= {
+		.platform_data = &rx51_dss_board_info,
+	},
+};
+
+static struct platform_device *rx51_video_devices[] __initdata = {
+	&rx51_display_device,
+};
+
+static int __init rx51_video_init(void)
+{
+	if (!machine_is_nokia_rx51())
+		return 0;
+
+	if (omap_mux_init_gpio(RX51_LCD_RESET_GPIO, OMAP_PIN_OUTPUT)) {
+		pr_err("%s cannot configure MUX for LCD RESET\n", __func__);
+		return 0;
+	}
+
+	if (gpio_request(RX51_LCD_RESET_GPIO, "LCD ACX565AKM reset")) {
+		pr_err("%s failed to get LCD Reset GPIO\n", __func__);
+		return 0;
+	}
+
+	gpio_direction_output(RX51_LCD_RESET_GPIO, 1);
+
+	platform_add_devices(rx51_video_devices,
+				ARRAY_SIZE(rx51_video_devices));
+	return 0;
+}
+
+subsys_initcall(rx51_video_init);
+
+void __init rx51_video_mem_init(void)
+{
+	/*
+	 * GFX 864x480x32bpp
+	 * VID1/2 1280x720x32bpp double buffered
+	 */
+	omap_vram_set_sdram_vram(PAGE_ALIGN(864 * 480 * 4) +
+			2 * PAGE_ALIGN(1280 * 720 * 4 * 2), 0);
+}
+
+#endif /* defined(CONFIG_FB_OMAP2) || defined(CONFIG_FB_OMAP2_MODULE) */
diff --git a/arch/arm/mach-omap2/board-rx51.c b/arch/arm/mach-omap2/board-rx51.c
index 67bb347..f1f81cf 100644
--- a/arch/arm/mach-omap2/board-rx51.c
+++ b/arch/arm/mach-omap2/board-rx51.c
@@ -32,6 +32,7 @@
 #include "mux.h"
 
 struct omap_sdrc_params *rx51_get_sdram_timings(void);
+extern void rx51_video_mem_init(void);
 
 static struct omap_lcd_config rx51_lcd_config = {
 	.ctrl_name	= "internal",
@@ -93,6 +94,7 @@ static void __init rx51_init(void)
 static void __init rx51_map_io(void)
 {
 	omap2_set_globals_343x();
+	rx51_video_mem_init();
 	omap2_map_common_io();
 }
 
-- 
1.6.0.4

