From ad422f476ce04636f911557bbfd066c516e9b472 Mon Sep 17 00:00:00 2001
From: Aguirre Rodriguez, Sergio Alberto <saaguirre@ti.com>
Date: Tue, 20 Jan 2009 16:29:26 -0600
Subject: [PATCH] V4L2: Add COLORFX user control

From 07396d67b39bf7bcc81440d3e72d253ad6c54f11 Mon Sep 17 00:00:00 2001
From: Sergio Aguirre <saaguirre@ti.com>
Date: Tue, 20 Jan 2009 15:34:43 -0600
Subject: [PATCH v2] V4L2: Add COLORFX user control

This is a common feature on many cameras. the options are:
Default colors,
B & W,
Sepia

Signed-off-by: Sergio Aguirre <saaguirre@ti.com>
---
 include/linux/videodev2.h |    9 ++++++++-
 1 files changed, 8 insertions(+), 1 deletions(-)

diff --git a/include/linux/videodev2.h b/include/linux/videodev2.h
index 5571dbe..8e4e25e 100644
--- a/include/linux/videodev2.h
+++ b/include/linux/videodev2.h
@@ -879,8 +879,15 @@ enum v4l2_power_line_frequency {
 #define V4L2_CID_BACKLIGHT_COMPENSATION 	(V4L2_CID_BASE+28)
 #define V4L2_CID_CHROMA_AGC                     (V4L2_CID_BASE+29)
 #define V4L2_CID_COLOR_KILLER                   (V4L2_CID_BASE+30)
+#define V4L2_CID_COLORFX			(V4L2_CID_BASE+31)
+enum v4l2_colorfx {
+	V4L2_COLORFX_NONE	= 0,
+	V4L2_COLORFX_BW		= 1,
+	V4L2_COLORFX_SEPIA	= 2,
+};
+
 /* last CID + 1 */
-#define V4L2_CID_LASTP1                         (V4L2_CID_BASE+31)
+#define V4L2_CID_LASTP1                         (V4L2_CID_BASE+32)
 
 /*  MPEG-class control IDs defined by V4L2 */
 #define V4L2_CID_MPEG_BASE 			(V4L2_CTRL_CLASS_MPEG | 0x900)
-- 
1.5.6.5

