From 1a91088e389bd3bbf5d9ee1f3a15edd9edb84eb6 Mon Sep 17 00:00:00 2001
From: Enric Balletbo i Serra <eballetbo@iseebcn.com>
Date: Wed, 16 Jun 2010 17:41:26 +0200
Subject: [PATCH] omap3: init MUX for OMAP3 IGEP module.

Signed-off-by: Enric Balletbo i Serra <eballetbo@iseebcn.com>
---
 arch/arm/mach-omap2/board-igep0030.c |   10 ++++++++++
 1 files changed, 10 insertions(+), 0 deletions(-)

diff --git a/arch/arm/mach-omap2/board-igep0030.c b/arch/arm/mach-omap2/board-igep0030.c
index aa99236..425b2ec 100644
--- a/arch/arm/mach-omap2/board-igep0030.c
+++ b/arch/arm/mach-omap2/board-igep0030.c
@@ -420,8 +420,18 @@ static void __init igep3_init_wifi_bt(void)
 		pr_warning("IGEP: Could not obtain gpio GPIO_BT_NRESET\n");
 }
 
+#ifdef CONFIG_OMAP_MUX
+static struct omap_board_mux board_mux[] __initdata = {
+	{ .reg_offset = OMAP_MUX_TERMINATOR },
+};
+#else
+#define board_mux	NULL
+#endif
+
 static void __init igep3_init(void)
 {
+	omap3_mux_init(board_mux, OMAP_PACKAGE_CBB);
+
 	omap_serial_init();
 	usb_musb_init(&musb_board_data);
 	usb_ehci_init(&ehci_pdata);
-- 
1.7.0.4

