From 32beea722c1167c9b33f1ecfdc28d360cabd6823 Mon Sep 17 00:00:00 2001
From: Peter Hoyes <Peter.Hoyes@arm.com>
Date: Tue, 22 Feb 2022 15:32:51 +0000
Subject: [PATCH 7/9] vexpress64: Enable LIBFDT_OVERLAY in the vexpress_aemv8r
 defconfig

Issue-Id: SCM-3874
Upstream-Status: Inappropriate [other]
  Implementation pending further discussion
Signed-off-by: Peter Hoyes <Peter.Hoyes@arm.com>
Change-Id: Ide0532cf2de89f1bca9c8d4bd2ed0c1a1c57599f
---
 configs/vexpress_aemv8r_defconfig | 1 +
 1 file changed, 1 insertion(+)

diff --git a/configs/vexpress_aemv8r_defconfig b/configs/vexpress_aemv8r_defconfig
index b902a6a7d9..a58a9db385 100644
--- a/configs/vexpress_aemv8r_defconfig
+++ b/configs/vexpress_aemv8r_defconfig
@@ -18,3 +18,4 @@ CONFIG_VIRTIO_MMIO=y
 CONFIG_ARMV8_EXCEPTION_VECTORS=n
 CONFIG_ARMV8_SWITCH_TO_EL1=y
 CONFIG_ARMV8_DISABLE_HVC=n
+CONFIG_OF_LIBFDT_OVERLAY=y
-- 
2.25.1

