From 9c98333d7c5f4c2611c76d60f5e7cb96bfdaca26 Mon Sep 17 00:00:00 2001
From: Diego Sueiro <diego.sueiro@arm.com>
Date: Wed, 4 Oct 2023 06:29:12 +0100
Subject: [PATCH] vexpress64: Imply CONFIG_ARM64_CRC32 by default

Enable the Arm64 CRC-32 instruction by default for
vexpress64. The CRC-32 instruction is a required
feature of ARMv8.1 and newer.

Upstream-Status: Pending
Signed-off-by: Diego Sueiro <diego.sueiro@arm.com>
---
 board/armltd/vexpress64/Kconfig | 1 +
 1 file changed, 1 insertion(+)

diff --git a/board/armltd/vexpress64/Kconfig b/board/armltd/vexpress64/Kconfig
index d0733ba62432..543cbdb5631b 100644
--- a/board/armltd/vexpress64/Kconfig
+++ b/board/armltd/vexpress64/Kconfig
@@ -22,6 +22,7 @@ config VEXPRESS64_BASE_MODEL
 	select LINUX_KERNEL_IMAGE_HEADER
 	select POSITION_INDEPENDENT
 	imply DM_RNG
+	imply ARM64_CRC32
 
 choice
 	prompt "VExpress64 board variant"
