From 5a2565d002084a4c6b80329a4a23cb6c98c4f344 Mon Sep 17 00:00:00 2001
From: Jens Wiklander <jens.wiklander@linaro.org>
Date: Thu, 25 Mar 2021 15:08:46 +0100
Subject: [PATCH 09/40] optee: simplify optee_release()

Simplifies optee_release() with a new helper function,
optee_close_session_helper() which has been factored out from
optee_close_session().

A separate optee_release_supp() is added for the supplicant device.

Reviewed-by: Sumit Garg <sumit.garg@linaro.org>
Signed-off-by: Jens Wiklander <jens.wiklander@linaro.org>
Upstream-Status: Backport [c0ab6db39a908d86ed44e8a5632548e2ec1b4dca]
Signed-off-by: Rupinderjit Singh <rupinderjit.singh@arm.com>
---
 drivers/tee/optee/call.c          | 31 ++++++++++-------
 drivers/tee/optee/core.c          | 56 +++++++++++--------------------
 drivers/tee/optee/optee_private.h |  1 +
 3 files changed, 39 insertions(+), 49 deletions(-)

diff --git a/drivers/tee/optee/call.c b/drivers/tee/optee/call.c
index 945f03da0223..103976df2062 100644
--- a/drivers/tee/optee/call.c
+++ b/drivers/tee/optee/call.c
@@ -288,12 +288,28 @@ int optee_open_session(struct tee_context *ctx,
 	return rc;
 }
 
-int optee_close_session(struct tee_context *ctx, u32 session)
+int optee_close_session_helper(struct tee_context *ctx, u32 session)
 {
-	struct optee_context_data *ctxdata = ctx->data;
 	struct tee_shm *shm;
 	struct optee_msg_arg *msg_arg;
 	phys_addr_t msg_parg;
+
+	shm = get_msg_arg(ctx, 0, &msg_arg, &msg_parg);
+	if (IS_ERR(shm))
+		return PTR_ERR(shm);
+
+	msg_arg->cmd = OPTEE_MSG_CMD_CLOSE_SESSION;
+	msg_arg->session = session;
+	optee_do_call_with_arg(ctx, msg_parg);
+
+	tee_shm_free(shm);
+
+	return 0;
+}
+
+int optee_close_session(struct tee_context *ctx, u32 session)
+{
+	struct optee_context_data *ctxdata = ctx->data;
 	struct optee_session *sess;
 
 	/* Check that the session is valid and remove it from the list */
@@ -306,16 +322,7 @@ int optee_close_session(struct tee_context *ctx, u32 session)
 		return -EINVAL;
 	kfree(sess);
 
-	shm = get_msg_arg(ctx, 0, &msg_arg, &msg_parg);
-	if (IS_ERR(shm))
-		return PTR_ERR(shm);
-
-	msg_arg->cmd = OPTEE_MSG_CMD_CLOSE_SESSION;
-	msg_arg->session = session;
-	optee_do_call_with_arg(ctx, msg_parg);
-
-	tee_shm_free(shm);
-	return 0;
+	return optee_close_session_helper(ctx, session);
 }
 
 int optee_invoke_func(struct tee_context *ctx, struct tee_ioctl_invoke_arg *arg,
diff --git a/drivers/tee/optee/core.c b/drivers/tee/optee/core.c
index 5363ebebfc35..79f67a79e7b7 100644
--- a/drivers/tee/optee/core.c
+++ b/drivers/tee/optee/core.c
@@ -264,60 +264,42 @@ static int optee_open(struct tee_context *ctx)
 	return 0;
 }
 
-static void optee_release(struct tee_context *ctx)
+static void optee_release_helper(struct tee_context *ctx,
+				 int (*close_session)(struct tee_context *ctx,
+						      u32 session))
 {
 	struct optee_context_data *ctxdata = ctx->data;
-	struct tee_device *teedev = ctx->teedev;
-	struct optee *optee = tee_get_drvdata(teedev);
-	struct tee_shm *shm;
-	struct optee_msg_arg *arg = NULL;
-	phys_addr_t parg;
 	struct optee_session *sess;
 	struct optee_session *sess_tmp;
 
 	if (!ctxdata)
 		return;
 
-	shm = tee_shm_alloc(ctx, sizeof(struct optee_msg_arg),
-			    TEE_SHM_MAPPED | TEE_SHM_PRIV);
-	if (!IS_ERR(shm)) {
-		arg = tee_shm_get_va(shm, 0);
-		/*
-		 * If va2pa fails for some reason, we can't call into
-		 * secure world, only free the memory. Secure OS will leak
-		 * sessions and finally refuse more sessions, but we will
-		 * at least let normal world reclaim its memory.
-		 */
-		if (!IS_ERR(arg))
-			if (tee_shm_va2pa(shm, arg, &parg))
-				arg = NULL; /* prevent usage of parg below */
-	}
-
 	list_for_each_entry_safe(sess, sess_tmp, &ctxdata->sess_list,
 				 list_node) {
 		list_del(&sess->list_node);
-		if (!IS_ERR_OR_NULL(arg)) {
-			memset(arg, 0, sizeof(*arg));
-			arg->cmd = OPTEE_MSG_CMD_CLOSE_SESSION;
-			arg->session = sess->session_id;
-			optee_do_call_with_arg(ctx, parg);
-		}
+		close_session(ctx, sess->session_id);
 		kfree(sess);
 	}
 	kfree(ctxdata);
+	ctx->data = NULL;
+}
 
-	if (!IS_ERR(shm))
-		tee_shm_free(shm);
+static void optee_release(struct tee_context *ctx)
+{
+	optee_release_helper(ctx, optee_close_session_helper);
+}
 
-	ctx->data = NULL;
+static void optee_release_supp(struct tee_context *ctx)
+{
+	struct optee *optee = tee_get_drvdata(ctx->teedev);
 
-	if (teedev == optee->supp_teedev) {
-		if (optee->scan_bus_wq) {
-			destroy_workqueue(optee->scan_bus_wq);
-			optee->scan_bus_wq = NULL;
-		}
-		optee_supp_release(&optee->supp);
+	optee_release_helper(ctx, optee_close_session_helper);
+	if (optee->scan_bus_wq) {
+		destroy_workqueue(optee->scan_bus_wq);
+		optee->scan_bus_wq = NULL;
 	}
+	optee_supp_release(&optee->supp);
 }
 
 static const struct tee_driver_ops optee_ops = {
@@ -341,7 +323,7 @@ static const struct tee_desc optee_desc = {
 static const struct tee_driver_ops optee_supp_ops = {
 	.get_version = optee_get_version,
 	.open = optee_open,
-	.release = optee_release,
+	.release = optee_release_supp,
 	.supp_recv = optee_supp_recv,
 	.supp_send = optee_supp_send,
 	.shm_register = optee_shm_register_supp,
diff --git a/drivers/tee/optee/optee_private.h b/drivers/tee/optee/optee_private.h
index f6bb4a763ba9..a55793f9f6eb 100644
--- a/drivers/tee/optee/optee_private.h
+++ b/drivers/tee/optee/optee_private.h
@@ -152,6 +152,7 @@ u32 optee_do_call_with_arg(struct tee_context *ctx, phys_addr_t parg);
 int optee_open_session(struct tee_context *ctx,
 		       struct tee_ioctl_open_session_arg *arg,
 		       struct tee_param *param);
+int optee_close_session_helper(struct tee_context *ctx, u32 session);
 int optee_close_session(struct tee_context *ctx, u32 session);
 int optee_invoke_func(struct tee_context *ctx, struct tee_ioctl_invoke_arg *arg,
 		      struct tee_param *param);
-- 
2.34.1

