# WIC partitioning for corstone500
# Layout and maximum sizes (to be defined):
#

# Rawcopy of the FIP binary
part --source rawcopy --sourceparams="file=fip.bin" --no-table --align 1 --fixed-size 1

# Rawcopy of the kernel binary
part --source rawcopy --sourceparams="file=zImage" --no-table --fixed-size 12

# Rawcopy of the rootfs
part --source rawcopy --sourceparams="file=${IMGDEPLOYDIR}/core-image-minimal-corstone500.squashfs" --no-table
