# Australia / Sydney (transmitters at Artarmon/Gore Hill/Willoughby)
#
# ## Service - Channel - Network owner
#
## ABC - CH12 - ABC
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 226500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = AUTO
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

## ATN - CH6 - Seven Network
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 177500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = AUTO
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

## TCN - CH8 - Nine Network
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 191625000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = AUTO
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

## TEN - CH11 - Network Ten
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 219500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = AUTO
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

## SBS - CH7 - SBS
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 184500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = AUTO
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

## TSN - CH29 - Community Television
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 536625000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = AUTO
	MODULATION = QPSK
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

