From b1196ec5f007cef5cd3342ed3dbf3415bf721bd4 Mon Sep 17 00:00:00 2001
From: Sergio Aguirre <saaguirre@ti.com>
Date: Sun, 18 Jul 2010 01:45:29 -0500
Subject: [PATCH 67/75] mt9t112: Disable JPEG in Context B

Signed-off-by: Sergio Aguirre <saaguirre@ti.com>
---
 drivers/media/video/mt9t112.c |    8 --------
 1 files changed, 0 insertions(+), 8 deletions(-)

diff --git a/drivers/media/video/mt9t112.c b/drivers/media/video/mt9t112.c
index ec7514f..18d7ce5 100644
--- a/drivers/media/video/mt9t112.c
+++ b/drivers/media/video/mt9t112.c
@@ -812,14 +812,6 @@ static int mt9t112_init_camera(const struct i2c_client *client)
 	mt9t112_mcu_write(ret, client, VAR(26, 160), 0x0A2E);
 	mt9t112_mcu_write(ret, client, VAR(27, 160), 0x0A2E);
 
-	/* Configure STatus in Status_before_length Format and enable header */
-	/* PRI_B_CONFIG_JPEG_OB_TX_CONTROL_VAR */
-	mt9t112_mcu_write(ret, client, VAR(27, 144), 0x0CB4);
-
-	/* Enable JPEG in context B */
-	/* PRI_B_CONFIG_JPEG_OB_TX_CONTROL_VAR */
-	mt9t112_mcu_write(ret, client, VAR8(27, 142), 0x01);
-
 	/* Disable Dac_TXLO */
 	mt9t112_reg_write(ret, client, 0x316C, 0x350F);
 
-- 
1.6.6.1

