From f5b19d6609a540a9eafa60dad902e7416df57771 Mon Sep 17 00:00:00 2001
From: Koen Kooi <koen@dominion.thruhere.net>
Date: Mon, 30 Apr 2012 11:10:07 +0200
Subject: [PATCH 13/13] beagleboard: switch mmcroots to ext4

Signed-off-by: Koen Kooi <koen@dominion.thruhere.net>
---
 include/configs/omap3_beagle.h |    5 +++--
 1 file changed, 3 insertions(+), 2 deletions(-)

diff --git a/include/configs/omap3_beagle.h b/include/configs/omap3_beagle.h
index 65ab8ee..3157d47 100644
--- a/include/configs/omap3_beagle.h
+++ b/include/configs/omap3_beagle.h
@@ -140,6 +140,7 @@
 
 #define CONFIG_CMD_CACHE
 #define CONFIG_CMD_EXT2		/* EXT2 Support			*/
+#define CONFIG_CMD_EXT4
 #define CONFIG_CMD_FAT		/* FAT support			*/
 #define CONFIG_CMD_JFFS2	/* JFFS2 Support		*/
 #define CONFIG_CMD_MTDPARTS	/* Enable MTD parts commands */
@@ -222,7 +223,7 @@
 	"defaultdisplay=dvi\0" \
 	"mmcdev=0\0" \
 	"mmcroot=/dev/mmcblk0p2 ro\0" \
-	"mmcrootfstype=ext3 rootwait\0" \
+	"mmcrootfstype=ext4 rootwait\0" \
 	"nandroot=ubi0:rootfs ubi.mtd=4\0" \
 	"nandrootfstype=ubifs\0" \
 	"ramroot=/dev/ram0 rw ramdisk_size=65536 initrd=0x81000000,64M\0" \
@@ -265,7 +266,7 @@
 		"rootfstype=${ramrootfstype}\0" \
 	"loadramdisk=fatload mmc ${mmcdev} ${rdaddr} ramdisk.gz\0" \
 	"loaduimagefat=fatload mmc ${mmcdev} ${loadaddr} uImage\0" \
-	"loaduimage=ext2load mmc ${mmcdev}:2 ${loadaddr} /boot/uImage\0" \
+	"loaduimage=ext4load mmc ${mmcdev}:2 ${loadaddr} /boot/uImage\0" \
 	"mmcboot=echo Booting from mmc ...; " \
 		"run mmcargs; " \
 		"bootm ${loadaddr}\0" \
-- 
1.7.10

