From bfb12525292fbd7a9837de23fc1e8dda589b43a1 Mon Sep 17 00:00:00 2001
From: Alex Deucher <alexander.deucher@amd.com>
Date: Thu, 29 Mar 2012 19:04:08 -0400
Subject: [PATCH 26/60] drm/radeon/kms: fix fans after resume
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

commit 402976fe51b2d1a58a29ba06fa1ca5ace3a4cdcd upstream.

On pre-R600 asics, the SpeedFanControl table is not
executed as part of ASIC_Init as it is on newer asics.

Fixes:
https://bugzilla.kernel.org/show_bug.cgi?id=29412

Signed-off-by: Alex Deucher <alexander.deucher@amd.com>
Reviewed-by: Michel Dänzer <michel.daenzer@amd.com>
Signed-off-by: Dave Airlie <airlied@redhat.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/gpu/drm/radeon/atom.c |   15 ++++++++++++++-
 drivers/gpu/drm/radeon/atom.h |    1 +
 2 files changed, 15 insertions(+), 1 deletion(-)

diff --git a/drivers/gpu/drm/radeon/atom.c b/drivers/gpu/drm/radeon/atom.c
index 14cc88a..3a05cdb 100644
--- a/drivers/gpu/drm/radeon/atom.c
+++ b/drivers/gpu/drm/radeon/atom.c
@@ -1304,8 +1304,11 @@ struct atom_context *atom_parse(struct card_info *card, void *bios)
 
 int atom_asic_init(struct atom_context *ctx)
 {
+	struct radeon_device *rdev = ctx->card->dev->dev_private;
 	int hwi = CU16(ctx->data_table + ATOM_DATA_FWI_PTR);
 	uint32_t ps[16];
+	int ret;
+
 	memset(ps, 0, 64);
 
 	ps[0] = cpu_to_le32(CU32(hwi + ATOM_FWI_DEFSCLK_PTR));
@@ -1315,7 +1318,17 @@ int atom_asic_init(struct atom_context *ctx)
 
 	if (!CU16(ctx->cmd_table + 4 + 2 * ATOM_CMD_INIT))
 		return 1;
-	return atom_execute_table(ctx, ATOM_CMD_INIT, ps);
+	ret = atom_execute_table(ctx, ATOM_CMD_INIT, ps);
+	if (ret)
+		return ret;
+
+	memset(ps, 0, 64);
+
+	if (rdev->family < CHIP_R600) {
+		if (CU16(ctx->cmd_table + 4 + 2 * ATOM_CMD_SPDFANCNTL))
+			atom_execute_table(ctx, ATOM_CMD_SPDFANCNTL, ps);
+	}
+	return ret;
 }
 
 void atom_destroy(struct atom_context *ctx)
diff --git a/drivers/gpu/drm/radeon/atom.h b/drivers/gpu/drm/radeon/atom.h
index 93cfe20..25fea63 100644
--- a/drivers/gpu/drm/radeon/atom.h
+++ b/drivers/gpu/drm/radeon/atom.h
@@ -44,6 +44,7 @@
 #define ATOM_CMD_SETSCLK	0x0A
 #define ATOM_CMD_SETMCLK	0x0B
 #define ATOM_CMD_SETPCLK	0x0C
+#define ATOM_CMD_SPDFANCNTL	0x39
 
 #define ATOM_DATA_FWI_PTR	0xC
 #define ATOM_DATA_IIO_PTR	0x32
-- 
1.7.9.5

