From 17cd354184d7ffe9fcef97a0e1beeb6e8b2a2c38 Mon Sep 17 00:00:00 2001
From: Kevin Hilman <khilman@ti.com>
Date: Wed, 23 Mar 2011 13:30:33 -0700
Subject: [PATCH 101/149] OMAP3: voltagedomain data: add wakeup domain

Add wakeup voltage domain so that the wakeup powerdomain can have an
associated powerdomain.  Note that the scalable flat is not set for
the this voltagedomain, so it will not be fully initialized like
scalable voltage domains.

Signed-off-by: Kevin Hilman <khilman@ti.com>
---
 arch/arm/mach-omap2/voltagedomains3xxx_data.c |    5 +++++
 1 files changed, 5 insertions(+), 0 deletions(-)

diff --git a/arch/arm/mach-omap2/voltagedomains3xxx_data.c b/arch/arm/mach-omap2/voltagedomains3xxx_data.c
index 2167ef4..42d0b11 100644
--- a/arch/arm/mach-omap2/voltagedomains3xxx_data.c
+++ b/arch/arm/mach-omap2/voltagedomains3xxx_data.c
@@ -69,9 +69,14 @@ static struct voltagedomain omap3_voltdm_core = {
 	.vdd = &omap3_vdd2_info,
 };
 
+static struct voltagedomain omap3_voltdm_wkup = {
+	.name = "wakeup",
+};
+
 static struct voltagedomain *voltagedomains_omap3[] __initdata = {
 	&omap3_voltdm_mpu,
 	&omap3_voltdm_core,
+	&omap3_voltdm_wkup,
 	NULL,
 };
 
-- 
1.7.2.5

