From 61fa0a2298850898c90ce67bb0b9b440c452820a Mon Sep 17 00:00:00 2001
From: Guenter Roeck <linux@roeck-us.net>
Date: Mon, 12 Mar 2012 08:33:10 -0700
Subject: [PATCH 35/42] hwmon: (w83627ehf) Fix memory leak in probe function

commit 32260d94408c553dca4ce54104edf79941a27536 upstream.

The driver probe function leaked memory if creating the cpu0_vid attribute file
failed. Fix by converting the driver to use devm_kzalloc.

Signed-off-by: Guenter Roeck <linux@roeck-us.net>
Acked-by: Jean Delvare <khali@linux-fr.org>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/hwmon/w83627ehf.c |    7 +++----
 1 file changed, 3 insertions(+), 4 deletions(-)

diff --git a/drivers/hwmon/w83627ehf.c b/drivers/hwmon/w83627ehf.c
index 7a44a56..3ffa1fa 100644
--- a/drivers/hwmon/w83627ehf.c
+++ b/drivers/hwmon/w83627ehf.c
@@ -2004,7 +2004,8 @@ static int __devinit w83627ehf_probe(struct platform_device *pdev)
 		goto exit;
 	}
 
-	data = kzalloc(sizeof(struct w83627ehf_data), GFP_KERNEL);
+	data = devm_kzalloc(&pdev->dev, sizeof(struct w83627ehf_data),
+			    GFP_KERNEL);
 	if (!data) {
 		err = -ENOMEM;
 		goto exit_release;
@@ -2498,9 +2499,8 @@ static int __devinit w83627ehf_probe(struct platform_device *pdev)
 
 exit_remove:
 	w83627ehf_device_remove_files(dev);
-	kfree(data);
-	platform_set_drvdata(pdev, NULL);
 exit_release:
+	platform_set_drvdata(pdev, NULL);
 	release_region(res->start, IOREGION_LENGTH);
 exit:
 	return err;
@@ -2514,7 +2514,6 @@ static int __devexit w83627ehf_remove(struct platform_device *pdev)
 	w83627ehf_device_remove_files(&pdev->dev);
 	release_region(data->addr, IOREGION_LENGTH);
 	platform_set_drvdata(pdev, NULL);
-	kfree(data);
 
 	return 0;
 }
-- 
1.7.9.4

