From b55d48c7cec81071f13dc9e88a657b507573a4ec Mon Sep 17 00:00:00 2001
From: Alex Williamson <alex.williamson@redhat.com>
Date: Wed, 16 Nov 2011 09:24:16 -0700
Subject: [PATCH 031/130] PCI: Fix PCI_EXP_TYPE_RC_EC value

commit 1830ea91c20b06608f7cdb2455ce05ba834b3214 upstream.

Spec shows this as 1010b = 0xa

Signed-off-by: Alex Williamson <alex.williamson@redhat.com>
Signed-off-by: Jesse Barnes <jbarnes@virtuousgeek.org>
Signed-off-by: Greg Kroah-Hartman <gregkh@suse.de>
---
 include/linux/pci_regs.h |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/include/linux/pci_regs.h b/include/linux/pci_regs.h
index b5d9657..411c412 100644
--- a/include/linux/pci_regs.h
+++ b/include/linux/pci_regs.h
@@ -392,7 +392,7 @@
 #define  PCI_EXP_TYPE_DOWNSTREAM 0x6	/* Downstream Port */
 #define  PCI_EXP_TYPE_PCI_BRIDGE 0x7	/* PCI/PCI-X Bridge */
 #define  PCI_EXP_TYPE_RC_END	0x9	/* Root Complex Integrated Endpoint */
-#define  PCI_EXP_TYPE_RC_EC	0x10	/* Root Complex Event Collector */
+#define  PCI_EXP_TYPE_RC_EC	0xa	/* Root Complex Event Collector */
 #define PCI_EXP_FLAGS_SLOT	0x0100	/* Slot implemented */
 #define PCI_EXP_FLAGS_IRQ	0x3e00	/* Interrupt message number */
 #define PCI_EXP_DEVCAP		4	/* Device capabilities */
-- 
1.7.9.4

