From 16c7667d2908631149ef38b7b6dd7b08d6d5502e Mon Sep 17 00:00:00 2001
From: Nishanth Menon <nm@ti.com>
Date: Wed, 5 Jan 2011 14:14:55 -0600
Subject: [PATCH 18/20] omap3|4: opp: make omapx_opp_init non-static

omap3 and omap4 opp_init should be made non-static to allow
for platform specific opp table tweaking. making these static
conflicts with the definition in pm.h(global) as well.
we include pm.h as well to ensure that there are no such prototype
conflicts with actual implementation in the future.

Signed-off-by: Nishanth Menon <nm@ti.com>
---
 arch/arm/mach-omap2/opp3xxx_data.c |    3 ++-
 arch/arm/mach-omap2/opp4xxx_data.c |    3 ++-
 2 files changed, 4 insertions(+), 2 deletions(-)

diff --git a/arch/arm/mach-omap2/opp3xxx_data.c b/arch/arm/mach-omap2/opp3xxx_data.c
index 0486fce..fd3a1af 100644
--- a/arch/arm/mach-omap2/opp3xxx_data.c
+++ b/arch/arm/mach-omap2/opp3xxx_data.c
@@ -21,6 +21,7 @@
 #include <plat/cpu.h>
 
 #include "omap_opp_data.h"
+#include "pm.h"
 
 static struct omap_opp_def __initdata omap34xx_opp_def_list[] = {
 	/* MPU OPP1 */
@@ -88,7 +89,7 @@ static struct omap_opp_def __initdata omap36xx_opp_def_list[] = {
 /**
  * omap3_opp_init() - initialize omap3 opp table
  */
-static int __init omap3_opp_init(void)
+int __init omap3_opp_init(void)
 {
 	int r = -ENODEV;
 
diff --git a/arch/arm/mach-omap2/opp4xxx_data.c b/arch/arm/mach-omap2/opp4xxx_data.c
index a11fa56..f0e9939 100644
--- a/arch/arm/mach-omap2/opp4xxx_data.c
+++ b/arch/arm/mach-omap2/opp4xxx_data.c
@@ -22,6 +22,7 @@
 #include <plat/cpu.h>
 
 #include "omap_opp_data.h"
+#include "pm.h"
 
 static struct omap_opp_def __initdata omap44xx_opp_def_list[] = {
 	/* MPU OPP1 - OPP50 */
@@ -42,7 +43,7 @@ static struct omap_opp_def __initdata omap44xx_opp_def_list[] = {
 /**
  * omap4_opp_init() - initialize omap4 opp table
  */
-static int __init omap4_opp_init(void)
+int __init omap4_opp_init(void)
 {
 	int r = -ENODEV;
 
-- 
1.6.6.1

