From ef89a7b5f82deaac432a4a797155b199d7d39c67 Mon Sep 17 00:00:00 2001
From: Kuninori Morimoto <kuninori.morimoto.gx@renesas.com>
Date: Wed, 4 Apr 2012 23:28:01 -0700
Subject: [PATCH 56/60] ASoC: ak4642: fixup: mute needs +1 step

commit 1f99e44cf059d2ed43c5a0724fa738b83800f725 upstream.

ak4642 out_tlv is +12.0dB to -115.0 dB, and it supports mute.
But current settings didn't care +1 step for mute.
This patch adds it

Signed-off-by: Kuninori Morimoto <kuninori.morimoto.gx@renesas.com>
Signed-off-by: Mark Brown <broonie@opensource.wolfsonmicro.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 sound/soc/codecs/ak4642.c |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/sound/soc/codecs/ak4642.c b/sound/soc/codecs/ak4642.c
index 12c1bde..1c4999d 100644
--- a/sound/soc/codecs/ak4642.c
+++ b/sound/soc/codecs/ak4642.c
@@ -144,7 +144,7 @@
  * min : 0xFE : -115.0 dB
  * mute: 0xFF
  */
-static const DECLARE_TLV_DB_SCALE(out_tlv, -11500, 50, 1);
+static const DECLARE_TLV_DB_SCALE(out_tlv, -11550, 50, 1);
 
 static const struct snd_kcontrol_new ak4642_snd_controls[] = {
 
-- 
1.7.9.5

