From 88ee784eddb634074895d68572b896aebd10bb5d Mon Sep 17 00:00:00 2001
From: Steve Sakoman <steve@sakoman.com>
Date: Thu, 30 Dec 2010 07:19:44 +0000
Subject: [PATCH 02/30] OMAP: Remove omapfb.debug=y from Beagle and Overo env settings

The kernel DSS2 code is mature now, and keeping this setting hurts performance

Signed-off-by: Steve Sakoman <steve@sakoman.com>
---
 include/configs/omap3_beagle.h |    2 --
 include/configs/omap3_overo.h  |    2 --
 2 files changed, 0 insertions(+), 4 deletions(-)

diff --git a/include/configs/omap3_beagle.h b/include/configs/omap3_beagle.h
index 9fd80ed..42575f1 100644
--- a/include/configs/omap3_beagle.h
+++ b/include/configs/omap3_beagle.h
@@ -214,7 +214,6 @@
 		"mpurate=${mpurate} " \
 		"vram=${vram} " \
 		"omapfb.mode=dvi:${dvimode} " \
-		"omapfb.debug=y " \
 		"omapdss.def_disp=${defaultdisplay} " \
 		"root=${mmcroot} " \
 		"rootfstype=${mmcrootfstype}\0" \
@@ -222,7 +221,6 @@
 		"mpurate=${mpurate} " \
 		"vram=${vram} " \
 		"omapfb.mode=dvi:${dvimode} " \
-		"omapfb.debug=y " \
 		"omapdss.def_disp=${defaultdisplay} " \
 		"root=${nandroot} " \
 		"rootfstype=${nandrootfstype}\0" \
diff --git a/include/configs/omap3_overo.h b/include/configs/omap3_overo.h
index 242b317..0f64054 100644
--- a/include/configs/omap3_overo.h
+++ b/include/configs/omap3_overo.h
@@ -170,7 +170,6 @@
 		"mpurate=${mpurate} " \
 		"vram=${vram} " \
 		"omapfb.mode=dvi:${dvimode} " \
-		"omapfb.debug=y " \
 		"omapdss.def_disp=${defaultdisplay} " \
 		"root=${mmcroot} " \
 		"rootfstype=${mmcrootfstype}\0" \
@@ -178,7 +177,6 @@
 		"mpurate=${mpurate} " \
 		"vram=${vram} " \
 		"omapfb.mode=dvi:${dvimode} " \
-		"omapfb.debug=y " \
 		"omapdss.def_disp=${defaultdisplay} " \
 		"root=${nandroot} " \
 		"rootfstype=${nandrootfstype}\0" \
-- 
1.6.6.1

