From efa82e03e24743425f4cb3d3632f29756b70d5b5 Mon Sep 17 00:00:00 2001
From: Eran <eran@over-here.org>
Date: Mon, 5 Dec 2011 22:15:29 +0000
Subject: [PATCH 62/69] Bluetooth: Adding USB device 13d3:3375 as an Atheros
 AR3012.

commit 9498ba7a1d38d42eef4ef6d906ab1743c9f0fd6f upstream.

The bluetooth module in the Asus UX31/UX21 is based on Atheros AR3012
and requires a firmware to be uploaded before it's usable.

output of usb-devices for this module:
T:  Bus=01 Lev=02 Prnt=02 Port=07 Cnt=03 Dev#=  6 Spd=12  MxCh= 0
D:  Ver= 1.10 Cls=e0(wlcon) Sub=01 Prot=01 MxPS=64 #Cfgs=  1
P:  Vendor=13d3 ProdID=3375 Rev=00.02
S:  Manufacturer=Atheros Communications
S:  Product=Bluetooth USB Host Controller
S:  SerialNumber=Alaska Day 2006
C:  #Ifs= 2 Cfg#= 1 Atr=e0 MxPwr=100mA
I:  If#= 0 Alt= 0 #EPs= 3 Cls=e0(wlcon) Sub=01 Prot=01 Driver=btusb
I:  If#= 1 Alt= 0 #EPs= 2 Cls=e0(wlcon) Sub=01 Prot=01 Driver=btusb

Signed-off-by: Eran <eran@over-here.org>
Tested-by: Michal Labedzki <michal.labedzki@tieto.com>
Signed-off-by: Gustavo F. Padovan <padovan@profusion.mobi>
Cc: Jonathan Nieder <jrnieder@gmail.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/bluetooth/ath3k.c |    2 ++
 drivers/bluetooth/btusb.c |    1 +
 2 files changed, 3 insertions(+)

diff --git a/drivers/bluetooth/ath3k.c b/drivers/bluetooth/ath3k.c
index db811d2..67a79b0 100644
--- a/drivers/bluetooth/ath3k.c
+++ b/drivers/bluetooth/ath3k.c
@@ -71,6 +71,7 @@ static struct usb_device_id ath3k_table[] = {
 
 	/* Atheros AR3012 with sflash firmware*/
 	{ USB_DEVICE(0x0CF3, 0x3004) },
+	{ USB_DEVICE(0x13d3, 0x3375) },
 
 	/* Atheros AR5BBU12 with sflash firmware */
 	{ USB_DEVICE(0x0489, 0xE02C) },
@@ -87,6 +88,7 @@ static struct usb_device_id ath3k_blist_tbl[] = {
 
 	/* Atheros AR3012 with sflash firmware*/
 	{ USB_DEVICE(0x0cf3, 0x3004), .driver_info = BTUSB_ATH3012 },
+	{ USB_DEVICE(0x13d3, 0x3375), .driver_info = BTUSB_ATH3012 },
 
 	{ }	/* Terminating entry */
 };
diff --git a/drivers/bluetooth/btusb.c b/drivers/bluetooth/btusb.c
index c16c750..df0331a 100644
--- a/drivers/bluetooth/btusb.c
+++ b/drivers/bluetooth/btusb.c
@@ -126,6 +126,7 @@ static struct usb_device_id blacklist_table[] = {
 
 	/* Atheros 3012 with sflash firmware */
 	{ USB_DEVICE(0x0cf3, 0x3004), .driver_info = BTUSB_ATH3012 },
+	{ USB_DEVICE(0x13d3, 0x3375), .driver_info = BTUSB_ATH3012 },
 
 	/* Atheros AR5BBU12 with sflash firmware */
 	{ USB_DEVICE(0x0489, 0xe02c), .driver_info = BTUSB_IGNORE },
-- 
1.7.9.5

