From 13b85c61c69eec7cfd6dde8ce87540ca0760fb49 Mon Sep 17 00:00:00 2001
From: Larry Finger <Larry.Finger@lwfinger.net>
Date: Tue, 27 Dec 2011 12:22:51 -0600
Subject: [PATCH 04/49] rt2800usb: Move ID out of unknown

commit 3f81f8f1524ccca24df1029b0cf825ecef5e5cdc upstream.

Testing on the openSUSE wireless forum has shown that a Linksys
WUSB54GC v3 with USB ID 1737:0077 works with rt2800usb when the ID is
written to /sys/.../new_id. This ID can therefore be moved out of UNKNOWN.

Signed-off-by: Larry Finger <Larry.Finger@lwfinger.net>
Acked-by: Gertjan van Wingerde <gwingerde@gmail.com>
Acked-by: Ivo van Doorn <IvDoorn@gmail.com>
Signed-off-by: John W. Linville <linville@tuxdriver.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@suse.de>
---
 drivers/net/wireless/rt2x00/rt2800usb.c |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/drivers/net/wireless/rt2x00/rt2800usb.c b/drivers/net/wireless/rt2x00/rt2800usb.c
index 3778763..3265b34 100644
--- a/drivers/net/wireless/rt2x00/rt2800usb.c
+++ b/drivers/net/wireless/rt2x00/rt2800usb.c
@@ -976,6 +976,7 @@ static struct usb_device_id rt2800usb_device_table[] = {
 	{ USB_DEVICE(0x13b1, 0x0031) },
 	{ USB_DEVICE(0x1737, 0x0070) },
 	{ USB_DEVICE(0x1737, 0x0071) },
+	{ USB_DEVICE(0x1737, 0x0077) },
 	/* Logitec */
 	{ USB_DEVICE(0x0789, 0x0162) },
 	{ USB_DEVICE(0x0789, 0x0163) },
@@ -1171,7 +1172,6 @@ static struct usb_device_id rt2800usb_device_table[] = {
 	{ USB_DEVICE(0x1740, 0x0605) },
 	{ USB_DEVICE(0x1740, 0x0615) },
 	/* Linksys */
-	{ USB_DEVICE(0x1737, 0x0077) },
 	{ USB_DEVICE(0x1737, 0x0078) },
 	/* Logitec */
 	{ USB_DEVICE(0x0789, 0x0168) },
-- 
1.7.9.4

