From d559faa856c1c6f84dc400b9e77af843d3b79c10 Mon Sep 17 00:00:00 2001
From: Keng-Yu Lin <kengyu@canonical.com>
Date: Wed, 30 Nov 2011 18:32:37 +0800
Subject: [PATCH 078/147] Bluetooth: Add AR30XX device ID on Asus laptops

commit 6b6ba88b5bb8779156b21bb957520a448c3642e2 upstream.

The ID is found on Asus K54HR and K53U.
Blacklist the AR3011-based device ID [0489:e03d]
and add to ath3k.c for firmware loading.

Below is the output of usb-devices script:

Before the fiwmware loading:

T:  Bus=01 Lev=02 Prnt=02 Port=00 Cnt=01 Dev#=  3 Spd=12  MxCh= 0
D:  Ver= 1.10 Cls=e0(wlcon) Sub=01 Prot=01 MxPS=64 #Cfgs=  1
P:  Vendor=0489 ProdID=e03d Rev=00.01
C:  #Ifs= 2 Cfg#= 1 Atr=e0 MxPwr=100mA
I:  If#= 0 Alt= 0 #EPs= 3 Cls=e0(wlcon) Sub=01 Prot=01 Driver=btusb
I:  If#= 1 Alt= 0 #EPs= 2 Cls=e0(wlcon) Sub=01 Prot=01 Driver=btusb

After the fiwmware loading:

T:  Bus=01 Lev=02 Prnt=02 Port=00 Cnt=01 Dev#=  5 Spd=12  MxCh= 0
D:  Ver= 1.10 Cls=e0(wlcon) Sub=01 Prot=01 MxPS=64 #Cfgs=  1
P:  Vendor=0cf3 ProdID=3005 Rev=00.01
C:  #Ifs= 2 Cfg#= 1 Atr=e0 MxPwr=100mA
I:  If#= 0 Alt= 0 #EPs= 3 Cls=e0(wlcon) Sub=01 Prot=01 Driver=btusb
I:  If#= 1 Alt= 0 #EPs= 2 Cls=e0(wlcon) Sub=01 Prot=01 Driver=btusb

Signed-off-by: Keng-Yu Lin <kengyu@canonical.com>
Signed-off-by: Gustavo F. Padovan <padovan@profusion.mobi>
Signed-off-by: Johan Hedberg <johan.hedberg@intel.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/bluetooth/ath3k.c |    1 +
 drivers/bluetooth/btusb.c |    1 +
 2 files changed, 2 insertions(+)

diff --git a/drivers/bluetooth/ath3k.c b/drivers/bluetooth/ath3k.c
index 106beb1..db811d2 100644
--- a/drivers/bluetooth/ath3k.c
+++ b/drivers/bluetooth/ath3k.c
@@ -64,6 +64,7 @@ static struct usb_device_id ath3k_table[] = {
 	{ USB_DEVICE(0x0CF3, 0x3002) },
 	{ USB_DEVICE(0x13d3, 0x3304) },
 	{ USB_DEVICE(0x0930, 0x0215) },
+	{ USB_DEVICE(0x0489, 0xE03D) },
 
 	/* Atheros AR9285 Malbec with sflash firmware */
 	{ USB_DEVICE(0x03F0, 0x311D) },
diff --git a/drivers/bluetooth/btusb.c b/drivers/bluetooth/btusb.c
index eabc437..11a925c 100644
--- a/drivers/bluetooth/btusb.c
+++ b/drivers/bluetooth/btusb.c
@@ -119,6 +119,7 @@ static struct usb_device_id blacklist_table[] = {
 	{ USB_DEVICE(0x0cf3, 0x3002), .driver_info = BTUSB_IGNORE },
 	{ USB_DEVICE(0x13d3, 0x3304), .driver_info = BTUSB_IGNORE },
 	{ USB_DEVICE(0x0930, 0x0215), .driver_info = BTUSB_IGNORE },
+	{ USB_DEVICE(0x0489, 0xe03d), .driver_info = BTUSB_IGNORE },
 
 	/* Atheros AR9285 Malbec with sflash firmware */
 	{ USB_DEVICE(0x03f0, 0x311d), .driver_info = BTUSB_IGNORE },
-- 
1.7.9.4

