From a0aa9c88e27b160651f685945b42749a2a9e1a0a Mon Sep 17 00:00:00 2001
From: Robert Nelson <robertcnelson@gmail.com>
Date: Wed, 5 Oct 2011 16:19:20 -0500
Subject: [PATCH 05/14] ks8851.h it helps to include the include file

Signed-off-by: Robert Nelson <robertcnelson@gmail.com>
---
 include/linux/ks8851.h |   23 +++++++++++++++++++++++
 1 files changed, 23 insertions(+), 0 deletions(-)
 create mode 100644 include/linux/ks8851.h

diff --git a/include/linux/ks8851.h b/include/linux/ks8851.h
new file mode 100644
index 0000000..c933688
--- /dev/null
+++ b/include/linux/ks8851.h
@@ -0,0 +1,23 @@
+/* include/linux/ks8851.h
+ *
+ * Platform specific configuration data for KS8851 driver.
+ *
+ * Copyright 2009 Simtec Electronics
+ *	http://www.simtec.co.uk/
+ *	Ben Dooks <ben@simtec.co.uk>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+/**
+ * struct ks8851_pdata - platform specific configuration data
+ * @irq_flags: The IRQ trigger flags to pass to request_irq().
+ *
+ * Platform specific configuration to be passed from board support
+ * registering the spi device to the driver.
+ */
+struct ks8851_pdata {
+	unsigned	irq_flags;
+};
-- 
1.7.7.4

