From 51d31aff64b1ebc13cab146aea7e34e0b9deec9a Mon Sep 17 00:00:00 2001
From: Tomoya MORINAGA <tomoya.rohm@gmail.com>
Date: Thu, 12 Jan 2012 11:27:05 +0900
Subject: [PATCH 50/69] usb: gadget: pch_udc: Fix disconnect issue

commit c50a3bff0edb0acd49d8033a12ea4668e09a31ad upstream.

ISSUE:
When the driver notifies a gadget of a disconnect event, a system
rarely freezes.

CAUSE:
When the driver calls dev->driver->disconnect(), it is not calling
spin_unlock().

Signed-off-by: Tomoya MORINAGA <tomoya.rohm@gmail.com>
Signed-off-by: Felipe Balbi <balbi@ti.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/usb/gadget/pch_udc.c |    5 ++++-
 1 file changed, 4 insertions(+), 1 deletion(-)

diff --git a/drivers/usb/gadget/pch_udc.c b/drivers/usb/gadget/pch_udc.c
index dd2313c..521e995 100644
--- a/drivers/usb/gadget/pch_udc.c
+++ b/drivers/usb/gadget/pch_udc.c
@@ -2335,8 +2335,11 @@ static void pch_udc_svc_ur_interrupt(struct pch_udc_dev *dev)
 		/* Complete request queue */
 		empty_req_queue(ep);
 	}
-	if (dev->driver && dev->driver->disconnect)
+	if (dev->driver && dev->driver->disconnect) {
+		spin_unlock(&dev->lock);
 		dev->driver->disconnect(&dev->gadget);
+		spin_lock(&dev->lock);
+	}
 }
 
 /**
-- 
1.7.9.5

