From 70fa21fa8918eaa6eb4e7bc98be328412804f52c Mon Sep 17 00:00:00 2001
From: Robert Nelson <robertcnelson@gmail.com>
Date: Tue, 2 Aug 2011 21:55:34 -0500
Subject: [PATCH 1/3] panda: fix wl12xx regulator

pulled from: http://elinux.org/Panda_How_to_kernel_3_0_rel

Signed-off-by: Robert Nelson <robertcnelson@gmail.com>
---
 arch/arm/mach-omap2/twl-common.c |    1 +
 1 files changed, 1 insertions(+), 0 deletions(-)

diff --git a/arch/arm/mach-omap2/twl-common.c b/arch/arm/mach-omap2/twl-common.c
index 10b20c6..5a1f23a 100644
--- a/arch/arm/mach-omap2/twl-common.c
+++ b/arch/arm/mach-omap2/twl-common.c
@@ -281,6 +281,7 @@ static struct regulator_init_data omap4_vusb_idata = {
 static struct regulator_init_data omap4_clk32kg_idata = {
 	.constraints = {
 		.valid_ops_mask		= REGULATOR_CHANGE_STATUS,
+		.always_on		= true,
 	},
 };
 
-- 
1.7.7.4

