From 174b386a16563b183073b5edd7d50f35ffacacdb Mon Sep 17 00:00:00 2001
From: Dan Williams <dcbw@redhat.com>
Date: Tue, 24 Jan 2012 17:16:54 -0600
Subject: [PATCH 47/90] qcaux: add more Pantech UML190 and UML290 ports

commit 074cc73506f529f39fef32ad1c9e1d4cdd8acf6c upstream.

More ports we now know how to talk to.

Signed-off-by: Dan Williams <dcbw@redhat.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/usb/serial/qcaux.c |    7 ++++++-
 1 file changed, 6 insertions(+), 1 deletion(-)

diff --git a/drivers/usb/serial/qcaux.c b/drivers/usb/serial/qcaux.c
index 30b73e6..a348198 100644
--- a/drivers/usb/serial/qcaux.c
+++ b/drivers/usb/serial/qcaux.c
@@ -36,6 +36,7 @@
 #define UTSTARCOM_PRODUCT_UM175_V1		0x3712
 #define UTSTARCOM_PRODUCT_UM175_V2		0x3714
 #define UTSTARCOM_PRODUCT_UM175_ALLTEL		0x3715
+#define PANTECH_PRODUCT_UML190_VZW		0x3716
 #define PANTECH_PRODUCT_UML290_VZW		0x3718
 
 /* CMOTECH devices */
@@ -67,7 +68,11 @@ static struct usb_device_id id_table[] = {
 	{ USB_DEVICE_AND_INTERFACE_INFO(LG_VENDOR_ID, LG_PRODUCT_VX4400_6000, 0xff, 0xff, 0x00) },
 	{ USB_DEVICE_AND_INTERFACE_INFO(SANYO_VENDOR_ID, SANYO_PRODUCT_KATANA_LX, 0xff, 0xff, 0x00) },
 	{ USB_DEVICE_AND_INTERFACE_INFO(SAMSUNG_VENDOR_ID, SAMSUNG_PRODUCT_U520, 0xff, 0x00, 0x00) },
-	{ USB_DEVICE_AND_INTERFACE_INFO(UTSTARCOM_VENDOR_ID, PANTECH_PRODUCT_UML290_VZW, 0xff, 0xff, 0xff) },
+	{ USB_DEVICE_AND_INTERFACE_INFO(UTSTARCOM_VENDOR_ID, PANTECH_PRODUCT_UML190_VZW, 0xff, 0xff, 0xff) },
+	{ USB_DEVICE_AND_INTERFACE_INFO(UTSTARCOM_VENDOR_ID, PANTECH_PRODUCT_UML190_VZW, 0xff, 0xfe, 0xff) },
+	{ USB_DEVICE_AND_INTERFACE_INFO(UTSTARCOM_VENDOR_ID, PANTECH_PRODUCT_UML290_VZW, 0xff, 0xfd, 0xff) },  /* NMEA */
+	{ USB_DEVICE_AND_INTERFACE_INFO(UTSTARCOM_VENDOR_ID, PANTECH_PRODUCT_UML290_VZW, 0xff, 0xfe, 0xff) },  /* WMC */
+	{ USB_DEVICE_AND_INTERFACE_INFO(UTSTARCOM_VENDOR_ID, PANTECH_PRODUCT_UML290_VZW, 0xff, 0xff, 0xff) },  /* DIAG */
 	{ },
 };
 MODULE_DEVICE_TABLE(usb, id_table);
-- 
1.7.9.4

