From 38c2bda521b456704bd7b7376e79d69b0e867198 Mon Sep 17 00:00:00 2001
From: Dave Airlie <airlied@redhat.com>
Date: Wed, 28 Mar 2012 10:48:49 +0100
Subject: [PATCH 130/147] drm/i915: suspend fbdev device around
 suspend/hibernate

commit 3fa016a0b5c5237e9c387fc3249592b2cb5391c6 upstream.

Looking at hibernate overwriting I though it looked like a cursor,
so I tracked down this missing piece to stop the cursor blink
timer. I've no idea if this is sufficient to fix the hibernate
problems people are seeing, but please test it.

Both radeon and nouveau have done this for a long time.

I've run this personally all night hib/resume cycles with no fails.

Reviewed-by: Keith Packard <keithp@keithp.com>
Reported-by: Petr Tesarik <kernel@tesarici.cz>
Reported-by: Stanislaw Gruszka <sgruszka@redhat.com>
Reported-by: Lots of misc segfaults after hibernate across the world.
Bugzilla: https://bugzilla.kernel.org/show_bug.cgi?id=37142
Tested-by: Dave Airlie <airlied@redhat.com>
Tested-by: Bojan Smojver <bojan@rexursive.com>
Tested-by: Andreas Hartmann <andihartmann@01019freenet.de>
Signed-off-by: Dave Airlie <airlied@redhat.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/gpu/drm/i915/i915_drv.c  |    7 +++++++
 drivers/gpu/drm/i915/intel_drv.h |    2 +-
 drivers/gpu/drm/i915/intel_fb.c  |   10 ++++++++++
 3 files changed, 18 insertions(+), 1 deletion(-)

diff --git a/drivers/gpu/drm/i915/i915_drv.c b/drivers/gpu/drm/i915/i915_drv.c
index e2d85a9..d04597d 100644
--- a/drivers/gpu/drm/i915/i915_drv.c
+++ b/drivers/gpu/drm/i915/i915_drv.c
@@ -442,6 +442,10 @@ static int i915_drm_freeze(struct drm_device *dev)
 	/* Modeset on resume, not lid events */
 	dev_priv->modeset_on_lid = 0;
 
+	console_lock();
+	intel_fbdev_set_suspend(dev, 1);
+	console_unlock();
+
 	return 0;
 }
 
@@ -514,6 +518,9 @@ static int i915_drm_thaw(struct drm_device *dev)
 
 	dev_priv->modeset_on_lid = 0;
 
+	console_lock();
+	intel_fbdev_set_suspend(dev, 0);
+	console_unlock();
 	return error;
 }
 
diff --git a/drivers/gpu/drm/i915/intel_drv.h b/drivers/gpu/drm/i915/intel_drv.h
index a1b4343..83e820e 100644
--- a/drivers/gpu/drm/i915/intel_drv.h
+++ b/drivers/gpu/drm/i915/intel_drv.h
@@ -364,7 +364,7 @@ extern int intel_framebuffer_init(struct drm_device *dev,
 				  struct drm_i915_gem_object *obj);
 extern int intel_fbdev_init(struct drm_device *dev);
 extern void intel_fbdev_fini(struct drm_device *dev);
-
+extern void intel_fbdev_set_suspend(struct drm_device *dev, int state);
 extern void intel_prepare_page_flip(struct drm_device *dev, int plane);
 extern void intel_finish_page_flip(struct drm_device *dev, int pipe);
 extern void intel_finish_page_flip_plane(struct drm_device *dev, int plane);
diff --git a/drivers/gpu/drm/i915/intel_fb.c b/drivers/gpu/drm/i915/intel_fb.c
index ec49bae..d0ce34b 100644
--- a/drivers/gpu/drm/i915/intel_fb.c
+++ b/drivers/gpu/drm/i915/intel_fb.c
@@ -257,6 +257,16 @@ void intel_fbdev_fini(struct drm_device *dev)
 	kfree(dev_priv->fbdev);
 	dev_priv->fbdev = NULL;
 }
+
+void intel_fbdev_set_suspend(struct drm_device *dev, int state)
+{
+	drm_i915_private_t *dev_priv = dev->dev_private;
+	if (!dev_priv->fbdev)
+		return;
+
+	fb_set_suspend(dev_priv->fbdev->helper.fbdev, state);
+}
+
 MODULE_LICENSE("GPL and additional rights");
 
 void intel_fb_output_poll_changed(struct drm_device *dev)
-- 
1.7.9.4

