From 80ee9108bee3d22e90191a67036133de09faf7cc Mon Sep 17 00:00:00 2001
From: Simon Graham <simon.graham@virtualcomputer.com>
Date: Tue, 7 Feb 2012 18:07:38 -0600
Subject: [PATCH 037/147] rtlwifi: Handle previous allocation failures when
 freeing device memory

commit 7f66c2f93e5779625c10d262c84537427a2673ca upstream.

Handle previous allocation failures when freeing device memory

Signed-off-by: Simon Graham <simon.graham@virtualcomputer.com>
Signed-off-by: Larry Finger <Larry.Finger@lwfinger.net>
Signed-off-by: John W. Linville <linville@tuxdriver.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/net/wireless/rtlwifi/pci.c |   16 ++++++++++------
 1 file changed, 10 insertions(+), 6 deletions(-)

diff --git a/drivers/net/wireless/rtlwifi/pci.c b/drivers/net/wireless/rtlwifi/pci.c
index 19bb550..9afcad3 100644
--- a/drivers/net/wireless/rtlwifi/pci.c
+++ b/drivers/net/wireless/rtlwifi/pci.c
@@ -1155,10 +1155,12 @@ static void _rtl_pci_free_tx_ring(struct ieee80211_hw *hw,
 		ring->idx = (ring->idx + 1) % ring->entries;
 	}
 
-	pci_free_consistent(rtlpci->pdev,
-			    sizeof(*ring->desc) * ring->entries,
-			    ring->desc, ring->dma);
-	ring->desc = NULL;
+	if (ring->desc) {
+		pci_free_consistent(rtlpci->pdev,
+				    sizeof(*ring->desc) * ring->entries,
+				    ring->desc, ring->dma);
+		ring->desc = NULL;
+	}
 }
 
 static void _rtl_pci_free_rx_ring(struct rtl_pci *rtlpci)
@@ -1182,12 +1184,14 @@ static void _rtl_pci_free_rx_ring(struct rtl_pci *rtlpci)
 			kfree_skb(skb);
 		}
 
-		pci_free_consistent(rtlpci->pdev,
+		if (rtlpci->rx_ring[rx_queue_idx].desc) {
+			pci_free_consistent(rtlpci->pdev,
 				    sizeof(*rtlpci->rx_ring[rx_queue_idx].
 					   desc) * rtlpci->rxringcount,
 				    rtlpci->rx_ring[rx_queue_idx].desc,
 				    rtlpci->rx_ring[rx_queue_idx].dma);
-		rtlpci->rx_ring[rx_queue_idx].desc = NULL;
+			rtlpci->rx_ring[rx_queue_idx].desc = NULL;
+		}
 	}
 }
 
-- 
1.7.9.4

